(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "M2S025-VFG256"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 106.68 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "M2S025-VFG256"
				(at 106.68 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "M2S025-VFG256"
				(at 106.68 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/268/IGLOO_2_FPGA_And_SmartFusion_2_SoC_FPGA_Data_Sheet-3082672.pdf"
				(at 106.68 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "ARM® Cortex®-M3 System On Chip (SOC) IC SmartFusion®2 FPGA - 25K Logic Modules 166MHz 256-FPBGA (17x17)"
				(at 106.68 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "M2S025-VFG256"
				(at 106.68 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 106.68 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 106.68 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 106.68 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "VF256_MCH VF256_MCH-M VF256_MCH-L"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "M2S025-VFG256_1_1"
				(pin bidirectional line
					(at 73.66 -22.86 180)
					(length 3.81)
					(name "DDRIO60NB0/MDDR_DQ1")
					(number "A2")
				)
				(pin bidirectional line
					(at 73.66 -5.08 180)
					(length 3.81)
					(name "DDRIO57PB0/MDDR_DM_RDQS0")
					(number "A3")
				)
				(pin bidirectional line
					(at 73.66 -12.7 180)
					(length 3.81)
					(name "DDRIO58NB0/MDDR_DQS0_N")
					(number "A4")
				)
				(pin bidirectional line
					(at 73.66 -10.16 180)
					(length 3.81)
					(name "DDRIO58PB0/MDDR_DQS0")
					(number "A5")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 3.81)
					(name "DDRIO55PB0/MDDR_DQ7")
					(number "A7")
				)
				(pin output line
					(at 0 -104.14 0)
					(length 3.81)
					(name "DDRIO55NB0/MDDR_TMATCH_0_OUT")
					(number "A8")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 3.81)
					(name "DDRIO52PB0/MDDR_DQS1/GB8/CCC_NE0_CLKI3")
					(number "A9")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 3.81)
					(name "DDRIO52NB0/MDDR_DQS1_N")
					(number "A10")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "DDRIO46NB0/MDDR_CAS_N")
					(number "A12")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "DDRIO46PB0/MDDR_RESET_N")
					(number "A13")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "DDRIO45PB0/MDDR_CLK")
					(number "A14")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "DDRIO45NB0/MDDR_CLK_N")
					(number "A15")
				)
				(pin bidirectional line
					(at 73.66 -43.18 180)
					(length 3.81)
					(name "DDRIO64NB0/MDDR_DQS_ECC_N")
					(number "B1")
				)
				(pin bidirectional line
					(at 73.66 -20.32 180)
					(length 3.81)
					(name "DDRIO60PB0/MDDR_DQ0")
					(number "B2")
				)
				(pin bidirectional line
					(at 73.66 -7.62 180)
					(length 3.81)
					(name "DDRIO57NB0/MDDR_DQ4")
					(number "B3")
				)
				(pin bidirectional line
					(at 73.66 -17.78 180)
					(length 3.81)
					(name "DDRIO59NB0/MDDR_DQ3")
					(number "B5")
				)
				(pin bidirectional line
					(at 73.66 -15.24 180)
					(length 3.81)
					(name "DDRIO59PB0/MDDR_DQ2")
					(number "B6")
				)
				(pin bidirectional line
					(at 73.66 0 180)
					(length 3.81)
					(name "DDRIO56PB0/MDDR_DQ5")
					(number "B7")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 3.81)
					(name "DDRIO51PB0/MDDR_TMATCH_0_IN")
					(number "B8")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 3.81)
					(name "DDRIO50NB0/MDDR_DQ13")
					(number "B10")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 3.81)
					(name "DDRIO50PB0/MDDR_DQ12/GB12/CCC_NE1_CLKI2")
					(number "B11")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 3.81)
					(name "DDRIO48PB0/MDDR_RAS_N")
					(number "B12")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "DDRIO43PB0/MDDR_BA2")
					(number "B13")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "DDRIO35NB0/MDDR_ADDR15")
					(number "B15")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "DDRIO41PB0/MDDR_ADDR3")
					(number "B16")
				)
				(pin bidirectional line
					(at 73.66 -40.64 180)
					(length 3.81)
					(name "DDRIO64PB0/MDDR_DQS_ECC")
					(number "C1")
				)
				(pin bidirectional line
					(at 73.66 -38.1 180)
					(length 3.81)
					(name "DDRIO63NB0/MDDR_DM_RDQS_ECC")
					(number "C3")
				)
				(pin bidirectional line
					(at 73.66 -35.56 180)
					(length 3.81)
					(name "DDRIO63PB0/MDDR_TMATCH_ECC_IN")
					(number "C4")
				)
				(pin bidirectional line
					(at 73.66 -30.48 180)
					(length 3.81)
					(name "DDRIO62PB0/MDDR_DQ_ECC3")
					(number "C5")
				)
				(pin bidirectional line
					(at 73.66 -2.54 180)
					(length 3.81)
					(name "DDRIO56NB0/MDDR_DQ6")
					(number "C6")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 3.81)
					(name "DDRIO54PB0/MDDR_DQ8")
					(number "C8")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 3.81)
					(name "DDRIO54NB0/MDDR_DQ9")
					(number "C9")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 3.81)
					(name "DDRIO51NB0/MDDR_DM_RDQS1")
					(number "C10")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 3.81)
					(name "DDRIO48NB0/MDDR_WE_N")
					(number "C11")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "DDRIO44PB0/MDDR_BA0")
					(number "C12")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "DDRIO43NB0/MDDR_ADDR0")
					(number "C14")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "DDRIO35PB0/MDDR_ADDR14")
					(number "C15")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "DDRIO41NB0/MDDR_ADDR4")
					(number "C16")
				)
				(pin bidirectional line
					(at 73.66 -25.4 180)
					(length 3.81)
					(name "DDRIO61PB0/CCC_NW1_CLKI3")
					(number "D1")
				)
				(pin bidirectional line
					(at 73.66 -27.94 180)
					(length 3.81)
					(name "DDRIO61NB0")
					(number "D2")
				)
				(pin output line
					(at 73.66 -50.8 180)
					(length 3.81)
					(name "DDRIO66PB0/MDDR_TMATCH_ECC_OUT")
					(number "D3")
				)
				(pin bidirectional line
					(at 73.66 -45.72 180)
					(length 3.81)
					(name "DDRIO65PB0/GB0/CCC_NW0_CLKI3")
					(number "D4")
				)
				(pin bidirectional line
					(at 73.66 -33.02 180)
					(length 3.81)
					(name "DDRIO62NB0/MDDR_DQ_ECC2")
					(number "D6")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 3.81)
					(name "DDRIO53PB0/MDDR_DQ10/CCC_NE0_CLKI2")
					(number "D7")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 3.81)
					(name "DDRIO53NB0/MDDR_DQ11")
					(number "D8")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 3.81)
					(name "DDRIO49PB0/MDDR_DQ14/CCC_NE1_CLKI3")
					(number "D9")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 3.81)
					(name "DDRIO47NB0/MDDR_CS_N")
					(number "D11")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "DDRIO44NB0/MDDR_BA1")
					(number "D12")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "DDRIO36NB0/MDDR_ADDR13")
					(number "D13")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "DDRIO36PB0/MDDR_ADDR12")
					(number "D14")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "DDRIO40PB0/MDDR_ADDR5")
					(number "D16")
				)
				(pin unspecified line
					(at 73.66 -104.14 180)
					(length 3.81)
					(name "MDDR_IMP_CALIB")
					(number "E1")
				)
				(pin bidirectional line
					(at 73.66 -53.34 180)
					(length 3.81)
					(name "DDRIO66NB0/CCC_NW0_CLKI2")
					(number "E2")
				)
				(pin bidirectional line
					(at 73.66 -48.26 180)
					(length 3.81)
					(name "DDRIO65NB0/GB4/CCC_NW1_CLKI2")
					(number "E4")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 3.81)
					(name "DDRIO49NB0/MDDR_DQ15")
					(number "E8")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 3.81)
					(name "DDRIO47PB0/MDDR_CKE")
					(number "E10")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "DDRIO42PB0/MDDR_ADDR1")
					(number "E11")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "DDRIO42NB0/MDDR_ADDR2")
					(number "E12")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "DDRIO37PB0/MDDR_ADDR10")
					(number "E14")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "DDRIO38NB0/MDDR_ADDR9")
					(number "E15")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "DDRIO40NB0/MDDR_ADDR6")
					(number "E16")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "DDRIO37NB0/MDDR_ADDR11")
					(number "F13")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "DDRIO38PB0/MDDR_ADDR8")
					(number "F14")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "DDRIO39NB0/MDDR_ADDR7")
					(number "F15")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "DDRIO39PB0/MDDR_ODT")
					(number "F16")
				)
				(pin unspecified line
					(at 73.66 -101.6 180)
					(length 3.81)
					(name "MSI32NB1/MMUART_0_TXD/GPIO_27_B")
					(number "G12")
				)
				(pin unspecified line
					(at 73.66 -99.06 180)
					(length 3.81)
					(name "FLASH_GOLDEN_N")
					(number "H11")
				)
				(pin unspecified line
					(at 73.66 -96.52 180)
					(length 3.81)
					(name "DEVRST_N")
					(number "M11")
				)
				(pin unspecified line
					(at 73.66 -71.12 180)
					(length 3.81)
					(name "JTAGSEL")
					(number "M12")
				)
				(pin unspecified line
					(at 73.66 -66.04 180)
					(length 3.81)
					(name "JTAG_TMS/M3_TMS/M3_SWDIO")
					(number "N11")
				)
				(pin unspecified line
					(at 73.66 -68.58 180)
					(length 3.81)
					(name "JTAG_TRSTB/M3_TRSTB")
					(number "N13")
				)
				(pin unspecified line
					(at 73.66 -63.5 180)
					(length 3.81)
					(name "JTAG_TDO/M3_TDO/M3_SWO")
					(number "P14")
				)
				(pin unspecified line
					(at 73.66 -60.96 180)
					(length 3.81)
					(name "JTAG_TDI/M3_TDI")
					(number "P16")
				)
				(pin unspecified line
					(at 73.66 -58.42 180)
					(length 3.81)
					(name "JTAG_TCK/M3_TCK")
					(number "R14")
				)
			)
			(symbol "M2S025-VFG256_2_1"
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 3.81)
					(name "MSIO97NB7")
					(number "F2")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 3.81)
					(name "MSIO96NB7")
					(number "F3")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 3.81)
					(name "MSIO96PB7/GB6/CCC_NW1_CLKI1")
					(number "F4")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 3.81)
					(name "MSIO95NB7")
					(number "F5")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 3.81)
					(name "MSIO97PB7/GB2/CCC_NW0_CLKI1")
					(number "G1")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 3.81)
					(name "MSIO98NB7")
					(number "G2")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 3.81)
					(name "MSIO98PB7/CCC_NW1_CLKI0")
					(number "G3")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 3.81)
					(name "MSIO95PB7")
					(number "G5")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 3.81)
					(name "MSIO33PB1/MMUART_0_RXD/GPIO_28_B")
					(number "G13")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "MSIO15NB2/SPI_0_SS7/GPIO_22_A")
					(number "G14")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "MSIO14NB2/SPI_0_SS5/GPIO_20_A")
					(number "G16")
				)
				(pin bidirectional line
					(at 92.71 -68.58 180)
					(length 3.81)
					(name "MSIOD103PB6/CCC_SW0_CLKI0")
					(number "H1")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 3.81)
					(name "MSIO99PB7/CCC_NW0_CLKI0")
					(number "H3")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 3.81)
					(name "MSIO99NB7")
					(number "H4")
				)
				(pin bidirectional line
					(at 92.71 -60.96 180)
					(length 3.81)
					(name "MSIOD100PB6/GB5/CCC_SW1_CLKI1")
					(number "H5")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 3.81)
					(name "MSIO27NB1/MMUART_1_TXD/GPIO_24_B")
					(number "H12")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 3.81)
					(name "MSIO28NB1/MMUART_1_RXD/GPIO_26_B")
					(number "H13")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "MSIO15PB2/SPI_0_SS6/GPIO_21_A")
					(number "H14")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "MSIO14PB2/SPI_0_SS4/GPIO_19_A")
					(number "H15")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "MSIO11NB2/I2C_1_SCL/GPIO_1_A/CCC_NE1_CLKI0")
					(number "H16")
				)
				(pin bidirectional line
					(at 92.71 -73.66 180)
					(length 3.81)
					(name "MSIOD118PB5")
					(number "J1")
				)
				(pin bidirectional line
					(at 92.71 -71.12 180)
					(length 3.81)
					(name "MSIOD118NB5")
					(number "J2")
				)
				(pin bidirectional line
					(at 92.71 -66.04 180)
					(length 3.81)
					(name "MSIOD102PB6/CCC_SW1_CLKI0")
					(number "J3")
				)
				(pin bidirectional line
					(at 92.71 -63.5 180)
					(length 3.81)
					(name "MSIOD101PB6/GB1/CCC_SW0_CLKI1")
					(number "J5")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "MSIO13NB2/SPI_0_SS0/GPIO_7_A")
					(number "J12")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "MSIO12NB2/SPI_0_SDI/GPIO_5_A")
					(number "J13")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "MSIO12PB2/SPI_0_CLK")
					(number "J14")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "MSIO11PB2/I2C_1_SDA/GPIO_0_A/CCC_NE0_CLKI0")
					(number "J16")
				)
				(pin bidirectional line
					(at 92.71 -76.2 180)
					(length 3.81)
					(name "MSIOD119NB5")
					(number "K1")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "MSIO13PB2/SPI_0_SDO/GPIO_6_A")
					(number "K12")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "MSIO6PB2/USB_DATA6_B")
					(number "K14")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "MSIO6NB2")
					(number "K15")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "MSIO4PB2/USB_DATA2_B")
					(number "K16")
				)
				(pin bidirectional line
					(at 92.71 -78.74 180)
					(length 3.81)
					(name "MSIOD119PB5")
					(number "L1")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "MSIO3PB2/USB_DATA0_B")
					(number "L11")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "MSIO3NB2/USB_DATA1_B")
					(number "L12")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "MSIO5NB2/USB_DATA5_B")
					(number "L13")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "MSIO5PB2/USB_DATA4_B")
					(number "L14")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "MSIO4NB2/USB_DATA3_B")
					(number "L15")
				)
				(pin bidirectional line
					(at 92.71 -5.08 180)
					(length 3.81)
					(name "MSIO125PB4/GB3/CCC_SW0_CLKI3")
					(number "M7")
				)
				(pin bidirectional line
					(at 92.71 -17.78 180)
					(length 3.81)
					(name "MSIO129NB4")
					(number "M8")
				)
				(pin bidirectional line
					(at 92.71 -30.48 180)
					(length 3.81)
					(name "MSIO132PB4")
					(number "M9")
				)
				(pin bidirectional line
					(at 92.71 -33.02 180)
					(length 3.81)
					(name "MSIO132NB4")
					(number "M10")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "MSIO2NB2/USB_NXT_B")
					(number "M13")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "MSIO0PB2")
					(number "M15")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "MSIO1NB2/USB_DIR_B")
					(number "M16")
				)
				(pin bidirectional line
					(at 92.71 -7.62 180)
					(length 3.81)
					(name "MSIO125NB4/GB7/CCC_SW1_CLKI2")
					(number "N7")
				)
				(pin bidirectional line
					(at 92.71 -15.24 180)
					(length 3.81)
					(name "MSIO129PB4/CCC_SW1_CLKI3")
					(number "N8")
				)
				(pin bidirectional line
					(at 92.71 -38.1 180)
					(length 3.81)
					(name "MSIO133NB4")
					(number "N10")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "MSIO2PB2/USB_STP_B")
					(number "N14")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "MSIO0NB2/USB_DATA7_B")
					(number "N15")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "MSIO1PB2/USB_XCLK_B")
					(number "N16")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 3.81)
					(name "MSIO121PB4/PROBE_A")
					(number "P6")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 3.81)
					(name "MSIO121NB4/PROBE_B")
					(number "P7")
				)
				(pin bidirectional line
					(at 92.71 -12.7 180)
					(length 3.81)
					(name "MSIO126NB4")
					(number "P8")
				)
				(pin bidirectional line
					(at 92.71 -25.4 180)
					(length 3.81)
					(name "MSIO131PB4/GB11/VCCC_SE0_CLKI")
					(number "P9")
				)
				(pin bidirectional line
					(at 92.71 -35.56 180)
					(length 3.81)
					(name "MSIO133PB4/GB15/VCCC_SE1_CLKI")
					(number "P10")
				)
				(pin bidirectional line
					(at 92.71 -50.8 180)
					(length 3.81)
					(name "MSIO143PB4")
					(number "P12")
				)
				(pin bidirectional line
					(at 92.71 -53.34 180)
					(length 3.81)
					(name "MSIO143NB4")
					(number "P13")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 3.81)
					(name "MSIO120PB4")
					(number "R6")
				)
				(pin bidirectional line
					(at 92.71 -10.16 180)
					(length 3.81)
					(name "MSIO126PB4")
					(number "R8")
				)
				(pin bidirectional line
					(at 92.71 -22.86 180)
					(length 3.81)
					(name "MSIO130NB4")
					(number "R9")
				)
				(pin bidirectional line
					(at 92.71 -27.94 180)
					(length 3.81)
					(name "MSIO131NB4")
					(number "R10")
				)
				(pin bidirectional line
					(at 92.71 -43.18 180)
					(length 3.81)
					(name "MSIO134NB4")
					(number "R11")
				)
				(pin bidirectional line
					(at 92.71 -48.26 180)
					(length 3.81)
					(name "MSIO138NB4")
					(number "R12")
				)
				(pin bidirectional line
					(at 92.71 -58.42 180)
					(length 3.81)
					(name "MSIO145NB4")
					(number "R13")
				)
				(pin unspecified line
					(at 92.71 -99.06 180)
					(length 3.81)
					(name "XTLOSC_MAIN_EXTAL")
					(number "R15")
				)
				(pin unspecified line
					(at 92.71 -101.6 180)
					(length 3.81)
					(name "XTLOSC_MAIN_XTAL")
					(number "R16")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 3.81)
					(name "MSIO120NB4/CCC_SW0_CLKI2")
					(number "T6")
				)
				(pin bidirectional line
					(at 92.71 0 180)
					(length 3.81)
					(name "MSIO122PB4")
					(number "T7")
				)
				(pin bidirectional line
					(at 92.71 -2.54 180)
					(length 3.81)
					(name "MSIO122NB4")
					(number "T8")
				)
				(pin bidirectional line
					(at 92.71 -20.32 180)
					(length 3.81)
					(name "MSIO130PB4/VCCC_SE0_CLKI")
					(number "T9")
				)
				(pin bidirectional line
					(at 92.71 -40.64 180)
					(length 3.81)
					(name "MSIO134PB4/VCCC_SE1_CLKI")
					(number "T11")
				)
				(pin bidirectional line
					(at 92.71 -45.72 180)
					(length 3.81)
					(name "MSIO138PB4")
					(number "T12")
				)
				(pin bidirectional line
					(at 92.71 -55.88 180)
					(length 3.81)
					(name "MSIO145PB4")
					(number "T13")
				)
				(pin unspecified line
					(at 92.71 -96.52 180)
					(length 3.81)
					(name "XTLOSC_AUX_XTAL")
					(number "T15")
				)
				(pin unspecified line
					(at 92.71 -93.98 180)
					(length 3.81)
					(name "XTLOSC_AUX_EXTAL")
					(number "T16")
				)
			)
			(symbol "M2S025-VFG256_3_1"
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VDDI0")
					(number "A1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDDI0")
					(number "A11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDDI0")
					(number "B4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDDI0")
					(number "B14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDDI0")
					(number "C7")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDDI0")
					(number "D10")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDDI0")
					(number "E3")
				)
				(pin power_out line
					(at 48.26 -2.54 180)
					(length 3.81)
					(name "CCC_NW0_NW1_PLL_VSSA")
					(number "E5")
				)
				(pin power_in line
					(at 48.26 -21.59 180)
					(length 3.81)
					(name "CCC_NW0_NW1_PLL_VDDA")
					(number "E6")
				)
				(pin power_in line
					(at 0 -29.21 0)
					(length 3.81)
					(name "VREF0")
					(number "E7")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 3.81)
					(hide yes)
					(name "VREF0")
					(number "E9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDDI0")
					(number "E13")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 3.81)
					(name "VDDI7")
					(number "F6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDDI0")
					(number "F8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDDI0")
					(number "F10")
				)
				(pin power_in line
					(at 48.26 -19.05 180)
					(length 3.81)
					(name "CCC_NE0_NE1_MSS_MDDR_PLL_VDDA")
					(number "F11")
				)
				(pin power_out line
					(at 48.26 0 180)
					(length 3.81)
					(name "CCC_NE0_NE1_MSS_MDDR_PLL_VSSA")
					(number "F12")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "G7")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "G9")
				)
				(pin power_out line
					(at 48.26 -29.21 180)
					(length 3.81)
					(name "VSS")
					(number "G10")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDDI1")
					(number "G11")
				)
				(pin passive line
					(at 48.26 -29.21 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G15")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "VDDI7")
					(number "H2")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 3.81)
					(name "VDDI6")
					(number "H6")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "H8")
				)
				(pin power_in line
					(at 0 -24.13 0)
					(length 3.81)
					(name "VPP")
					(number "H10")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "J7")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "J9")
				)
				(pin passive line
					(at 48.26 -29.21 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "J10")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VDDI2")
					(number "J11")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "VDDI2")
					(number "J15")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 3.81)
					(name "VDDI5")
					(number "K2")
				)
				(pin no_connect line
					(at 44.45 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "DNC")
					(number "K3")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 3.81)
					(hide yes)
					(name "VPP")
					(number "K5")
				)
				(pin power_out line
					(at 48.26 -5.08 180)
					(length 3.81)
					(name "CCC_SW0_SW1_PLL_VSSA")
					(number "K6")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "K8")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "K10")
				)
				(pin power_in line
					(at 0 -26.67 0)
					(length 3.81)
					(name "VPPNVM")
					(number "K11")
				)
				(pin passive line
					(at 48.26 -29.21 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "K13")
				)
				(pin no_connect line
					(at 44.45 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "DNC")
					(number "L2")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "L3")
				)
				(pin power_in line
					(at 48.26 -24.13 180)
					(length 3.81)
					(name "CCC_SW0_SW1_PLL_VDDA")
					(number "L5")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "L7")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 3.81)
					(hide yes)
					(name "VPP")
					(number "L9")
				)
				(pin power_out line
					(at 48.26 -26.67 180)
					(length 3.81)
					(name "VSSNVM")
					(number "L10")
				)
				(pin passive line
					(at 48.26 -29.21 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "L16")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "M4")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "M5")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "M6")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "VDDI2")
					(number "M14")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "N5")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VDDI3")
					(number "N12")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 3.81)
					(name "VDDI4")
					(number "P11")
				)
				(pin passive line
					(at 48.26 -29.21 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "P15")
				)
				(pin no_connect line
					(at 44.45 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "DNC")
					(number "R2")
				)
				(pin no_connect line
					(at 44.45 -10.16 180)
					(length 3.81)
					(hide yes)
					(name "DNC")
					(number "R4")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "VDDI4")
					(number "R7")
				)
				(pin no_connect line
					(at 44.45 -11.43 180)
					(length 3.81)
					(hide yes)
					(name "DNC")
					(number "T2")
				)
				(pin no_connect line
					(at 44.45 -13.97 180)
					(length 3.81)
					(hide yes)
					(name "DNC")
					(number "T4")
				)
				(pin passive line
					(at 48.26 -29.21 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "T10")
				)
				(pin passive line
					(at 48.26 -29.21 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "T14")
				)
			)
			(embedded_fonts no)
		)
)
