(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "GNSS_MAX-7Q-0"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 53.34 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "GNSS_MAX-7Q-0"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "GNSS_MAX-7Q-0"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://content.u-blox.com/sites/default/files/products/documents/MAX-7_DataSheet_UBX-13004068.pdf"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "GNSS Module, u-blox, 1.57542 GHz"
				(at 53.34 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "u-blox"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX-7Q-0"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MODULE, GNSS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "GNSS_MAX-7Q-0_1_1"
				(pin power_in line
					(at 0 -22.86 0)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin output line
					(at 26.67 -5.08 180)
					(length 2.54)
					(name "TXD")
					(number "2")
				)
				(pin input line
					(at 26.67 -7.62 180)
					(length 2.54)
					(name "RXD")
					(number "3")
				)
				(pin output line
					(at 26.67 -20.32 180)
					(length 2.54)
					(name "TIMEPULSE")
					(number "4")
				)
				(pin input line
					(at 26.67 -22.86 180)
					(length 2.54)
					(name "EXTINT")
					(number "5")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "V_BCKP")
					(number "6")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC_IO")
					(number "7")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "RESET_N")
					(number "9")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "10")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "RF_IN")
					(number "11")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "12")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 2.54)
					(name "LNA_EN")
					(number "13")
				)
				(pin power_out line
					(at 26.67 0 180)
					(length 2.54)
					(name "VCC_RF")
					(number "14")
				)
				(pin no_connect line
					(at 13.97 -25.4 90)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "15")
				)
				(pin bidirectional line
					(at 26.67 -12.7 180)
					(length 2.54)
					(name "SDA")
					(number "16")
				)
				(pin bidirectional line
					(at 26.67 -15.24 180)
					(length 2.54)
					(name "SCL")
					(number "17")
				)
				(pin no_connect line
					(at 13.97 -25.4 90)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "18")
				)
			)
			(embedded_fonts no)
		)
)
