(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bluetooth_MDBT50Q-ATMS"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "A"
				(at 43.18 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bluetooth_MDBT50Q-ATMS"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bluetooth_MDBT50Q-ATMS"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.raytac.com/download/index.php?index_id=49.pdf"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Bluetooth 5.1/5 Module based on Nordic nRF52833 SoC"
				(at 43.18 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MDBT50Q-ATMS"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Raytac Corporation"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bluetooth_MDBT50Q-ATMS_1_1"
				(pin power_out line
					(at 0 -45.72 0)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "2")
				)
				(pin no_connect line
					(at 25.4 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "3")
				)
				(pin no_connect line
					(at 25.4 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "4")
				)
				(pin no_connect line
					(at 25.4 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "USB")
					(number "6")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "FLASH_DEFAULT")
					(number "7")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "WAKEUP")
					(number "8")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "ADC")
					(number "9")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "10")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "UART_PD")
					(number "11")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "XL1")
					(number "12")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "XL2")
					(number "13")
				)
				(pin output line
					(at 27.94 -17.78 180)
					(length 2.54)
					(name "UART_RTS")
					(number "14")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "UART_CTS")
					(number "15")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "UART_RX")
					(number "16")
				)
				(pin output line
					(at 27.94 -20.32 180)
					(length 2.54)
					(name "UART_TX")
					(number "17")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "18")
				)
				(pin power_in line
					(at 27.94 0 180)
					(length 2.54)
					(name "VDDH")
					(number "19")
				)
				(pin no_connect line
					(at 25.4 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "20")
				)
				(pin power_in line
					(at 27.94 -2.54 180)
					(length 2.54)
					(name "VBUS")
					(number "21")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "22")
				)
				(pin bidirectional line
					(at 27.94 -10.16 180)
					(length 2.54)
					(name "D-")
					(number "23")
				)
				(pin bidirectional line
					(at 27.94 -7.62 180)
					(length 2.54)
					(name "D+")
					(number "24")
				)
				(pin output line
					(at 27.94 -25.4 180)
					(length 2.54)
					(name "INDICATOR")
					(number "25")
				)
				(pin output line
					(at 27.94 -27.94 180)
					(length 2.54)
					(name "LED")
					(number "26")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "RESET")
					(number "27")
				)
				(pin no_connect line
					(at 25.4 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "28")
				)
				(pin no_connect line
					(at 25.4 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "29")
				)
				(pin no_connect line
					(at 25.4 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "30")
				)
				(pin no_connect line
					(at 25.4 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "31")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "SWDIO")
					(number "32")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "SWDCLK")
					(number "33")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "34")
				)
			)
			(embedded_fonts no)
		)
)
