(footprint "BGA-484_19x19mm_Layout22x22_P0.8mm_FCVG484"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "FCVG484, 19.0x19.0mm, 484 Ball, 22x22 Layout, 0.8mm Pitch")
	(tags "BGA 484 0.8")
	(property "Reference" "REF**"
		(at 0 -10.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-484_19x19mm_Layout22x22_P0.8mm_FCVG484"
		(at 0 11.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -10.5 12.499 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -10.5 13.699 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -10.5 14.899 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -8.401 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -7.6 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.723)
	)
	(pad "A3" smd circle
		(at -6.8 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.2271)
	)
	(pad "A4" smd circle
		(at -6 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at -5.201 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.59962)
	)
	(pad "A6" smd circle
		(at -4.401 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.56707)
	)
	(pad "A7" smd circle
		(at -3.601 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.40706)
	)
	(pad "A8" smd circle
		(at -2.8 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.73131)
	)
	(pad "A9" smd circle
		(at -2 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd circle
		(at -1.2 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.84164)
	)
	(pad "A11" smd circle
		(at -0.401 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.8195)
	)
	(pad "A12" smd circle
		(at 0.4 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.19699)
	)
	(pad "A13" smd circle
		(at 1.199 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.21046)
	)
	(pad "A14" smd circle
		(at 1.999 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A15" smd circle
		(at 2.799 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.65884)
	)
	(pad "A16" smd circle
		(at 3.6 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.4183)
	)
	(pad "A17" smd circle
		(at 4.4 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.3918)
	)
	(pad "A18" smd circle
		(at 5.2 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.8908)
	)
	(pad "A19" smd circle
		(at 5.999 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A20" smd circle
		(at 6.799 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.6967)
	)
	(pad "A21" smd circle
		(at 7.599 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.6945)
	)
	(pad "A22" smd circle
		(at 8.4 -8.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA1" smd circle
		(at -8.401 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.09637)
	)
	(pad "AA2" smd circle
		(at -7.6 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.03691)
	)
	(pad "AA3" smd circle
		(at -6.8 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.04366)
	)
	(pad "AA4" smd circle
		(at -6 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA5" smd circle
		(at -5.201 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.44591)
	)
	(pad "AA6" smd circle
		(at -4.401 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.62748)
	)
	(pad "AA7" smd circle
		(at -3.601 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.55419)
	)
	(pad "AA8" smd circle
		(at -2.8 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.33971)
	)
	(pad "AA9" smd circle
		(at -2 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA10" smd circle
		(at -1.2 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.02694)
	)
	(pad "AA11" smd circle
		(at -0.401 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.03866)
	)
	(pad "AA12" smd circle
		(at 0.4 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.6173)
	)
	(pad "AA13" smd circle
		(at 1.199 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.19556)
	)
	(pad "AA14" smd circle
		(at 1.999 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA15" smd circle
		(at 2.799 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.45513)
	)
	(pad "AA16" smd circle
		(at 3.6 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.6422)
	)
	(pad "AA17" smd circle
		(at 4.4 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.85921)
	)
	(pad "AA18" smd circle
		(at 5.2 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.90226)
	)
	(pad "AA19" smd circle
		(at 5.999 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA20" smd circle
		(at 6.799 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.7924)
	)
	(pad "AA21" smd circle
		(at 7.599 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.08107)
	)
	(pad "AA22" smd circle
		(at 8.4 7.599)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.0736)
	)
	(pad "AB1" smd circle
		(at -8.401 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB2" smd circle
		(at -7.6 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.33626)
	)
	(pad "AB3" smd circle
		(at -6.8 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.58315)
	)
	(pad "AB4" smd circle
		(at -6 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.56141)
	)
	(pad "AB5" smd circle
		(at -5.201 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.67168)
	)
	(pad "AB6" smd circle
		(at -4.401 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB7" smd circle
		(at -3.601 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.08953)
	)
	(pad "AB8" smd circle
		(at -2.8 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.89642)
	)
	(pad "AB9" smd circle
		(at -2 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.07175)
	)
	(pad "AB10" smd circle
		(at -1.2 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.08818)
	)
	(pad "AB11" smd circle
		(at -0.401 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB12" smd circle
		(at 0.4 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.62943)
	)
	(pad "AB13" smd circle
		(at 1.199 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.18996)
	)
	(pad "AB14" smd circle
		(at 1.999 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.95763)
	)
	(pad "AB15" smd circle
		(at 2.799 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.94946)
	)
	(pad "AB16" smd circle
		(at 3.6 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB17" smd circle
		(at 4.4 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.85682)
	)
	(pad "AB18" smd circle
		(at 5.2 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.89156)
	)
	(pad "AB19" smd circle
		(at 5.999 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.78063)
	)
	(pad "AB20" smd circle
		(at 6.799 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.76848)
	)
	(pad "AB21" smd circle
		(at 7.599 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.81909)
	)
	(pad "AB22" smd circle
		(at 8.4 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -8.401 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.6754)
	)
	(pad "B2" smd circle
		(at -7.6 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.9065)
	)
	(pad "B3" smd circle
		(at -6.8 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.3654)
	)
	(pad "B4" smd circle
		(at -6 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.68841)
	)
	(pad "B5" smd circle
		(at -5.201 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.42359)
	)
	(pad "B6" smd circle
		(at -4.401 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd circle
		(at -3.601 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.39951)
	)
	(pad "B8" smd circle
		(at -2.8 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.72389)
	)
	(pad "B9" smd circle
		(at -2 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.41584)
	)
	(pad "B10" smd circle
		(at -1.2 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.43586)
	)
	(pad "B11" smd circle
		(at -0.401 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B12" smd circle
		(at 0.4 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.45678)
	)
	(pad "B13" smd circle
		(at 1.199 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.81993)
	)
	(pad "B14" smd circle
		(at 1.999 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.83621)
	)
	(pad "B15" smd circle
		(at 2.799 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.64736)
	)
	(pad "B16" smd circle
		(at 3.6 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B17" smd circle
		(at 4.4 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.4627)
	)
	(pad "B18" smd circle
		(at 5.2 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.8909)
	)
	(pad "B19" smd circle
		(at 5.999 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.83847)
	)
	(pad "B20" smd circle
		(at 6.799 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.84464)
	)
	(pad "B21" smd circle
		(at 7.599 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.6697)
	)
	(pad "B22" smd circle
		(at 8.4 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.6676)
	)
	(pad "C1" smd circle
		(at -8.401 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.9779)
	)
	(pad "C2" smd circle
		(at -7.6 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.7338)
	)
	(pad "C3" smd circle
		(at -6.8 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at -6 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.70234)
	)
	(pad "C5" smd circle
		(at -5.201 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.43731)
	)
	(pad "C6" smd circle
		(at -4.401 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.13895)
	)
	(pad "C7" smd circle
		(at -3.601 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.14822)
	)
	(pad "C8" smd circle
		(at -2.8 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C9" smd circle
		(at -2 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.80518)
	)
	(pad "C10" smd circle
		(at -1.2 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.81684)
	)
	(pad "C11" smd circle
		(at -0.401 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.84089)
	)
	(pad "C12" smd circle
		(at 0.4 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.46342)
	)
	(pad "C13" smd circle
		(at 1.199 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C14" smd circle
		(at 1.999 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.46872)
	)
	(pad "C15" smd circle
		(at 2.799 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.50071)
	)
	(pad "C16" smd circle
		(at 3.6 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.1134)
	)
	(pad "C17" smd circle
		(at 4.4 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.4762)
	)
	(pad "C18" smd circle
		(at 5.2 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C19" smd circle
		(at 5.999 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.19379)
	)
	(pad "C20" smd circle
		(at 6.799 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.14934)
	)
	(pad "C21" smd circle
		(at 7.599 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C22" smd circle
		(at 8.4 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.3467)
	)
	(pad "D1" smd circle
		(at -8.401 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.1837)
	)
	(pad "D2" smd circle
		(at -7.6 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.99134)
	)
	(pad "D3" smd circle
		(at -6.8 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.49076)
	)
	(pad "D4" smd circle
		(at -6 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.41653)
	)
	(pad "D5" smd circle
		(at -5.201 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D6" smd circle
		(at -4.401 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.98256)
	)
	(pad "D7" smd circle
		(at -3.601 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.98411)
	)
	(pad "D8" smd circle
		(at -2.8 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.07352)
	)
	(pad "D9" smd circle
		(at -2 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.0517)
	)
	(pad "D10" smd circle
		(at -1.2 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D11" smd circle
		(at -0.401 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.80638)
	)
	(pad "D12" smd circle
		(at 0.4 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.0319)
	)
	(pad "D13" smd circle
		(at 1.199 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.05981)
	)
	(pad "D14" smd circle
		(at 1.999 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.06844)
	)
	(pad "D15" smd circle
		(at 2.799 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D16" smd circle
		(at 3.6 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.5394)
	)
	(pad "D17" smd circle
		(at 4.4 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.1368)
	)
	(pad "D18" smd circle
		(at 5.2 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.3636)
	)
	(pad "D19" smd circle
		(at 5.999 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.7354)
	)
	(pad "D20" smd circle
		(at 6.799 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.54946)
	)
	(pad "D21" smd circle
		(at 7.599 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.60192)
	)
	(pad "D22" smd circle
		(at 8.4 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.342)
	)
	(pad "E1" smd circle
		(at -8.401 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.80097)
	)
	(pad "E2" smd circle
		(at -7.6 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at -6.8 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.49579)
	)
	(pad "E4" smd circle
		(at -6 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.1708)
	)
	(pad "E5" smd circle
		(at -5.201 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.7656)
	)
	(pad "E6" smd circle
		(at -4.401 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.66068)
	)
	(pad "E7" smd circle
		(at -3.601 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E8" smd circle
		(at -2.8 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.21041)
	)
	(pad "E9" smd circle
		(at -2 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.35251)
	)
	(pad "E10" smd circle
		(at -1.2 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.3535)
	)
	(pad "E11" smd circle
		(at -0.401 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.0538)
	)
	(pad "E12" smd circle
		(at 0.4 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E13" smd circle
		(at 1.199 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.5139)
	)
	(pad "E14" smd circle
		(at 1.999 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.4171)
	)
	(pad "E15" smd circle
		(at 2.799 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.4372)
	)
	(pad "E16" smd circle
		(at 3.6 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.5384)
	)
	(pad "E17" smd circle
		(at 4.4 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E18" smd circle
		(at 5.2 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.4012)
	)
	(pad "E19" smd circle
		(at 5.999 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.7473)
	)
	(pad "E20" smd circle
		(at 6.799 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E21" smd circle
		(at 7.599 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E22" smd circle
		(at 8.4 -5.201)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd circle
		(at -8.401 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.16566)
	)
	(pad "F2" smd circle
		(at -7.6 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.71051)
	)
	(pad "F3" smd circle
		(at -6.8 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.44991)
	)
	(pad "F4" smd circle
		(at -6 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F5" smd circle
		(at -5.201 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.2446)
	)
	(pad "F6" smd circle
		(at -4.401 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.3029)
	)
	(pad "F7" smd circle
		(at -3.601 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.03293)
	)
	(pad "F8" smd circle
		(at -2.8 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.98175)
	)
	(pad "F9" smd circle
		(at -2 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F10" smd circle
		(at -1.2 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.3496)
	)
	(pad "F11" smd circle
		(at -0.401 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.0237)
	)
	(pad "F12" smd circle
		(at 0.4 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.0311)
	)
	(pad "F13" smd circle
		(at 1.199 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.4935)
	)
	(pad "F14" smd circle
		(at 1.999 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F15" smd circle
		(at 2.799 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.3454)
	)
	(pad "F16" smd circle
		(at 3.6 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.7073)
	)
	(pad "F17" smd circle
		(at 4.4 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.7212)
	)
	(pad "F18" smd circle
		(at 5.2 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F19" smd circle
		(at 5.999 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F20" smd circle
		(at 6.799 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F21" smd circle
		(at 7.599 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.36558)
	)
	(pad "F22" smd circle
		(at 8.4 -4.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.34976)
	)
	(pad "G1" smd circle
		(at -8.401 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at -7.6 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.06194)
	)
	(pad "G3" smd circle
		(at -6.8 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.76964)
	)
	(pad "G4" smd circle
		(at -6 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.16295)
	)
	(pad "G5" smd circle
		(at -5.201 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.71)
	)
	(pad "G6" smd circle
		(at -4.401 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G7" smd circle
		(at -3.601 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.17538)
	)
	(pad "G8" smd circle
		(at -2.8 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.93266)
	)
	(pad "G9" smd circle
		(at -2 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.59612)
	)
	(pad "G10" smd circle
		(at -1.2 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.55259)
	)
	(pad "G11" smd circle
		(at -0.401 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G12" smd circle
		(at 0.4 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.3908)
	)
	(pad "G13" smd circle
		(at 1.199 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.308)
	)
	(pad "G14" smd circle
		(at 1.999 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.3354)
	)
	(pad "G15" smd circle
		(at 2.799 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.6356)
	)
	(pad "G16" smd circle
		(at 3.6 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G17" smd circle
		(at 4.4 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.6563)
	)
	(pad "G18" smd circle
		(at 5.2 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G19" smd circle
		(at 5.999 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.56405)
	)
	(pad "G20" smd circle
		(at 6.799 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.55062)
	)
	(pad "G21" smd circle
		(at 7.599 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G22" smd circle
		(at 8.4 -3.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H1" smd circle
		(at -8.401 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.33301)
	)
	(pad "H2" smd circle
		(at -7.6 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.77805)
	)
	(pad "H3" smd circle
		(at -6.8 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H4" smd circle
		(at -6 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.16535)
	)
	(pad "H5" smd circle
		(at -5.201 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.27031)
	)
	(pad "H6" smd circle
		(at -4.401 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.6795)
	)
	(pad "H7" smd circle
		(at -3.601 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.65884)
	)
	(pad "H8" smd circle
		(at -2.8 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H9" smd circle
		(at -2 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.79819)
	)
	(pad "H10" smd circle
		(at -1.2 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.8817)
	)
	(pad "H11" smd circle
		(at -0.401 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.76583)
	)
	(pad "H12" smd circle
		(at 0.4 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.3884)
	)
	(pad "H13" smd circle
		(at 1.199 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.28)
	)
	(pad "H14" smd circle
		(at 1.999 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H15" smd circle
		(at 2.799 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.5915)
	)
	(pad "H16" smd circle
		(at 3.6 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H17" smd circle
		(at 4.4 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.6441)
	)
	(pad "H18" smd circle
		(at 5.2 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H19" smd circle
		(at 5.999 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H20" smd circle
		(at 6.799 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H21" smd circle
		(at 7.599 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.41112)
	)
	(pad "H22" smd circle
		(at 8.4 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.39947)
	)
	(pad "J1" smd circle
		(at -8.401 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.51872)
	)
	(pad "J2" smd circle
		(at -7.6 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.70124)
	)
	(pad "J3" smd circle
		(at -6.8 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.82186)
	)
	(pad "J4" smd circle
		(at -6 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.67867)
	)
	(pad "J5" smd circle
		(at -5.201 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J6" smd circle
		(at -4.401 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.38542)
	)
	(pad "J7" smd circle
		(at -3.601 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.8496)
	)
	(pad "J8" smd circle
		(at -2.8 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J9" smd circle
		(at -2 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J10" smd circle
		(at -1.2 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J11" smd circle
		(at -0.401 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J12" smd circle
		(at 0.4 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J13" smd circle
		(at 1.199 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J14" smd circle
		(at 1.999 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J15" smd circle
		(at 2.799 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J16" smd circle
		(at 3.6 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J17" smd circle
		(at 4.4 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J18" smd circle
		(at 5.2 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J19" smd circle
		(at 5.999 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.98524)
	)
	(pad "J20" smd circle
		(at 6.799 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.97965)
	)
	(pad "J21" smd circle
		(at 7.599 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J22" smd circle
		(at 8.4 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K1" smd circle
		(at -8.401 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.39963)
	)
	(pad "K2" smd circle
		(at -7.6 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K3" smd circle
		(at -6.8 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.2517)
	)
	(pad "K4" smd circle
		(at -6 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.47273)
	)
	(pad "K5" smd circle
		(at -5.201 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.04979)
	)
	(pad "K6" smd circle
		(at -4.401 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.8747)
	)
	(pad "K7" smd circle
		(at -3.601 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.9008)
	)
	(pad "K8" smd circle
		(at -2.8 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K9" smd circle
		(at -2 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K10" smd circle
		(at -1.2 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K11" smd circle
		(at -0.401 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K12" smd circle
		(at 0.4 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K13" smd circle
		(at 1.199 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K14" smd circle
		(at 1.999 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K15" smd circle
		(at 2.799 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K16" smd circle
		(at 3.6 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K17" smd circle
		(at 4.4 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K18" smd circle
		(at 5.2 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K19" smd circle
		(at 5.999 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K20" smd circle
		(at 6.799 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K21" smd circle
		(at 7.599 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.26367)
	)
	(pad "K22" smd circle
		(at 8.4 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.25117)
	)
	(pad "L1" smd circle
		(at -8.401 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.44348)
	)
	(pad "L2" smd circle
		(at -7.6 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.88475)
	)
	(pad "L3" smd circle
		(at -6.8 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.35905)
	)
	(pad "L4" smd circle
		(at -6 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L5" smd circle
		(at -5.201 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.80775)
	)
	(pad "L6" smd circle
		(at -4.401 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.80095)
	)
	(pad "L7" smd circle
		(at -3.601 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.0914)
	)
	(pad "L8" smd circle
		(at -2.8 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.0825)
	)
	(pad "L9" smd circle
		(at -2 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L10" smd circle
		(at -1.2 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L11" smd circle
		(at -0.401 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L12" smd circle
		(at 0.4 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L13" smd circle
		(at 1.199 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L14" smd circle
		(at 1.999 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L15" smd circle
		(at 2.799 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L16" smd circle
		(at 3.6 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L17" smd circle
		(at 4.4 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L18" smd circle
		(at 5.2 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L19" smd circle
		(at 5.999 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.39647)
	)
	(pad "L20" smd circle
		(at 6.799 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.40211)
	)
	(pad "L21" smd circle
		(at 7.599 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L22" smd circle
		(at 8.4 -0.401)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M1" smd circle
		(at -8.401 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M2" smd circle
		(at -7.6 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.23809)
	)
	(pad "M3" smd circle
		(at -6.8 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.42569)
	)
	(pad "M4" smd circle
		(at -6 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.26668)
	)
	(pad "M5" smd circle
		(at -5.201 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.72139)
	)
	(pad "M6" smd circle
		(at -4.401 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M7" smd circle
		(at -3.601 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.1667)
	)
	(pad "M8" smd circle
		(at -2.8 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M9" smd circle
		(at -2 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M10" smd circle
		(at -1.2 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M11" smd circle
		(at -0.401 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M12" smd circle
		(at 0.4 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M13" smd circle
		(at 1.199 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M14" smd circle
		(at 1.999 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M15" smd circle
		(at 2.799 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M16" smd circle
		(at 3.6 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M17" smd circle
		(at 4.4 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M18" smd circle
		(at 5.2 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M19" smd circle
		(at 5.999 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M20" smd circle
		(at 6.799 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M21" smd circle
		(at 7.599 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.06127)
	)
	(pad "M22" smd circle
		(at 8.4 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.05345)
	)
	(pad "N1" smd circle
		(at -8.401 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.69155)
	)
	(pad "N2" smd circle
		(at -7.6 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.87548)
	)
	(pad "N3" smd circle
		(at -6.8 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N4" smd circle
		(at -6 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.90664)
	)
	(pad "N5" smd circle
		(at -5.201 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.32348)
	)
	(pad "N6" smd circle
		(at -4.401 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.82437)
	)
	(pad "N7" smd circle
		(at -3.601 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.84193)
	)
	(pad "N8" smd circle
		(at -2.8 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.1512)
	)
	(pad "N9" smd circle
		(at -2 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N10" smd circle
		(at -1.2 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N11" smd circle
		(at -0.401 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N12" smd circle
		(at 0.4 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N13" smd circle
		(at 1.199 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N14" smd circle
		(at 1.999 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N15" smd circle
		(at 2.799 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N16" smd circle
		(at 3.6 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N17" smd circle
		(at 4.4 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N18" smd circle
		(at 5.2 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N19" smd circle
		(at 5.999 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 3.66682)
	)
	(pad "N20" smd circle
		(at 6.799 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 3.67223)
	)
	(pad "N21" smd circle
		(at 7.599 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N22" smd circle
		(at 8.4 1.199)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P1" smd circle
		(at -8.401 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.26134)
	)
	(pad "P2" smd circle
		(at -7.6 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.7942)
	)
	(pad "P3" smd circle
		(at -6.8 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.81429)
	)
	(pad "P4" smd circle
		(at -6 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.15969)
	)
	(pad "P5" smd circle
		(at -5.201 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P6" smd circle
		(at -4.401 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.75834)
	)
	(pad "P7" smd circle
		(at -3.601 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.75727)
	)
	(pad "P8" smd circle
		(at -2.8 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.47712)
	)
	(pad "P9" smd circle
		(at -2 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P10" smd circle
		(at -1.2 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P11" smd circle
		(at -0.401 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P12" smd circle
		(at 0.4 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P13" smd circle
		(at 1.199 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P14" smd circle
		(at 1.999 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P15" smd circle
		(at 2.799 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P16" smd circle
		(at 3.6 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P17" smd circle
		(at 4.4 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P18" smd circle
		(at 5.2 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P19" smd circle
		(at 5.999 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P20" smd circle
		(at 6.799 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P21" smd circle
		(at 7.599 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.22418)
	)
	(pad "P22" smd circle
		(at 8.4 1.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.20705)
	)
	(pad "R1" smd circle
		(at -8.401 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.25487)
	)
	(pad "R2" smd circle
		(at -7.6 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R3" smd circle
		(at -6.8 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.32263)
	)
	(pad "R4" smd circle
		(at -6 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.07803)
	)
	(pad "R5" smd circle
		(at -5.201 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.19696)
	)
	(pad "R6" smd circle
		(at -4.401 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.05244)
	)
	(pad "R7" smd circle
		(at -3.601 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R8" smd circle
		(at -2.8 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.62709)
	)
	(pad "R9" smd circle
		(at -2 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R10" smd circle
		(at -1.2 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.80076)
	)
	(pad "R11" smd circle
		(at -0.401 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.72485)
	)
	(pad "R12" smd circle
		(at 0.4 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.47419)
	)
	(pad "R13" smd circle
		(at 1.199 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R14" smd circle
		(at 1.999 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.79849)
	)
	(pad "R15" smd circle
		(at 2.799 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.79503)
	)
	(pad "R16" smd circle
		(at 3.6 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.16841)
	)
	(pad "R17" smd circle
		(at 4.4 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R18" smd circle
		(at 5.2 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R19" smd circle
		(at 5.999 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 3.50387)
	)
	(pad "R20" smd circle
		(at 6.799 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 3.48923)
	)
	(pad "R21" smd circle
		(at 7.599 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R22" smd circle
		(at 8.4 2.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T1" smd circle
		(at -8.401 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.79804)
	)
	(pad "T2" smd circle
		(at -7.6 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.67044)
	)
	(pad "T3" smd circle
		(at -6.8 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.12005)
	)
	(pad "T4" smd circle
		(at -6 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T5" smd circle
		(at -5.201 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.63353)
	)
	(pad "T6" smd circle
		(at -4.401 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.29046)
	)
	(pad "T7" smd circle
		(at -3.601 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.35265)
	)
	(pad "T8" smd circle
		(at -2.8 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.08383)
	)
	(pad "T9" smd circle
		(at -2 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T10" smd circle
		(at -1.2 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.77046)
	)
	(pad "T11" smd circle
		(at -0.401 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.39636)
	)
	(pad "T12" smd circle
		(at 0.4 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.24278)
	)
	(pad "T13" smd circle
		(at 1.199 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.48434)
	)
	(pad "T14" smd circle
		(at 1.999 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T15" smd circle
		(at 2.799 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.08627)
	)
	(pad "T16" smd circle
		(at 3.6 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.1755)
	)
	(pad "T17" smd circle
		(at 4.4 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.13684)
	)
	(pad "T18" smd circle
		(at 5.2 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T19" smd circle
		(at 5.999 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T20" smd circle
		(at 6.799 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T21" smd circle
		(at 7.599 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.78253)
	)
	(pad "T22" smd circle
		(at 8.4 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.76703)
	)
	(pad "U1" smd circle
		(at -8.401 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U2" smd circle
		(at -7.6 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.14531)
	)
	(pad "U3" smd circle
		(at -6.8 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.85174)
	)
	(pad "U4" smd circle
		(at -6 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.59715)
	)
	(pad "U5" smd circle
		(at -5.201 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.07391)
	)
	(pad "U6" smd circle
		(at -4.401 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U7" smd circle
		(at -3.601 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.68076)
	)
	(pad "U8" smd circle
		(at -2.8 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.11722)
	)
	(pad "U9" smd circle
		(at -2 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.22807)
	)
	(pad "U10" smd circle
		(at -1.2 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.48606)
	)
	(pad "U11" smd circle
		(at -0.401 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U12" smd circle
		(at 0.4 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.22878)
	)
	(pad "U13" smd circle
		(at 1.199 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.85376)
	)
	(pad "U14" smd circle
		(at 1.999 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.84078)
	)
	(pad "U15" smd circle
		(at 2.799 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.05354)
	)
	(pad "U16" smd circle
		(at 3.6 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U17" smd circle
		(at 4.4 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.1737)
	)
	(pad "U18" smd circle
		(at 5.2 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.75836)
	)
	(pad "U19" smd circle
		(at 5.999 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.74846)
	)
	(pad "U20" smd circle
		(at 6.799 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U21" smd circle
		(at 7.599 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U22" smd circle
		(at 8.4 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V1" smd circle
		(at -8.401 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.02325)
	)
	(pad "V2" smd circle
		(at -7.6 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.02709)
	)
	(pad "V3" smd circle
		(at -6.8 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V4" smd circle
		(at -6 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 3.57164)
	)
	(pad "V5" smd circle
		(at -5.201 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.03998)
	)
	(pad "V6" smd circle
		(at -4.401 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.53023)
	)
	(pad "V7" smd circle
		(at -3.601 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.68562)
	)
	(pad "V8" smd circle
		(at -2.8 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V9" smd circle
		(at -2 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.21899)
	)
	(pad "V10" smd circle
		(at -1.2 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.68063)
	)
	(pad "V11" smd circle
		(at -0.401 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.2829)
	)
	(pad "V12" smd circle
		(at 0.4 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.65608)
	)
	(pad "V13" smd circle
		(at 1.199 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V14" smd circle
		(at 1.999 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.13069)
	)
	(pad "V15" smd circle
		(at 2.799 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.12976)
	)
	(pad "V16" smd circle
		(at 3.6 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.53981)
	)
	(pad "V17" smd circle
		(at 4.4 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.54753)
	)
	(pad "V18" smd circle
		(at 5.2 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V19" smd circle
		(at 5.999 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.19662)
	)
	(pad "V20" smd circle
		(at 6.799 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.20769)
	)
	(pad "V21" smd circle
		(at 7.599 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.55804)
	)
	(pad "V22" smd circle
		(at 8.4 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.64242)
	)
	(pad "W1" smd circle
		(at -8.401 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.04829)
	)
	(pad "W2" smd circle
		(at -7.6 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.45648)
	)
	(pad "W3" smd circle
		(at -6.8 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 3.88376)
	)
	(pad "W4" smd circle
		(at -6 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.30238)
	)
	(pad "W5" smd circle
		(at -5.201 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W6" smd circle
		(at -4.401 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.70831)
	)
	(pad "W7" smd circle
		(at -3.601 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.57901)
	)
	(pad "W8" smd circle
		(at -2.8 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.65979)
	)
	(pad "W9" smd circle
		(at -2 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.80016)
	)
	(pad "W10" smd circle
		(at -1.2 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W11" smd circle
		(at -0.401 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.37032)
	)
	(pad "W12" smd circle
		(at 0.4 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.66699)
	)
	(pad "W13" smd circle
		(at 1.199 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.70016)
	)
	(pad "W14" smd circle
		(at 1.999 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.51699)
	)
	(pad "W15" smd circle
		(at 2.799 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W16" smd circle
		(at 3.6 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.04706)
	)
	(pad "W17" smd circle
		(at 4.4 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.04459)
	)
	(pad "W18" smd circle
		(at 5.2 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.53818)
	)
	(pad "W19" smd circle
		(at 5.999 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.51467)
	)
	(pad "W20" smd circle
		(at 6.799 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W21" smd circle
		(at 7.599 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.54838)
	)
	(pad "W22" smd circle
		(at 8.4 5.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.65293)
	)
	(pad "Y1" smd circle
		(at -8.401 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.78605)
	)
	(pad "Y2" smd circle
		(at -7.6 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y3" smd circle
		(at -6.8 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.09962)
	)
	(pad "Y4" smd circle
		(at -6 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.44242)
	)
	(pad "Y5" smd circle
		(at -5.201 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.77603)
	)
	(pad "Y6" smd circle
		(at -4.401 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.71775)
	)
	(pad "Y7" smd circle
		(at -3.601 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y8" smd circle
		(at -2.8 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.40444)
	)
	(pad "Y9" smd circle
		(at -2 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.5997)
	)
	(pad "Y10" smd circle
		(at -1.2 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.72065)
	)
	(pad "Y11" smd circle
		(at -0.401 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.06682)
	)
	(pad "Y12" smd circle
		(at 0.4 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y13" smd circle
		(at 1.199 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.65691)
	)
	(pad "Y14" smd circle
		(at 1.999 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.51034)
	)
	(pad "Y15" smd circle
		(at 2.799 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.39115)
	)
	(pad "Y16" smd circle
		(at 3.6 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.52137)
	)
	(pad "Y17" smd circle
		(at 4.4 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y18" smd circle
		(at 5.2 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.63395)
	)
	(pad "Y19" smd circle
		(at 5.999 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.64669)
	)
	(pad "Y20" smd circle
		(at 6.799 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.4505)
	)
	(pad "Y21" smd circle
		(at 7.599 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.38301)
	)
	(pad "Y22" smd circle
		(at 8.4 6.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_mpfs250t_fcvg484e.glb"
		(offset
			(xyz 0 0 -0.1)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
