(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ZigBee_MRF24J40MA"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "A"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ZigBee_MRF24J40MA"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ZigBee_MRF24J40MA"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/268/70329b-39211.pdf"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF Transceiver Radio Module, 250Kbps, PCB Antenna, 2.483 GHz"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MRF24J40MA-I/RM"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ZigBee_MRF24J40MA_1_1"
				(pin power_in line
					(at 17.78 -12.7 180)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{RESET}")
					(number "2")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "WAKE")
					(number "3")
				)
				(pin output line
					(at 17.78 0 180)
					(length 2.54)
					(name "INT")
					(number "4")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SDI")
					(number "5")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SCK")
					(number "6")
				)
				(pin output line
					(at 17.78 -2.54 180)
					(length 2.54)
					(name "SDO")
					(number "7")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{CS}")
					(number "8")
				)
				(pin no_connect line
					(at 15.24 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "10")
				)
				(pin passive line
					(at 17.78 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "11")
				)
				(pin passive line
					(at 17.78 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "12")
				)
			)
			(embedded_fonts no)
		)
)
