(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "WiFi_NINA-W102"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 43.18 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "WiFi_NINA-W102"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "WiFi_NINA-W102"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://content.u-blox.com/sites/default/files/NINA-W10_DataSheet_UBX-17065507.pdf"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Bluetooth Lew Energy and WiFi Module"
				(at 43.18 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "NINA-W102-00B"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "u-blox"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE, WIFI, BLUETOOTH"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "WiFi_NINA-W102_1_1"
				(pin bidirectional line
					(at 29.21 -35.56 180)
					(length 2.54)
					(name "SPI_V_MOSI")
					(number "1")
					(alternate "GPIO_1" passive line)
				)
				(pin input line
					(at 29.21 -10.16 180)
					(length 2.54)
					(name "ADC_2")
					(number "2")
					(alternate "GPI_2" passive line)
				)
				(pin input line
					(at 29.21 -12.7 180)
					(length 2.54)
					(name "ADC_3")
					(number "3")
					(alternate "GPI_3" passive line)
				)
				(pin input line
					(at 29.21 -15.24 180)
					(length 2.54)
					(name "ADC_4")
					(number "4")
					(alternate "GPI_4" passive line)
				)
				(pin bidirectional line
					(at 29.21 -17.78 180)
					(length 2.54)
					(name "GPIO_5")
					(number "5")
				)
				(pin passive line
					(at 29.21 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "6")
				)
				(pin bidirectional line
					(at 29.21 -38.1 180)
					(length 2.54)
					(name "LPO_IN")
					(number "7")
					(alternate "GPIO_7" passive line)
				)
				(pin bidirectional line
					(at 29.21 -40.64 180)
					(length 2.54)
					(name "RMII_TX_EN")
					(number "8")
					(alternate "GPIO_8" passive line)
					(alternate "SPI_V_HD" passive line)
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VCC_IO")
					(number "9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "10")
				)
				(pin no_connect line
					(at 29.21 -3.81 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "11")
				)
				(pin power_in line
					(at 29.21 -44.45 180)
					(length 2.54)
					(name "GND")
					(number "12")
				)
				(pin bidirectional line
					(at 29.21 0 180)
					(length 2.54)
					(name "ANT")
					(number "13")
				)
				(pin passive line
					(at 29.21 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "14")
				)
				(pin no_connect line
					(at 29.21 -3.81 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "GPIO_16")
					(number "16")
					(alternate "DAC_16" passive line)
					(alternate "RMII_RXD0" passive line)
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "GPIO_17")
					(number "17")
					(alternate "DAC_17" passive line)
					(alternate "RMII_RXD1" passive line)
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "GPIO_18")
					(number "18")
					(alternate "RMII_CRS_DV" passive line)
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "~{RESET}")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "GPIO_20")
					(number "20")
					(alternate "RMII_TXD1" passive line)
					(alternate "SPI_V_WP" passive line)
					(alternate "UART_RTS" passive line)
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "GPIO_21")
					(number "21")
					(alternate "RMII_TXD0" passive line)
					(alternate "SPI_V_MISO" passive line)
					(alternate "UART_CTS" passive line)
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "GPIO_22")
					(number "22")
					(alternate "UART_TXD" passive line)
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "GPIO_23")
					(number "23")
					(alternate "UART_RXD" passive line)
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "GPIO_24")
					(number "24")
					(alternate "RMII_MDIO" passive line)
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "GPIO_25")
					(number "25")
					(alternate "RMII_MDCLK" passive line)
				)
				(pin passive line
					(at 29.21 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "GPIO_27")
					(number "27")
					(alternate "RMII_CLK" passive line)
					(alternate "SYS_BOOT" passive line)
				)
				(pin bidirectional line
					(at 29.21 -33.02 180)
					(length 2.54)
					(name "SPI_V_CS")
					(number "28")
					(alternate "GPIO_28" passive line)
				)
				(pin bidirectional line
					(at 29.21 -30.48 180)
					(length 2.54)
					(name "SPI_V_CLK")
					(number "29")
					(alternate "GPIO_29" passive line)
				)
				(pin passive line
					(at 29.21 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "30")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 2.54)
					(name "JTAG_TMS")
					(number "31")
					(alternate "GPIO_31" passive line)
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 2.54)
					(name "JTAG_TDO")
					(number "32")
					(alternate "GPIO_32" passive line)
				)
				(pin no_connect line
					(at 29.21 -3.81 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "33")
				)
				(pin input line
					(at 29.21 -20.32 180)
					(length 2.54)
					(name "ADC_34")
					(number "34")
					(alternate "GPI_34" passive line)
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 2.54)
					(name "JTAG_TCK")
					(number "35")
					(alternate "GPIO_35" passive line)
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 2.54)
					(name "JTAG_TDI")
					(number "36")
					(alternate "GPIO_36" passive line)
				)
				(pin passive line
					(at 29.21 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "37")
				)
				(pin passive line
					(at 29.21 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "38")
				)
				(pin passive line
					(at 29.21 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "39")
				)
				(pin passive line
					(at 29.21 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "40")
				)
				(pin passive line
					(at 29.21 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "41")
				)
				(pin passive line
					(at 29.21 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "42")
				)
				(pin passive line
					(at 29.21 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "43")
				)
				(pin passive line
					(at 29.21 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "44")
				)
				(pin passive line
					(at 29.21 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "45")
				)
				(pin passive line
					(at 29.21 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "46")
				)
				(pin passive line
					(at 29.21 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "47")
				)
				(pin passive line
					(at 29.21 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "48")
				)
			)
			(embedded_fonts no)
		)
)
