(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "WiFi_NINA-W132"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "WiFi_NINA-W132"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "WiFi_NINA-W132"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://content.u-blox.com/sites/default/files/NINA-W13_DataSheet_UBX-17006694.pdf"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "WiFi Module"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "NINA-W132-04B"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "u-blox"
				(at 55.88 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE, WIFI"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "WiFi_NINA-W132_1_1"
				(pin output line
					(at 43.18 -35.56 180)
					(length 2.54)
					(name "RED")
					(number "1")
				)
				(pin input line
					(at 43.18 -16.51 180)
					(length 2.54)
					(name "GPI_2")
					(number "2")
				)
				(pin input line
					(at 43.18 -19.05 180)
					(length 2.54)
					(name "GPI_3")
					(number "3")
				)
				(pin input line
					(at 43.18 -21.59 180)
					(length 2.54)
					(name "GPI_4")
					(number "4")
				)
				(pin bidirectional line
					(at 43.18 -24.13 180)
					(length 2.54)
					(name "GPIO_5")
					(number "5")
				)
				(pin power_in line
					(at 43.18 -44.45 180)
					(length 2.54)
					(name "GND")
					(number "6")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 2.54)
					(name "GREEN/SWITCH_1")
					(number "7")
				)
				(pin output line
					(at 43.18 -40.64 180)
					(length 2.54)
					(name "BLUE/RMII_TXEN")
					(number "8")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VCC_IO")
					(number "9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "10")
				)
				(pin no_connect line
					(at 40.64 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "11")
				)
				(pin power_in line
					(at 43.18 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "12")
				)
				(pin bidirectional line
					(at 43.18 0 180)
					(length 2.54)
					(name "ANT")
					(number "13")
				)
				(pin power_in line
					(at 43.18 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "14")
				)
				(pin no_connect line
					(at 40.64 -11.43 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "UART_DTR/RMII_RXD0")
					(number "16")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "UART_DSR/RMII_RXD1")
					(number "17")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SWITCH_2/RMII_CRSDV")
					(number "18")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "~{RESET}")
					(number "19")
				)
				(pin output line
					(at 0 -25.4 0)
					(length 2.54)
					(name "UART_RTS/RMII_TXD1")
					(number "20")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "UART_CTS/RMII_TXD0")
					(number "21")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 2.54)
					(name "UART_TXD")
					(number "22")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "UART_RXD")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "RMII_MDIO")
					(number "24")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 2.54)
					(name "RMII_MDCLK/SPI_DRDY")
					(number "25")
				)
				(pin power_in line
					(at 43.18 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "26")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "RMII_CLK/SYS_BOOT")
					(number "27")
				)
				(pin bidirectional line
					(at 43.18 -26.67 180)
					(length 2.54)
					(name "GPIO_28")
					(number "28")
				)
				(pin bidirectional line
					(at 43.18 -29.21 180)
					(length 2.54)
					(name "GPIO_29")
					(number "29")
				)
				(pin power_in line
					(at 43.18 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "30")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 2.54)
					(name "SPI_SCLK")
					(number "31")
				)
				(pin input line
					(at 0 -39.37 0)
					(length 2.54)
					(name "LOG_BOOT/SPI_CS")
					(number "32")
				)
				(pin no_connect line
					(at 40.64 -10.16 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "33")
				)
				(pin input line
					(at 43.18 -31.75 180)
					(length 2.54)
					(name "GPI_34")
					(number "34")
				)
				(pin input line
					(at 0 -41.91 0)
					(length 2.54)
					(name "SPI_MOSI")
					(number "35")
				)
				(pin output line
					(at 0 -44.45 0)
					(length 2.54)
					(name "SPI_MISO")
					(number "36")
				)
				(pin power_in line
					(at 43.18 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "37")
				)
				(pin power_in line
					(at 43.18 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "38")
				)
				(pin power_in line
					(at 43.18 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "39")
				)
				(pin power_in line
					(at 43.18 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "40")
				)
				(pin power_in line
					(at 43.18 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "41")
				)
				(pin power_in line
					(at 43.18 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "42")
				)
				(pin power_in line
					(at 43.18 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "43")
				)
				(pin power_in line
					(at 43.18 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "44")
				)
				(pin power_in line
					(at 43.18 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "45")
				)
				(pin power_in line
					(at 43.18 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "46")
				)
				(pin power_in line
					(at 43.18 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "47")
				)
				(pin power_in line
					(at 43.18 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "48")
				)
			)
			(embedded_fonts no)
		)
)
