(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bluetooth_NORA-B206-00B"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 43.18 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bluetooth_NORA-B206-00B"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bluetooth_NORA-B206-00B"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://content.u-blox.com/sites/default/files/documents/NORA-B2_DataSheet_UBXDOC-1023859458-38975.pdf"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Bluetooth Modules - 802.15.1 nRF54L15, PCB antenna, open CPU"
				(at 43.18 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "NORA-B206-00B"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "u-blox"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE, WIFI, BLUETOOTH"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bluetooth_NORA-B206-00B_1_1"
				(pin power_in line
					(at 0 -50.8 0)
					(length 2.54)
					(name "GND")
					(number "A1")
				)
				(pin bidirectional line
					(at 29.21 -43.18 180)
					(length 2.54)
					(name "P1.11")
					(number "A3")
					(alternate "AIN4" input line)
					(alternate "ASO[3]" bidirectional line)
					(alternate "RADIO[2]" bidirectional line)
				)
				(pin bidirectional line
					(at 29.21 0 180)
					(length 2.54)
					(name "P0.00")
					(number "A5")
				)
				(pin bidirectional line
					(at 29.21 -2.54 180)
					(length 2.54)
					(name "P0.01")
					(number "A6")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "A7")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "A8")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "A9")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "P2.06")
					(number "B1")
					(alternate "TRACECLK" bidirectional line)
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "B2")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "P2.10")
					(number "B3")
					(alternate "TRACEDATA[3]" bidirectional line)
				)
				(pin bidirectional line
					(at 29.21 -45.72 180)
					(length 2.54)
					(name "P1.12")
					(number "B4")
					(alternate "AIN5" input line)
					(alternate "ASI[3]" bidirectional line)
					(alternate "RADIO[3]" bidirectional line)
				)
				(pin bidirectional line
					(at 29.21 -22.86 180)
					(length 2.54)
					(name "P1.03")
					(number "B5")
					(alternate "NFC2" input line)
				)
				(pin bidirectional line
					(at 29.21 -15.24 180)
					(length 2.54)
					(name "P1.00")
					(number "B6")
					(alternate "XL1" passive line)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "B7")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "B8")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "P2.09")
					(number "C1")
					(alternate "TRACEDATA[2]" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "P2.08")
					(number "C2")
					(alternate "TRACEDATA[1]" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "P2.07")
					(number "C4")
					(alternate "SWO" bidirectional line)
					(alternate "TRACEDATA[0]" bidirectional line)
				)
				(pin bidirectional line
					(at 29.21 -20.32 180)
					(length 2.54)
					(name "P1.02")
					(number "C5")
					(alternate "NFC1" input line)
				)
				(pin bidirectional line
					(at 29.21 -17.78 180)
					(length 2.54)
					(name "P1.01")
					(number "C6")
					(alternate "XL2" passive line)
				)
				(pin bidirectional line
					(at 29.21 -5.08 180)
					(length 2.54)
					(name "P0.02")
					(number "C8")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "P2.03")
					(number "D1")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "P2.02")
					(number "D2")
				)
				(pin bidirectional line
					(at 29.21 -38.1 180)
					(length 2.54)
					(name "P1.09")
					(number "D8")
					(alternate "ASO[2]" bidirectional line)
					(alternate "RADIO[0]" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "P2.05")
					(number "E1")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "P2.04")
					(number "E2")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "E4")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "E5")
				)
				(pin bidirectional line
					(at 29.21 -50.8 180)
					(length 2.54)
					(name "P1.14")
					(number "E8")
					(alternate "AIN7" input line)
					(alternate "RADIO[5]" bidirectional line)
				)
				(pin bidirectional line
					(at 29.21 -35.56 180)
					(length 2.54)
					(name "P1.08")
					(number "E9")
					(alternate "EXTREF" input line)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "P2.01")
					(number "F1")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "P2.00")
					(number "F2")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "F4")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "F5")
				)
				(pin bidirectional line
					(at 29.21 -30.48 180)
					(length 2.54)
					(name "P1.06")
					(number "F8")
					(alternate "AIN2" input line)
					(alternate "ASO[1]" bidirectional line)
				)
				(pin bidirectional line
					(at 29.21 -33.02 180)
					(length 2.54)
					(name "P1.07")
					(number "F9")
					(alternate "AIN3" input line)
					(alternate "ASI[1]" bidirectional line)
				)
				(pin bidirectional line
					(at 29.21 -48.26 180)
					(length 2.54)
					(name "P1.13")
					(number "G5")
					(alternate "AIN6" input line)
					(alternate "RADIO[4]" bidirectional line)
				)
				(pin passive line
					(at 29.21 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "P0.02")
					(number "G7")
				)
				(pin bidirectional line
					(at 29.21 -25.4 180)
					(length 2.54)
					(name "P1.04")
					(number "G8")
					(alternate "AIN0" input line)
					(alternate "ASO[0]" bidirectional line)
				)
				(pin bidirectional line
					(at 29.21 -27.94 180)
					(length 2.54)
					(name "P1.05")
					(number "G9")
					(alternate "AIN1" input line)
					(alternate "ASI[0]" bidirectional line)
					(alternate "RADIO[6]" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "SWDIO")
					(number "H2")
				)
				(pin bidirectional line
					(at 29.21 -10.16 180)
					(length 2.54)
					(name "P0.04")
					(number "H8")
				)
				(pin bidirectional line
					(at 29.21 -40.64 180)
					(length 2.54)
					(name "P1.10")
					(number "H9")
					(alternate "ASI[2]" bidirectional line)
					(alternate "RADIO[1]" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "SWDCLK")
					(number "J2")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 2.54)
					(name "~{RESET}")
					(number "J3")
				)
				(pin passive line
					(at 29.21 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "P1.13")
					(number "J8")
					(alternate "AIN6" passive line)
					(alternate "RADIO[4]" passive line)
				)
				(pin bidirectional line
					(at 29.21 -7.62 180)
					(length 2.54)
					(name "P0.03")
					(number "J9")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "K2")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "K3")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "K5")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "K7")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "K8")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "L1")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "L2")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "M1")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "M2")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "M8")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "M9")
				)
			)
			(embedded_fonts no)
		)
)
