(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "NRF9161"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 48.26 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "NRF9161"
				(at 48.26 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "NRF9161"
				(at 48.26 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/297/nRF9161_PS_v1_0-3439621.pdf"
				(at 48.26 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Multiprotocol Modules SiP (System-in-Package) for LTE-M, NB-IoT, GNSS and DECT NR+."
				(at 48.26 -26.67 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "NRF9161-LACA-R7"
				(at 48.26 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Nordic Semiconductor"
				(at 48.26 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 48.26 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "NRF9161_1_1"
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(name "GND")
					(number "1")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "5")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "6")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "7")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "8")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "9")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "11")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 3.81)
					(name "VDD_GPIO")
					(number "12")
				)
				(pin power_out line
					(at 0 -26.67 0)
					(length 3.81)
					(name "DEC0")
					(number "13")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "14")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "17")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "21")
				)
				(pin power_in line
					(at 0 -8.89 0)
					(length 3.81)
					(name "VDD2")
					(number "22")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "27")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "31")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "36")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "41")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "44")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "47")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "50")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "52")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "56")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "60")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "62")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "63")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "65")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "66")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "68")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "69")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "72")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "74")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "75")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "76")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "77")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "78")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "79")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "80")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "81")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "82")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "85")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "90")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "94")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "98")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 3.81)
					(name "ENABLE")
					(number "101")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VDD1")
					(number "102")
				)
				(pin passive line
					(at 25.4 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "103")
				)
			)
			(symbol "NRF9161_2_1"
				(pin bidirectional line
					(at 33.02 -12.7 180)
					(length 3.81)
					(name "P0.05")
					(number "2")
				)
				(pin bidirectional line
					(at 33.02 -15.24 180)
					(length 3.81)
					(name "P0.06")
					(number "3")
				)
				(pin bidirectional line
					(at 33.02 -17.78 180)
					(length 3.81)
					(name "P0.07")
					(number "4")
				)
				(pin no_connect line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "10")
				)
				(pin bidirectional line
					(at 33.02 -20.32 180)
					(length 3.81)
					(name "P0.08")
					(number "15")
				)
				(pin bidirectional line
					(at 33.02 -22.86 180)
					(length 3.81)
					(name "P0.09")
					(number "16")
				)
				(pin bidirectional line
					(at 33.02 -25.4 180)
					(length 3.81)
					(name "P0.10")
					(number "18")
				)
				(pin bidirectional line
					(at 33.02 -27.94 180)
					(length 3.81)
					(name "P0.11")
					(number "19")
				)
				(pin bidirectional line
					(at 33.02 -30.48 180)
					(length 3.81)
					(name "P0.12")
					(number "20")
				)
				(pin input line
					(at 33.02 -33.02 180)
					(length 3.81)
					(name "P0.13")
					(number "23")
					(alternate "AIN0" passive line)
				)
				(pin bidirectional line
					(at 33.02 -35.56 180)
					(length 3.81)
					(name "P0.14")
					(number "24")
					(alternate "AIN1" passive line)
				)
				(pin bidirectional line
					(at 33.02 -38.1 180)
					(length 3.81)
					(name "P0.15")
					(number "25")
					(alternate "AIN2" passive line)
				)
				(pin bidirectional line
					(at 33.02 -40.64 180)
					(length 3.81)
					(name "P0.16")
					(number "26")
					(alternate "AIN3" passive line)
				)
				(pin bidirectional line
					(at 33.02 -43.18 180)
					(length 3.81)
					(name "P0.17")
					(number "28")
					(alternate "AIN4" passive line)
				)
				(pin bidirectional line
					(at 33.02 -45.72 180)
					(length 3.81)
					(name "P0.18")
					(number "29")
					(alternate "AIN5" passive line)
				)
				(pin bidirectional line
					(at 33.02 -48.26 180)
					(length 3.81)
					(name "P0.19")
					(number "30")
					(alternate "AIN6" passive line)
				)
				(pin input line
					(at 0 -21.59 0)
					(length 3.81)
					(name "~{RESET}")
					(number "32")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 3.81)
					(name "SWDCLK")
					(number "33")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 3.81)
					(name "SWDIO")
					(number "34")
				)
				(pin bidirectional line
					(at 33.02 -50.8 180)
					(length 3.81)
					(name "P0.20")
					(number "35")
					(alternate "AIN7" passive line)
				)
				(pin input line
					(at 33.02 -53.34 180)
					(length 3.81)
					(name "P0.21")
					(number "37")
					(alternate "TRACECLK" passive line)
				)
				(pin bidirectional line
					(at 33.02 -55.88 180)
					(length 3.81)
					(name "P0.22")
					(number "38")
					(alternate "TRACEDATA[0]" passive line)
				)
				(pin bidirectional line
					(at 33.02 -58.42 180)
					(length 3.81)
					(name "P0.23")
					(number "39")
					(alternate "TRACEDATA[1]" passive line)
				)
				(pin bidirectional line
					(at 33.02 -60.96 180)
					(length 3.81)
					(name "P0.24")
					(number "40")
					(alternate "TRACEDATA[2]" passive line)
				)
				(pin bidirectional line
					(at 33.02 -63.5 180)
					(length 3.81)
					(name "P0.25")
					(number "42")
					(alternate "TRACEDATA[3]" passive line)
				)
				(pin output line
					(at 0 -60.96 0)
					(length 3.81)
					(name "SIM_RST")
					(number "43")
				)
				(pin input line
					(at 0 -63.5 0)
					(length 3.81)
					(name "SIM_DET")
					(number "45")
				)
				(pin output line
					(at 0 -66.04 0)
					(length 3.81)
					(name "SIM_CLK")
					(number "46")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 3.81)
					(name "SIM_IO")
					(number "48")
				)
				(pin power_in line
					(at 0 -73.66 0)
					(length 3.81)
					(name "SIM_1V8")
					(number "49")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "51")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 3.81)
					(name "MAGPIO2")
					(number "53")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 3.81)
					(name "MAGPIO1")
					(number "54")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 3.81)
					(name "MAGPIO0")
					(number "55")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "VIO")
					(number "57")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 3.81)
					(name "SCLK")
					(number "58")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "SDATA")
					(number "59")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "ANT")
					(number "61")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "AUX")
					(number "64")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "GPS")
					(number "67")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "70")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "71")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "73")
				)
				(pin input line
					(at 33.02 -66.04 180)
					(length 3.81)
					(name "P0.26")
					(number "83")
				)
				(pin bidirectional line
					(at 33.02 -68.58 180)
					(length 3.81)
					(name "P0.27")
					(number "84")
				)
				(pin bidirectional line
					(at 33.02 -71.12 180)
					(length 3.81)
					(name "P0.28")
					(number "86")
				)
				(pin bidirectional line
					(at 33.02 -73.66 180)
					(length 3.81)
					(name "P0.29")
					(number "87")
				)
				(pin bidirectional line
					(at 33.02 -76.2 180)
					(length 3.81)
					(name "P0.30")
					(number "88")
				)
				(pin bidirectional line
					(at 33.02 -78.74 180)
					(length 3.81)
					(name "P0.31")
					(number "89")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 3.81)
					(name "COEX2")
					(number "91")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 3.81)
					(name "COEX1")
					(number "92")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 3.81)
					(name "COEX0")
					(number "93")
				)
				(pin bidirectional line
					(at 33.02 0 180)
					(length 3.81)
					(name "P0.00")
					(number "95")
				)
				(pin bidirectional line
					(at 33.02 -2.54 180)
					(length 3.81)
					(name "P0.01")
					(number "96")
				)
				(pin bidirectional line
					(at 33.02 -5.08 180)
					(length 3.81)
					(name "P0.02")
					(number "97")
				)
				(pin bidirectional line
					(at 33.02 -7.62 180)
					(length 3.81)
					(name "P0.03")
					(number "99")
				)
				(pin bidirectional line
					(at 33.02 -10.16 180)
					(length 3.81)
					(name "P0.04")
					(number "100")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "104")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "105")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "106")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "107")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "108")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "109")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "110")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "111")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "112")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "113")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "114")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "115")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "116")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "117")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "118")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "119")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "120")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "121")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "122")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "123")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "124")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "125")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "126")
				)
				(pin passive line
					(at 3.81 -77.47 0)
					(length 3.81)
					(hide yes)
					(name "RES")
					(number "127")
				)
			)
			(embedded_fonts no)
		)
)
