(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "OSD32MP157F-512M"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 54.61 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "OSD32MP157F-512M"
				(at 54.61 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "OSD32MP157F-512M"
				(at 54.61 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://octavosystems.com/docs/osd32mp15x-datasheet/"
				(at 54.61 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "SIP containing STM32MP1 module with PMIC, RAM, EEPROM & clock"
				(at 54.61 -26.67 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Octavo Systems"
				(at 54.61 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "OSD32MP157F-512M-IAA"
				(at 54.61 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 54.61 -21.844 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 54.61 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "ARM, BGA, SIP, MICROPROCESSOR"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "OSD32MP157F-512M_1_1"
				(pin input line
					(at 0 -31.75 0)
					(length 3.81)
					(name "PMIC_PONKEYN")
					(number "D3")
				)
				(pin power_in line
					(at 0 -67.31 0)
					(length 3.81)
					(name "GND")
					(number "D4")
				)
				(pin output line
					(at 0 -34.29 0)
					(length 3.81)
					(name "PWR_ON")
					(number "D5")
					(alternate "PMIC_PWRCTRL" passive line)
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 3.81)
					(name "PC13/PMIC_WAKEUP")
					(number "D6")
					(alternate "PMIC_WAKEUP" passive line)
				)
				(pin no_connect line
					(at 38.1 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "RSVD")
					(number "D7")
				)
				(pin no_connect line
					(at 38.1 -36.83 180)
					(length 3.81)
					(hide yes)
					(name "RSVD")
					(number "D8")
				)
				(pin no_connect line
					(at 38.1 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "RSVD")
					(number "D9")
				)
				(pin no_connect line
					(at 38.1 -41.91 180)
					(length 3.81)
					(hide yes)
					(name "RSVD")
					(number "D10")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E4")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E5")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E6")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E7")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E8")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E9")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E10")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E11")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E12")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E13")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E14")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E15")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F4")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F5")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F6")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F7")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F8")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F9")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F10")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F11")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F12")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F13")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F14")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F15")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VIN")
					(number "G1")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VIN")
					(number "G2")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PMIC_LDO25IN")
					(number "G3")
				)
				(pin power_out line
					(at 41.91 -62.23 180)
					(length 3.81)
					(name "PMIC_LDO2")
					(number "G4")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G5")
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 3.81)
					(name "BOOT2")
					(number "G6")
				)
				(pin passive line
					(at 0 -52.07 0)
					(length 3.81)
					(name "TP_VDD")
					(number "G7")
				)
				(pin power_out line
					(at 41.91 -64.77 180)
					(length 3.81)
					(name "PMIC_LDO5")
					(number "G8")
				)
				(pin passive line
					(at 41.91 -54.61 180)
					(length 3.81)
					(hide yes)
					(name "PMIC_SWOUT")
					(number "G9")
				)
				(pin power_out line
					(at 41.91 -54.61 180)
					(length 3.81)
					(name "PMIC_SWOUT")
					(number "G10")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G11")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G12")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G13")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G14")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G15")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VIN")
					(number "H1")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VIN")
					(number "H2")
				)
				(pin power_out line
					(at 41.91 -49.53 180)
					(length 3.81)
					(name "PMIC_VOUT4")
					(number "H3")
				)
				(pin power_out line
					(at 41.91 -67.31 180)
					(length 3.81)
					(name "PMIC_LDO6")
					(number "H4")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H5")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 3.81)
					(name "BOOT1")
					(number "H6")
				)
				(pin passive line
					(at 0 -52.07 0)
					(length 3.81)
					(hide yes)
					(name "TP_VDD")
					(number "H7")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PMIC_SWIN")
					(number "H8")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "PMIC_SWIN")
					(number "H9")
				)
				(pin no_connect line
					(at 38.1 -45.72 180)
					(length 3.81)
					(hide yes)
					(name "RSVD")
					(number "H12")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H13")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H14")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H15")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 3.81)
					(name "~{HSE_OSC_OEN}")
					(number "J1")
				)
				(pin output line
					(at 0 -26.67 0)
					(length 3.81)
					(name "HSE_OSC_TP")
					(number "J2")
				)
				(pin passive line
					(at 41.91 -49.53 180)
					(length 3.81)
					(hide yes)
					(name "PMIC_VOUT4")
					(number "J3")
				)
				(pin power_out line
					(at 41.91 -59.69 180)
					(length 3.81)
					(name "PMIC_LDO1")
					(number "J4")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J5")
				)
				(pin passive line
					(at 0 -57.15 0)
					(length 3.81)
					(name "BOOT0")
					(number "J6")
				)
				(pin passive line
					(at 0 -52.07 0)
					(length 3.81)
					(hide yes)
					(name "TP_VDD")
					(number "J7")
				)
				(pin power_out line
					(at 41.91 -52.07 180)
					(length 3.81)
					(name "PMIC_BSTOUT")
					(number "J8")
				)
				(pin passive line
					(at 41.91 -52.07 180)
					(length 3.81)
					(hide yes)
					(name "PMIC_BSTOUT")
					(number "J9")
				)
				(pin passive line
					(at 41.91 -5.08 180)
					(length 3.81)
					(name "TP_VTT_DDR")
					(number "J12")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J13")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J14")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J15")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J16")
				)
				(pin output line
					(at 41.91 -33.02 180)
					(length 3.81)
					(name "VSSA")
					(number "K1")
				)
				(pin input line
					(at 41.91 -30.48 180)
					(length 3.81)
					(name "VREF-")
					(number "K2")
				)
				(pin power_in line
					(at 0 -13.97 0)
					(length 3.81)
					(name "VBAT")
					(number "K3")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 3.81)
					(name "TP_VDD1")
					(number "K4")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K5")
				)
				(pin output line
					(at 0 -36.83 0)
					(length 3.81)
					(name "PWR_LP")
					(number "K6")
				)
				(pin passive line
					(at 0 -52.07 0)
					(length 3.81)
					(hide yes)
					(name "TP_VDD")
					(number "K7")
				)
				(pin power_out line
					(at 41.91 -57.15 180)
					(length 3.81)
					(name "PMIC_VBUSOTG")
					(number "K8")
				)
				(pin passive line
					(at 41.91 -2.54 180)
					(length 3.81)
					(name "TP_VDD_DDR")
					(number "K12")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K13")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K14")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K15")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K16")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 3.81)
					(name "PA0/PMIC_INTN")
					(number "L3")
					(alternate "PMIC_INTN" passive line)
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 3.81)
					(hide yes)
					(name "TP_VDD1")
					(number "L4")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L5")
				)
				(pin input line
					(at 0 -41.91 0)
					(length 3.81)
					(name "PDR_ON_CORE")
					(number "L6")
				)
				(pin passive line
					(at 0 -52.07 0)
					(length 3.81)
					(hide yes)
					(name "TP_VDD")
					(number "L7")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PMIC_BSTIN")
					(number "L8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "PMIC_BSTIN")
					(number "L9")
				)
				(pin passive line
					(at 41.91 -7.62 180)
					(length 3.81)
					(name "TP_VREF_DDR")
					(number "L12")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L13")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L14")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L15")
				)
				(pin output line
					(at 41.91 -25.4 180)
					(length 3.81)
					(name "VDDA")
					(number "M1")
				)
				(pin input line
					(at 41.91 -27.94 180)
					(length 3.81)
					(name "VREF+")
					(number "M2")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 3.81)
					(name "NRST")
					(number "M3")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 3.81)
					(hide yes)
					(name "TP_VDD1")
					(number "M4")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M5")
				)
				(pin input line
					(at 0 -39.37 0)
					(length 3.81)
					(name "PDR_ON")
					(number "M6")
				)
				(pin passive line
					(at 0 -52.07 0)
					(length 3.81)
					(hide yes)
					(name "TP_VDD")
					(number "M7")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "PMIC_BSTIN")
					(number "M8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "PMIC_BSTIN")
					(number "M9")
				)
				(pin passive line
					(at 0 -64.77 0)
					(length 3.81)
					(name "BYPASS_REG1V8")
					(number "M10")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M11")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M12")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M13")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M14")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M15")
				)
				(pin no_connect line
					(at 38.1 -46.99 180)
					(length 3.81)
					(hide yes)
					(name "RSVD")
					(number "M16")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 3.81)
					(name "NRST_CORE")
					(number "N4")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N5")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N6")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N7")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N8")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N9")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N10")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N11")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N12")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N13")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N14")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N15")
				)
				(pin input line
					(at 0 -29.21 0)
					(length 3.81)
					(name "EEPROM_WP")
					(number "P4")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "P5")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "P6")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "P7")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "P8")
				)
				(pin no_connect line
					(at 38.1 -39.37 180)
					(length 3.81)
					(hide yes)
					(name "RSVD")
					(number "P9")
				)
				(pin no_connect line
					(at 38.1 -43.18 180)
					(length 3.81)
					(hide yes)
					(name "RSVD")
					(number "P10")
				)
				(pin passive line
					(at 41.91 0 180)
					(length 3.81)
					(name "TP_VDD_CORE")
					(number "R4")
				)
				(pin passive line
					(at 41.91 -10.16 180)
					(length 3.81)
					(name "TP_VDD3V3_USB")
					(number "R5")
				)
				(pin passive line
					(at 41.91 -17.78 180)
					(length 3.81)
					(name "TP_VDD1V2_DSI_REG")
					(number "R6")
				)
				(pin passive line
					(at 41.91 -15.24 180)
					(length 3.81)
					(name "TP_VDDA1V8_REG")
					(number "R7")
				)
				(pin passive line
					(at 41.91 -12.7 180)
					(length 3.81)
					(name "TP_VDDA1V1_REG")
					(number "R8")
				)
				(pin no_connect line
					(at 38.1 -40.64 180)
					(length 3.81)
					(hide yes)
					(name "RSVD")
					(number "R9")
				)
				(pin no_connect line
					(at 38.1 -44.45 180)
					(length 3.81)
					(hide yes)
					(name "RSVD")
					(number "R10")
				)
			)
			(symbol "OSD32MP157F-512M_2_1"
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PA13")
					(number "A3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PA3")
					(number "A5")
				)
				(pin bidirectional line
					(at 41.91 -27.94 180)
					(length 3.81)
					(name "PB11")
					(number "A9")
				)
				(pin bidirectional line
					(at 41.91 0 180)
					(length 3.81)
					(name "PB0")
					(number "A11")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PA7")
					(number "A12")
				)
				(pin bidirectional line
					(at 41.91 -25.4 180)
					(length 3.81)
					(name "PB10")
					(number "A13")
				)
				(pin bidirectional line
					(at 41.91 -33.02 180)
					(length 3.81)
					(name "PB13")
					(number "A14")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PA2")
					(number "A15")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PA5")
					(number "A16")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PA14")
					(number "B3")
				)
				(pin bidirectional line
					(at 41.91 -2.54 180)
					(length 3.81)
					(name "PB1")
					(number "B11")
				)
				(pin bidirectional line
					(at 41.91 -30.48 180)
					(length 3.81)
					(name "PB12")
					(number "B14")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PA4")
					(number "B16")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PA6")
					(number "B17")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PA1")
					(number "C16")
				)
				(pin bidirectional line
					(at 41.91 -12.7 180)
					(length 3.81)
					(name "PB5")
					(number "C17")
				)
				(pin bidirectional line
					(at 41.91 -15.24 180)
					(length 3.81)
					(name "PB6")
					(number "H18")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PA10")
					(number "L16")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PA11")
					(number "L17")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PA12")
					(number "L18")
				)
				(pin bidirectional line
					(at 41.91 -5.08 180)
					(length 3.81)
					(name "PB2")
					(number "M18")
				)
				(pin bidirectional line
					(at 41.91 -20.32 180)
					(length 3.81)
					(name "PB8")
					(number "T13")
				)
				(pin bidirectional line
					(at 41.91 -35.56 180)
					(length 3.81)
					(name "PB14")
					(number "T14")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PA15")
					(number "T15")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PA8")
					(number "T17")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PA9")
					(number "U12")
				)
				(pin bidirectional line
					(at 41.91 -22.86 180)
					(length 3.81)
					(name "PB9")
					(number "U13")
				)
				(pin bidirectional line
					(at 41.91 -10.16 180)
					(length 3.81)
					(name "PB4")
					(number "U14")
				)
				(pin bidirectional line
					(at 41.91 -17.78 180)
					(length 3.81)
					(name "PB7")
					(number "V12")
				)
				(pin bidirectional line
					(at 41.91 -38.1 180)
					(length 3.81)
					(name "PB15")
					(number "V13")
				)
				(pin bidirectional line
					(at 41.91 -7.62 180)
					(length 3.81)
					(name "PB3")
					(number "V14")
				)
			)
			(symbol "OSD32MP157F-512M_3_1"
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 3.81)
					(name "USB2_N")
					(number "J17")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 3.81)
					(name "USB2_P")
					(number "J18")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "OTG_VBUS")
					(number "K9")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 3.81)
					(name "USB1_P")
					(number "K17")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 3.81)
					(name "USB1_N")
					(number "K18")
				)
				(pin input line
					(at 41.91 0 180)
					(length 3.81)
					(name "ANA0")
					(number "L1")
				)
				(pin input line
					(at 41.91 -2.54 180)
					(length 3.81)
					(name "ANA1")
					(number "L2")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "DSI_CK_P")
					(number "N16")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "DSI_D1_P")
					(number "N17")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "DSI_D1_N")
					(number "N18")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "DSI_CK_N")
					(number "P16")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "DSI_D0_P")
					(number "P17")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "DSI_D0_N")
					(number "P18")
				)
				(pin bidirectional line
					(at 41.91 -25.4 180)
					(length 3.81)
					(name "NJTRST")
					(number "R11")
				)
				(pin bidirectional line
					(at 41.91 -22.86 180)
					(length 3.81)
					(name "JTDO-TRACESWO")
					(number "R12")
				)
				(pin bidirectional line
					(at 41.91 -20.32 180)
					(length 3.81)
					(name "JTDI")
					(number "R13")
				)
				(pin bidirectional line
					(at 41.91 -15.24 180)
					(length 3.81)
					(name "JTMS-SWDIO")
					(number "R14")
				)
				(pin bidirectional line
					(at 41.91 -17.78 180)
					(length 3.81)
					(name "JTCK-SWCLK")
					(number "R15")
				)
			)
			(symbol "OSD32MP157F-512M_4_1"
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PE2")
					(number "A6")
				)
				(pin bidirectional line
					(at 41.91 -33.02 180)
					(length 3.81)
					(name "PF13")
					(number "A10")
				)
				(pin bidirectional line
					(at 41.91 -35.56 180)
					(length 3.81)
					(name "PF14")
					(number "B10")
				)
				(pin bidirectional line
					(at 41.91 -27.94 180)
					(length 3.81)
					(name "PF11")
					(number "B18")
				)
				(pin bidirectional line
					(at 41.91 -7.62 180)
					(length 3.81)
					(name "PF3")
					(number "C6")
				)
				(pin bidirectional line
					(at 41.91 -38.1 180)
					(length 3.81)
					(name "PF15")
					(number "C10")
				)
				(pin bidirectional line
					(at 41.91 -30.48 180)
					(length 3.81)
					(name "PF12")
					(number "C11")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PE7")
					(number "D17")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PE8")
					(number "D18")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PE9")
					(number "E16")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PE10")
					(number "E17")
				)
				(pin bidirectional line
					(at 41.91 -15.24 180)
					(length 3.81)
					(name "PF6")
					(number "F18")
				)
				(pin bidirectional line
					(at 41.91 -17.78 180)
					(length 3.81)
					(name "PF7")
					(number "G16")
				)
				(pin bidirectional line
					(at 41.91 -20.32 180)
					(length 3.81)
					(name "PF8")
					(number "G17")
				)
				(pin bidirectional line
					(at 41.91 -22.86 180)
					(length 3.81)
					(name "PF9")
					(number "G18")
				)
				(pin bidirectional line
					(at 41.91 -25.4 180)
					(length 3.81)
					(name "PF10")
					(number "H16")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PE4")
					(number "R17")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PE13")
					(number "T5")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PE1")
					(number "T7")
				)
				(pin bidirectional line
					(at 41.91 -12.7 180)
					(length 3.81)
					(name "PF5")
					(number "T8")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PE6")
					(number "T9")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PE3")
					(number "T12")
				)
				(pin bidirectional line
					(at 41.91 -5.08 180)
					(length 3.81)
					(name "PF2")
					(number "T18")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PE15")
					(number "U4")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PE12")
					(number "U5")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "PE0")
					(number "U7")
				)
				(pin bidirectional line
					(at 41.91 0 180)
					(length 3.81)
					(name "PF0")
					(number "U8")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PE14")
					(number "V4")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PE11")
					(number "V5")
				)
				(pin bidirectional line
					(at 41.91 -10.16 180)
					(length 3.81)
					(name "PF4")
					(number "V7")
				)
				(pin bidirectional line
					(at 41.91 -2.54 180)
					(length 3.81)
					(name "PF1")
					(number "V8")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PE5")
					(number "V15")
				)
			)
			(symbol "OSD32MP157F-512M_5_1"
				(pin bidirectional line
					(at 41.91 -38.1 180)
					(length 3.81)
					(name "PD15")
					(number "A2")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "PC0")
					(number "A17")
				)
				(pin bidirectional line
					(at 41.91 -22.86 180)
					(length 3.81)
					(name "PD9")
					(number "B1")
				)
				(pin bidirectional line
					(at 41.91 -20.32 180)
					(length 3.81)
					(name "PD8")
					(number "B2")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PC3")
					(number "B6")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PC4")
					(number "B12")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PC1")
					(number "B15")
				)
				(pin bidirectional line
					(at 41.91 -35.56 180)
					(length 3.81)
					(name "PD14")
					(number "C3")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PC2")
					(number "C7")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PC5")
					(number "C12")
				)
				(pin bidirectional line
					(at 41.91 -27.94 180)
					(length 3.81)
					(name "PD11")
					(number "E18")
				)
				(pin bidirectional line
					(at 41.91 -30.48 180)
					(length 3.81)
					(name "PD12")
					(number "F16")
				)
				(pin bidirectional line
					(at 41.91 -33.02 180)
					(length 3.81)
					(name "PD13")
					(number "F17")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PC15-OSC32_OUT")
					(number "N1")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PC14-OSC32_IN")
					(number "N2")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PC7")
					(number "R16")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PC6")
					(number "R18")
				)
				(pin bidirectional line
					(at 41.91 -15.24 180)
					(length 3.81)
					(name "PD6")
					(number "T10")
				)
				(pin bidirectional line
					(at 41.91 -7.62 180)
					(length 3.81)
					(name "PD3")
					(number "T11")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PC8")
					(number "T16")
				)
				(pin bidirectional line
					(at 41.91 -17.78 180)
					(length 3.81)
					(name "PD7")
					(number "U9")
				)
				(pin bidirectional line
					(at 41.91 -12.7 180)
					(length 3.81)
					(name "PD5")
					(number "U10")
				)
				(pin bidirectional line
					(at 41.91 -2.54 180)
					(length 3.81)
					(name "PD1")
					(number "U11")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PC9")
					(number "U16")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PC11")
					(number "U17")
				)
				(pin bidirectional line
					(at 41.91 -5.08 180)
					(length 3.81)
					(name "PD2")
					(number "U18")
				)
				(pin bidirectional line
					(at 41.91 -25.4 180)
					(length 3.81)
					(name "PD10")
					(number "V6")
				)
				(pin bidirectional line
					(at 41.91 -10.16 180)
					(length 3.81)
					(name "PD4")
					(number "V10")
				)
				(pin bidirectional line
					(at 41.91 0 180)
					(length 3.81)
					(name "PD0")
					(number "V11")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PC10")
					(number "V16")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PC12")
					(number "V17")
				)
			)
			(symbol "OSD32MP157F-512M_6_1"
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PG12")
					(number "A4")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PG14")
					(number "A7")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PG2")
					(number "A8")
				)
				(pin bidirectional line
					(at 41.91 -15.24 180)
					(length 3.81)
					(name "PH6")
					(number "B5")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PG13")
					(number "B7")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PG1")
					(number "B8")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PG4")
					(number "B9")
				)
				(pin bidirectional line
					(at 41.91 -5.08 180)
					(length 3.81)
					(name "PH2")
					(number "B13")
				)
				(pin bidirectional line
					(at 41.91 -17.78 180)
					(length 3.81)
					(name "PH7")
					(number "C5")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "PG0")
					(number "C8")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PG3")
					(number "C9")
				)
				(pin bidirectional line
					(at 41.91 -7.62 180)
					(length 3.81)
					(name "PH3")
					(number "C13")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PG11")
					(number "C14")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PG5")
					(number "C15")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PG10")
					(number "C18")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PG8")
					(number "D16")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PG7")
					(number "H17")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PG9")
					(number "M17")
				)
				(pin bidirectional line
					(at 41.91 -35.56 180)
					(length 3.81)
					(name "PH14")
					(number "T1")
				)
				(pin bidirectional line
					(at 41.91 -38.1 180)
					(length 3.81)
					(name "PH15")
					(number "T2")
				)
				(pin bidirectional line
					(at 41.91 -20.32 180)
					(length 3.81)
					(name "PH8")
					(number "T4")
				)
				(pin bidirectional line
					(at 41.91 -12.7 180)
					(length 3.81)
					(name "PH5")
					(number "T6")
				)
				(pin bidirectional line
					(at 41.91 -33.02 180)
					(length 3.81)
					(name "PH13")
					(number "U1")
				)
				(pin bidirectional line
					(at 41.91 -30.48 180)
					(length 3.81)
					(name "PH12")
					(number "U2")
				)
				(pin bidirectional line
					(at 41.91 -25.4 180)
					(length 3.81)
					(name "PH10")
					(number "U3")
				)
				(pin bidirectional line
					(at 41.91 -10.16 180)
					(length 3.81)
					(name "PH4")
					(number "U6")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PG6")
					(number "U15")
				)
				(pin bidirectional line
					(at 41.91 -27.94 180)
					(length 3.81)
					(name "PH11")
					(number "V2")
				)
				(pin bidirectional line
					(at 41.91 -22.86 180)
					(length 3.81)
					(name "PH9")
					(number "V3")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PG15")
					(number "V9")
				)
			)
			(symbol "OSD32MP157F-512M_7_1"
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PI10")
					(number "B4")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PI8")
					(number "C1")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PI9")
					(number "C2")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PI11")
					(number "C4")
				)
				(pin bidirectional line
					(at 41.91 -15.24 180)
					(length 3.81)
					(name "PZ6")
					(number "D1")
				)
				(pin bidirectional line
					(at 41.91 -17.78 180)
					(length 3.81)
					(name "PZ7")
					(number "D2")
				)
				(pin bidirectional line
					(at 41.91 -7.62 180)
					(length 3.81)
					(name "PZ3")
					(number "E1")
				)
				(pin bidirectional line
					(at 41.91 -10.16 180)
					(length 3.81)
					(name "PZ4")
					(number "E2")
					(alternate "PMIC_SCL" passive line)
				)
				(pin bidirectional line
					(at 41.91 -12.7 180)
					(length 3.81)
					(name "PZ5")
					(number "E3")
					(alternate "PMIC_SDA" passive line)
				)
				(pin bidirectional line
					(at 41.91 0 180)
					(length 3.81)
					(name "PZ0")
					(number "F1")
				)
				(pin bidirectional line
					(at 41.91 -2.54 180)
					(length 3.81)
					(name "PZ1")
					(number "F2")
				)
				(pin bidirectional line
					(at 41.91 -5.08 180)
					(length 3.81)
					(name "PZ2")
					(number "F3")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PI7")
					(number "N3")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PI4")
					(number "P1")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PI5")
					(number "P2")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PI6")
					(number "P3")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PI1")
					(number "R1")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PI2")
					(number "R2")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PI3")
					(number "R3")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "PI0")
					(number "T3")
				)
			)
			(embedded_fonts no)
		)
)
