(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "RF_RAK811-868MHz"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "RF_RAK811-868MHz"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "RF_RAK811-868MHz"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://downloads.rakwireless.com/LoRa/RAK811/Hardware_Specification/RAK811_LoRa_Module_Datasheet_V1.4.pdf"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "LoRa Module, STM32L151, EU868, RAKwireless"
				(at 45.72 -30.48 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "RAK811-868MHz"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "RAKwireless"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, RF, MODULE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "RAK811*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "RF_RAK811-868MHz_1_1"
				(pin power_in line
					(at 30.48 -34.29 180)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin bidirectional line
					(at 30.48 -24.13 180)
					(length 2.54)
					(name "PB12")
					(number "2")
				)
				(pin bidirectional line
					(at 30.48 -26.67 180)
					(length 2.54)
					(name "PB14")
					(number "3")
				)
				(pin bidirectional line
					(at 30.48 -29.21 180)
					(length 2.54)
					(name "PB15")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 2.54)
					(name "PA8")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 2.54)
					(name "PA9")
					(number "6")
					(alternate "USART1_TX" passive line)
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 2.54)
					(name "PA10")
					(number "7")
					(alternate "USART1_RX" passive line)
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 2.54)
					(name "PA12")
					(number "8")
				)
				(pin bidirectional line
					(at 30.48 -8.89 180)
					(length 2.54)
					(name "PB4")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 2.54)
					(name "PA13")
					(number "10")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "11")
				)
				(pin passive line
					(at 30.48 -34.29 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 2.54)
					(name "PA14")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 2.54)
					(name "PA15")
					(number "14")
				)
				(pin bidirectional line
					(at 30.48 -6.35 180)
					(length 2.54)
					(name "PB3")
					(number "15")
				)
				(pin bidirectional line
					(at 30.48 -11.43 180)
					(length 2.54)
					(name "PB5")
					(number "16")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "BOOT0")
					(number "17")
				)
				(pin bidirectional line
					(at 30.48 -13.97 180)
					(length 2.54)
					(name "PB8")
					(number "18")
				)
				(pin bidirectional line
					(at 30.48 -16.51 180)
					(length 2.54)
					(name "PB9")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 2.54)
					(name "PA2")
					(number "20")
				)
				(pin passive line
					(at 30.48 -34.29 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "21")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 2.54)
					(name "PA1")
					(number "22")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 2.54)
					(name "PA0")
					(number "23")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "~{RST}")
					(number "24")
				)
				(pin bidirectional line
					(at 30.48 -19.05 180)
					(length 2.54)
					(name "PB10")
					(number "25")
				)
				(pin bidirectional line
					(at 30.48 -21.59 180)
					(length 2.54)
					(name "PB11")
					(number "26")
				)
				(pin bidirectional line
					(at 30.48 -3.81 180)
					(length 2.54)
					(name "PB2")
					(number "27")
				)
				(pin passive line
					(at 30.48 -34.29 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "28")
				)
				(pin passive line
					(at 30.48 -34.29 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "29")
				)
				(pin passive line
					(at 30.48 -34.29 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "30")
				)
				(pin passive line
					(at 30.48 -34.29 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "31")
				)
				(pin passive line
					(at 30.48 -34.29 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "32")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 2.54)
					(name "RF_OUT")
					(number "33")
				)
				(pin passive line
					(at 30.48 -34.29 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "34")
				)
			)
			(embedded_fonts no)
		)
)
