(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "WiFi_RN171-I_RM"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "A"
				(at 58.42 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "WiFi_RN171-I_RM"
				(at 58.42 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "WiFi_RN171-I_RM"
				(at 58.42 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.microchip.com/mymicrochip/filehandler.aspx?ddocname=en558063"
				(at 58.42 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Wireless LAN Module, 802.11 b/g, 2.4 GHz, Drop-in Wi-Fi Solution, On-board TCP/IP stack"
				(at 58.42 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "RN171-I/RM"
				(at 58.42 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 58.42 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 58.42 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 58.42 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "WiFi_RN171-I_RM_1_1"
				(pin power_in line
					(at 39.37 -48.26 180)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin output line
					(at 39.37 -7.62 180)
					(length 2.54)
					(name "ISP_TX")
					(number "2")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "ISP_RX")
					(number "3")
				)
				(pin bidirectional line
					(at 39.37 -17.78 180)
					(length 2.54)
					(name "GPIO9/SD_CLK/SCLK")
					(number "4")
				)
				(pin bidirectional line
					(at 39.37 -20.32 180)
					(length 2.54)
					(name "GPIO8/SD_D3/SS")
					(number "5")
				)
				(pin bidirectional line
					(at 39.37 -22.86 180)
					(length 2.54)
					(name "GPIO7/SD_D2")
					(number "6")
				)
				(pin bidirectional line
					(at 39.37 -25.4 180)
					(length 2.54)
					(name "GPIO6/SD_D1/INT")
					(number "7")
				)
				(pin bidirectional line
					(at 39.37 -27.94 180)
					(length 2.54)
					(name "GPIO5/SD_D0/MISO")
					(number "8")
				)
				(pin bidirectional line
					(at 39.37 -30.48 180)
					(length 2.54)
					(name "GPIO4/SD_CMD/MOSI")
					(number "9")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VDD")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "GPIO3")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "GPIO2")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "GPIO1")
					(number "13")
				)
				(pin passive line
					(at 39.37 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "14")
				)
				(pin output line
					(at 39.37 -10.16 180)
					(length 2.54)
					(name "SPI_CS")
					(number "15")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "SPI_MISO")
					(number "16")
				)
				(pin output line
					(at 39.37 -12.7 180)
					(length 2.54)
					(name "SPI_SCK")
					(number "17")
				)
				(pin output line
					(at 39.37 -15.24 180)
					(length 2.54)
					(name "SPI_MOSI")
					(number "18")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "FLASH_POWER")
					(number "19")
				)
				(pin passive line
					(at 39.37 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "20")
				)
				(pin passive line
					(at 39.37 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "21")
				)
				(pin passive line
					(at 39.37 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "22")
				)
				(pin passive line
					(at 39.37 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "23")
				)
				(pin bidirectional line
					(at 39.37 -5.08 180)
					(length 2.54)
					(name "ANT")
					(number "24")
				)
				(pin passive line
					(at 39.37 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "25")
				)
				(pin passive line
					(at 39.37 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "26")
				)
				(pin passive line
					(at 39.37 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "27")
				)
				(pin passive line
					(at 39.37 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "28")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "SENSOR0")
					(number "29")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "SENSOR1")
					(number "30")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "SENSOR2")
					(number "31")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "SENSOR3")
					(number "32")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SENSOR_POWER")
					(number "33")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "34")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "SENSOR4")
					(number "35")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 2.54)
					(name "SENSOR5")
					(number "36")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 2.54)
					(name "SENSOR6")
					(number "37")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 2.54)
					(name "SENSOR7")
					(number "38")
				)
				(pin passive line
					(at 39.37 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "39")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "RESET")
					(number "40")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "FORCE_AWAKE")
					(number "41")
				)
				(pin bidirectional line
					(at 39.37 -33.02 180)
					(length 2.54)
					(name "GPIO14")
					(number "42")
				)
				(pin bidirectional line
					(at 39.37 -35.56 180)
					(length 2.54)
					(name "RTS/GPIO13")
					(number "43")
				)
				(pin bidirectional line
					(at 39.37 -38.1 180)
					(length 2.54)
					(name "CTS/GPIO12")
					(number "44")
				)
				(pin bidirectional line
					(at 39.37 0 180)
					(length 2.54)
					(name "RX/GPIO11")
					(number "45")
				)
				(pin bidirectional line
					(at 39.37 -2.54 180)
					(length 2.54)
					(name "TX/GPIO10")
					(number "46")
				)
				(pin passive line
					(at 39.37 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "47")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SREG_3V3_CTRL")
					(number "48")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VBATT")
					(number "49")
				)
				(pin unspecified line
					(at 39.37 -40.64 180)
					(length 2.54)
					(name "")
					(number "50")
				)
			)
			(embedded_fonts no)
		)
)
