(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bluetooth_RN4020"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "A"
				(at 48.26 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bluetooth_RN4020"
				(at 48.26 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bluetooth_RN4020"
				(at 48.26 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.microchip.com/mymicrochip/filehandler.aspx?ddocname=en570043"
				(at 48.26 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Bluetooth 4.1, Class 2 Module, 1.8V to 3.6V Supply, 100m Range, 1Mbps, -92.5dBm Sensitivity"
				(at 48.26 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "RN4020-V/RM"
				(at 48.26 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 48.26 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 48.26 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bluetooth_RN4020_1_1"
				(pin power_in line
					(at 33.02 -25.4 180)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "AIO2")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "AIO1")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "AIO0")
					(number "4")
				)
				(pin output line
					(at 33.02 0 180)
					(length 2.54)
					(name "UART_TX")
					(number "5")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "UART_RX")
					(number "6")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "WAKE_SW")
					(number "7")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "CMD/MLDP")
					(number "8")
				)
				(pin output line
					(at 33.02 -2.54 180)
					(length 2.54)
					(name "LED/PIO/SCK")
					(number "10")
				)
				(pin output line
					(at 33.02 -5.08 180)
					(length 2.54)
					(name "MLDP_EV_PIO")
					(number "11")
				)
				(pin output line
					(at 33.02 -7.62 180)
					(length 2.54)
					(name "WS/PIO/MOSI")
					(number "12")
				)
				(pin bidirectional line
					(at 33.02 -10.16 180)
					(length 2.54)
					(name "PIO[4]")
					(number "13")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "CTS/PIO[5]")
					(number "14")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "WAKE_HW")
					(number "15")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "SPI/~{PIO}")
					(number "17")
				)
				(pin output line
					(at 33.02 -12.7 180)
					(length 2.54)
					(name "RTS/PIO")
					(number "18")
				)
				(pin bidirectional line
					(at 33.02 -15.24 180)
					(length 2.54)
					(name "PWM4/PIO")
					(number "19")
				)
				(pin no_connect line
					(at 30.48 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "20")
				)
				(pin bidirectional line
					(at 33.02 -20.32 180)
					(length 2.54)
					(name "SDA")
					(number "21")
				)
				(pin bidirectional line
					(at 33.02 -22.86 180)
					(length 2.54)
					(name "SCL")
					(number "22")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "23")
				)
				(pin passive line
					(at 33.02 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "24")
				)
			)
			(embedded_fonts no)
		)
)
