(footprint "BGA-784_23x23mm_Layout28x28_P0.8mm-microchip-technology-mpfs160T-fcvg784"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "U"
		(at -12.5 -13.05 0)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-784_23x23mm_Layout28x28_P0.8mm-microchip-technology-mpfs160T-fcvg784"
		(at -12.5 13.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -12.5 14.8 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -12.5 16 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -12.5 17.2 0)
		(layer "F.Fab")
	)
	(fp_text user ""
		(at 0 0 0)
		(layer "User.5")
	)
	(fp_text user ""
		(at 0 0 0)
		(layer "User.9")
	)
	(pad "A1" smd circle
		(at -10.8 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A2" smd circle
		(at -10 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.028)
		(solder_mask_margin 0.05)
	)
	(pad "A3" smd circle
		(at -9.2 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.0263)
		(solder_mask_margin 0.05)
	)
	(pad "A4" smd circle
		(at -8.4 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.3822)
		(solder_mask_margin 0.05)
	)
	(pad "A5" smd circle
		(at -7.6 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.7601)
		(solder_mask_margin 0.05)
	)
	(pad "A6" smd circle
		(at -6.8 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A7" smd circle
		(at -6 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.9607)
		(solder_mask_margin 0.05)
	)
	(pad "A8" smd circle
		(at -5.2 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.2976)
		(solder_mask_margin 0.05)
	)
	(pad "A9" smd circle
		(at -4.4 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.2866)
		(solder_mask_margin 0.05)
	)
	(pad "A10" smd circle
		(at -3.6 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.5508)
		(solder_mask_margin 0.05)
	)
	(pad "A11" smd circle
		(at -2.8 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A12" smd circle
		(at -2 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.1776)
		(solder_mask_margin 0.05)
	)
	(pad "A13" smd circle
		(at -1.2 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.1696)
		(solder_mask_margin 0.05)
	)
	(pad "A14" smd circle
		(at -0.4 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.06576)
		(solder_mask_margin 0.05)
	)
	(pad "A15" smd circle
		(at 0.4 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.08623)
		(solder_mask_margin 0.05)
	)
	(pad "A16" smd circle
		(at 1.2 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A17" smd circle
		(at 2 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A18" smd circle
		(at 2.8 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A19" smd circle
		(at 3.6 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A20" smd circle
		(at 4.4 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A21" smd circle
		(at 5.2 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A22" smd circle
		(at 6 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.67674)
		(solder_mask_margin 0.05)
	)
	(pad "A23" smd circle
		(at 6.8 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.6795)
		(solder_mask_margin 0.05)
	)
	(pad "A24" smd circle
		(at 7.6 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.818)
		(solder_mask_margin 0.05)
	)
	(pad "A25" smd circle
		(at 8.4 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.83555)
		(solder_mask_margin 0.05)
	)
	(pad "A26" smd circle
		(at 9.2 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A27" smd circle
		(at 10 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.6532)
		(solder_mask_margin 0.05)
	)
	(pad "A28" smd circle
		(at 10.8 -10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AA1" smd circle
		(at -10.8 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AA2" smd circle
		(at -10 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.67457)
		(solder_mask_margin 0.05)
	)
	(pad "AA3" smd circle
		(at -9.2 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.68366)
		(solder_mask_margin 0.05)
	)
	(pad "AA4" smd circle
		(at -8.4 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.80203)
		(solder_mask_margin 0.05)
	)
	(pad "AA5" smd circle
		(at -7.6 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.42333)
		(solder_mask_margin 0.05)
	)
	(pad "AA6" smd circle
		(at -6.8 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AA7" smd circle
		(at -6 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.92909)
		(solder_mask_margin 0.05)
	)
	(pad "AA8" smd circle
		(at -5.2 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.93812)
		(solder_mask_margin 0.05)
	)
	(pad "AA9" smd circle
		(at -4.4 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.92022)
		(solder_mask_margin 0.05)
	)
	(pad "AA10" smd circle
		(at -3.6 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.54249)
		(solder_mask_margin 0.05)
	)
	(pad "AA11" smd circle
		(at -2.8 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AA12" smd circle
		(at -2 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.76749)
		(solder_mask_margin 0.05)
	)
	(pad "AA13" smd circle
		(at -1.2 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.21696)
		(solder_mask_margin 0.05)
	)
	(pad "AA14" smd circle
		(at -0.4 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.27431)
		(solder_mask_margin 0.05)
	)
	(pad "AA15" smd circle
		(at 0.4 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.0242)
		(solder_mask_margin 0.05)
	)
	(pad "AA16" smd circle
		(at 1.2 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AA17" smd circle
		(at 2 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.95089)
		(solder_mask_margin 0.05)
	)
	(pad "AA18" smd circle
		(at 2.8 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.71845)
		(solder_mask_margin 0.05)
	)
	(pad "AA19" smd circle
		(at 3.6 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.99561)
		(solder_mask_margin 0.05)
	)
	(pad "AA20" smd circle
		(at 4.4 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.77995)
		(solder_mask_margin 0.05)
	)
	(pad "AA21" smd circle
		(at 5.2 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AA22" smd circle
		(at 6 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.0066)
		(solder_mask_margin 0.05)
	)
	(pad "AA23" smd circle
		(at 6.8 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.1639)
		(solder_mask_margin 0.05)
	)
	(pad "AA24" smd circle
		(at 7.6 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AA25" smd circle
		(at 8.4 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AA26" smd circle
		(at 9.2 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AA27" smd circle
		(at 10 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.80721)
		(solder_mask_margin 0.05)
	)
	(pad "AA28" smd circle
		(at 10.8 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.80407)
		(solder_mask_margin 0.05)
	)
	(pad "AB1" smd circle
		(at -10.8 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.7112)
		(solder_mask_margin 0.05)
	)
	(pad "AB2" smd circle
		(at -10 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.7075)
		(solder_mask_margin 0.05)
	)
	(pad "AB3" smd circle
		(at -9.2 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AB4" smd circle
		(at -8.4 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.74219)
		(solder_mask_margin 0.05)
	)
	(pad "AB5" smd circle
		(at -7.6 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.71765)
		(solder_mask_margin 0.05)
	)
	(pad "AB6" smd circle
		(at -6.8 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.31073)
		(solder_mask_margin 0.05)
	)
	(pad "AB7" smd circle
		(at -6 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.01204)
		(solder_mask_margin 0.05)
	)
	(pad "AB8" smd circle
		(at -5.2 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AB9" smd circle
		(at -4.4 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.54113)
		(solder_mask_margin 0.05)
	)
	(pad "AB10" smd circle
		(at -3.6 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.76911)
		(solder_mask_margin 0.05)
	)
	(pad "AB11" smd circle
		(at -2.8 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.04251)
		(solder_mask_margin 0.05)
	)
	(pad "AB12" smd circle
		(at -2 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.50945)
		(solder_mask_margin 0.05)
	)
	(pad "AB13" smd circle
		(at -1.2 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AB14" smd circle
		(at -0.4 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.1841)
		(solder_mask_margin 0.05)
	)
	(pad "AB15" smd circle
		(at 0.4 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.95987)
		(solder_mask_margin 0.05)
	)
	(pad "AB16" smd circle
		(at 1.2 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.9636)
		(solder_mask_margin 0.05)
	)
	(pad "AB17" smd circle
		(at 2 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.96709)
		(solder_mask_margin 0.05)
	)
	(pad "AB18" smd circle
		(at 2.8 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AB19" smd circle
		(at 3.6 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.96812)
		(solder_mask_margin 0.05)
	)
	(pad "AB20" smd circle
		(at 4.4 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.78487)
		(solder_mask_margin 0.05)
	)
	(pad "AB21" smd circle
		(at 5.2 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.67923)
		(solder_mask_margin 0.05)
	)
	(pad "AB22" smd circle
		(at 6 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.0201)
		(solder_mask_margin 0.05)
	)
	(pad "AB23" smd circle
		(at 6.8 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AB24" smd circle
		(at 7.6 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.1056)
		(solder_mask_margin 0.05)
	)
	(pad "AB25" smd circle
		(at 8.4 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.0929)
		(solder_mask_margin 0.05)
	)
	(pad "AB26" smd circle
		(at 9.2 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AB27" smd circle
		(at 10 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AB28" smd circle
		(at 10.8 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AC1" smd circle
		(at -10.8 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.6382)
		(solder_mask_margin 0.05)
	)
	(pad "AC2" smd circle
		(at -10 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.0518)
		(solder_mask_margin 0.05)
	)
	(pad "AC3" smd circle
		(at -9.2 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.77906)
		(solder_mask_margin 0.05)
	)
	(pad "AC4" smd circle
		(at -8.4 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.65439)
		(solder_mask_margin 0.05)
	)
	(pad "AC5" smd circle
		(at -7.6 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AC6" smd circle
		(at -6.8 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.40494)
		(solder_mask_margin 0.05)
	)
	(pad "AC7" smd circle
		(at -6 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.45932)
		(solder_mask_margin 0.05)
	)
	(pad "AC8" smd circle
		(at -5.2 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.34958)
		(solder_mask_margin 0.05)
	)
	(pad "AC9" smd circle
		(at -4.4 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.44591)
		(solder_mask_margin 0.05)
	)
	(pad "AC10" smd circle
		(at -3.6 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AC11" smd circle
		(at -2.8 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.12534)
		(solder_mask_margin 0.05)
	)
	(pad "AC12" smd circle
		(at -2 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.12521)
		(solder_mask_margin 0.05)
	)
	(pad "AC13" smd circle
		(at -1.2 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.50297)
		(solder_mask_margin 0.05)
	)
	(pad "AC14" smd circle
		(at -0.4 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.20682)
		(solder_mask_margin 0.05)
	)
	(pad "AC15" smd circle
		(at 0.4 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AC16" smd circle
		(at 1.2 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.78918)
		(solder_mask_margin 0.05)
	)
	(pad "AC17" smd circle
		(at 2 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.79573)
		(solder_mask_margin 0.05)
	)
	(pad "AC18" smd circle
		(at 2.8 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.97116)
		(solder_mask_margin 0.05)
	)
	(pad "AC19" smd circle
		(at 3.6 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.8751)
		(solder_mask_margin 0.05)
	)
	(pad "AC20" smd circle
		(at 4.4 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AC21" smd circle
		(at 5.2 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.69928)
		(solder_mask_margin 0.05)
	)
	(pad "AC22" smd circle
		(at 6 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.6324)
		(solder_mask_margin 0.05)
	)
	(pad "AC23" smd circle
		(at 6.8 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.88182)
		(solder_mask_margin 0.05)
	)
	(pad "AC24" smd circle
		(at 7.6 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.1275)
		(solder_mask_margin 0.05)
	)
	(pad "AC25" smd circle
		(at 8.4 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AC26" smd circle
		(at 9.2 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.1482)
		(solder_mask_margin 0.05)
	)
	(pad "AC27" smd circle
		(at 10 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.1534)
		(solder_mask_margin 0.05)
	)
	(pad "AC28" smd circle
		(at 10.8 6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.8354)
		(solder_mask_margin 0.05)
	)
	(pad "AD1" smd circle
		(at -10.8 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.0114)
		(solder_mask_margin 0.05)
	)
	(pad "AD2" smd circle
		(at -10 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AD3" smd circle
		(at -9.2 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.0219)
		(solder_mask_margin 0.05)
	)
	(pad "AD4" smd circle
		(at -8.4 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.0479)
		(solder_mask_margin 0.05)
	)
	(pad "AD5" smd circle
		(at -7.6 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.049)
		(solder_mask_margin 0.05)
	)
	(pad "AD6" smd circle
		(at -6.8 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.0983)
		(solder_mask_margin 0.05)
	)
	(pad "AD7" smd circle
		(at -6 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AD8" smd circle
		(at -5.2 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.8313)
		(solder_mask_margin 0.05)
	)
	(pad "AD9" smd circle
		(at -4.4 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.8301)
		(solder_mask_margin 0.05)
	)
	(pad "AD10" smd circle
		(at -3.6 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.96025)
		(solder_mask_margin 0.05)
	)
	(pad "AD11" smd circle
		(at -2.8 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.98001)
		(solder_mask_margin 0.05)
	)
	(pad "AD12" smd circle
		(at -2 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AD13" smd circle
		(at -1.2 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.09506)
		(solder_mask_margin 0.05)
	)
	(pad "AD14" smd circle
		(at -0.4 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.0849)
		(solder_mask_margin 0.05)
	)
	(pad "AD15" smd circle
		(at 0.4 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.17625)
		(solder_mask_margin 0.05)
	)
	(pad "AD16" smd circle
		(at 1.2 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.91202)
		(solder_mask_margin 0.05)
	)
	(pad "AD17" smd circle
		(at 2 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AD18" smd circle
		(at 2.8 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.94152)
		(solder_mask_margin 0.05)
	)
	(pad "AD19" smd circle
		(at 3.6 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.90395)
		(solder_mask_margin 0.05)
	)
	(pad "AD20" smd circle
		(at 4.4 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.61969)
		(solder_mask_margin 0.05)
	)
	(pad "AD21" smd circle
		(at 5.2 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.6308)
		(solder_mask_margin 0.05)
	)
	(pad "AD22" smd circle
		(at 6 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AD23" smd circle
		(at 6.8 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.86993)
		(solder_mask_margin 0.05)
	)
	(pad "AD24" smd circle
		(at 7.6 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.1423)
		(solder_mask_margin 0.05)
	)
	(pad "AD25" smd circle
		(at 8.4 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.87738)
		(solder_mask_margin 0.05)
	)
	(pad "AD26" smd circle
		(at 9.2 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.85267)
		(solder_mask_margin 0.05)
	)
	(pad "AD27" smd circle
		(at 10 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AD28" smd circle
		(at 10.8 7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.8493)
		(solder_mask_margin 0.05)
	)
	(pad "AE1" smd circle
		(at -10.8 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.6003)
		(solder_mask_margin 0.05)
	)
	(pad "AE2" smd circle
		(at -10 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.0661)
		(solder_mask_margin 0.05)
	)
	(pad "AE3" smd circle
		(at -9.2 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.0243)
		(solder_mask_margin 0.05)
	)
	(pad "AE4" smd circle
		(at -8.4 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AE5" smd circle
		(at -7.6 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.0256)
		(solder_mask_margin 0.05)
	)
	(pad "AE6" smd circle
		(at -6.8 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.0942)
		(solder_mask_margin 0.05)
	)
	(pad "AE7" smd circle
		(at -6 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.7933)
		(solder_mask_margin 0.05)
	)
	(pad "AE8" smd circle
		(at -5.2 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.7856)
		(solder_mask_margin 0.05)
	)
	(pad "AE9" smd circle
		(at -4.4 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AE10" smd circle
		(at -3.6 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.0534)
		(solder_mask_margin 0.05)
	)
	(pad "AE11" smd circle
		(at -2.8 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.92208)
		(solder_mask_margin 0.05)
	)
	(pad "AE12" smd circle
		(at -2 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.94119)
		(solder_mask_margin 0.05)
	)
	(pad "AE13" smd circle
		(at -1.2 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.18744)
		(solder_mask_margin 0.05)
	)
	(pad "AE14" smd circle
		(at -0.4 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AE15" smd circle
		(at 0.4 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.19851)
		(solder_mask_margin 0.05)
	)
	(pad "AE16" smd circle
		(at 1.2 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.94227)
		(solder_mask_margin 0.05)
	)
	(pad "AE17" smd circle
		(at 2 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.41218)
		(solder_mask_margin 0.05)
	)
	(pad "AE18" smd circle
		(at 2.8 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.29797)
		(solder_mask_margin 0.05)
	)
	(pad "AE19" smd circle
		(at 3.6 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AE20" smd circle
		(at 4.4 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.62025)
		(solder_mask_margin 0.05)
	)
	(pad "AE21" smd circle
		(at 5.2 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.35228)
		(solder_mask_margin 0.05)
	)
	(pad "AE22" smd circle
		(at 6 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.36029)
		(solder_mask_margin 0.05)
	)
	(pad "AE23" smd circle
		(at 6.8 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.18586)
		(solder_mask_margin 0.05)
	)
	(pad "AE24" smd circle
		(at 7.6 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AE25" smd circle
		(at 8.4 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.0083)
		(solder_mask_margin 0.05)
	)
	(pad "AE26" smd circle
		(at 9.2 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.0164)
		(solder_mask_margin 0.05)
	)
	(pad "AE27" smd circle
		(at 10 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.5576)
		(solder_mask_margin 0.05)
	)
	(pad "AE28" smd circle
		(at 10.8 8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.5571)
		(solder_mask_margin 0.05)
	)
	(pad "AF1" smd circle
		(at -10.8 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.7536)
		(solder_mask_margin 0.05)
	)
	(pad "AF2" smd circle
		(at -10 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.5751)
		(solder_mask_margin 0.05)
	)
	(pad "AF3" smd circle
		(at -9.2 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.5054)
		(solder_mask_margin 0.05)
	)
	(pad "AF4" smd circle
		(at -8.4 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.27)
		(solder_mask_margin 0.05)
	)
	(pad "AF5" smd circle
		(at -7.6 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.0428)
		(solder_mask_margin 0.05)
	)
	(pad "AF6" smd circle
		(at -6.8 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AF7" smd circle
		(at -6 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.8042)
		(solder_mask_margin 0.05)
	)
	(pad "AF8" smd circle
		(at -5.2 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.7037)
		(solder_mask_margin 0.05)
	)
	(pad "AF9" smd circle
		(at -4.4 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.7025)
		(solder_mask_margin 0.05)
	)
	(pad "AF10" smd circle
		(at -3.6 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.0569)
		(solder_mask_margin 0.05)
	)
	(pad "AF11" smd circle
		(at -2.8 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AF12" smd circle
		(at -2 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.5781)
		(solder_mask_margin 0.05)
	)
	(pad "AF13" smd circle
		(at -1.2 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.20466)
		(solder_mask_margin 0.05)
	)
	(pad "AF14" smd circle
		(at -0.4 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.64364)
		(solder_mask_margin 0.05)
	)
	(pad "AF15" smd circle
		(at 0.4 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.82702)
		(solder_mask_margin 0.05)
	)
	(pad "AF16" smd circle
		(at 1.2 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AF17" smd circle
		(at 2 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.42416)
		(solder_mask_margin 0.05)
	)
	(pad "AF18" smd circle
		(at 2.8 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.30425)
		(solder_mask_margin 0.05)
	)
	(pad "AF19" smd circle
		(at 3.6 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.60109)
		(solder_mask_margin 0.05)
	)
	(pad "AF20" smd circle
		(at 4.4 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.88895)
		(solder_mask_margin 0.05)
	)
	(pad "AF21" smd circle
		(at 5.2 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AF22" smd circle
		(at 6 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.56548)
		(solder_mask_margin 0.05)
	)
	(pad "AF23" smd circle
		(at 6.8 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.19596)
		(solder_mask_margin 0.05)
	)
	(pad "AF24" smd circle
		(at 7.6 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.1677)
		(solder_mask_margin 0.05)
	)
	(pad "AF25" smd circle
		(at 8.4 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.1547)
		(solder_mask_margin 0.05)
	)
	(pad "AF26" smd circle
		(at 9.2 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AF27" smd circle
		(at 10 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.9872)
		(solder_mask_margin 0.05)
	)
	(pad "AF28" smd circle
		(at 10.8 9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.0055)
		(solder_mask_margin 0.05)
	)
	(pad "AG1" smd circle
		(at -10.8 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.2077)
		(solder_mask_margin 0.05)
	)
	(pad "AG2" smd circle
		(at -10 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.5811)
		(solder_mask_margin 0.05)
	)
	(pad "AG3" smd circle
		(at -9.2 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AG4" smd circle
		(at -8.4 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.8648)
		(solder_mask_margin 0.05)
	)
	(pad "AG5" smd circle
		(at -7.6 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.4397)
		(solder_mask_margin 0.05)
	)
	(pad "AG6" smd circle
		(at -6.8 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.4005)
		(solder_mask_margin 0.05)
	)
	(pad "AG7" smd circle
		(at -6 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.8124)
		(solder_mask_margin 0.05)
	)
	(pad "AG8" smd circle
		(at -5.2 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AG9" smd circle
		(at -4.4 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.1596)
		(solder_mask_margin 0.05)
	)
	(pad "AG10" smd circle
		(at -3.6 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.6114)
		(solder_mask_margin 0.05)
	)
	(pad "AG11" smd circle
		(at -2.8 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.5982)
		(solder_mask_margin 0.05)
	)
	(pad "AG12" smd circle
		(at -2 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.5584)
		(solder_mask_margin 0.05)
	)
	(pad "AG13" smd circle
		(at -1.2 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AG14" smd circle
		(at -0.4 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.65591)
		(solder_mask_margin 0.05)
	)
	(pad "AG15" smd circle
		(at 0.4 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.85578)
		(solder_mask_margin 0.05)
	)
	(pad "AG16" smd circle
		(at 1.2 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.18115)
		(solder_mask_margin 0.05)
	)
	(pad "AG17" smd circle
		(at 2 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.89895)
		(solder_mask_margin 0.05)
	)
	(pad "AG18" smd circle
		(at 2.8 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AG19" smd circle
		(at 3.6 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.60797)
		(solder_mask_margin 0.05)
	)
	(pad "AG20" smd circle
		(at 4.4 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.89104)
		(solder_mask_margin 0.05)
	)
	(pad "AG21" smd circle
		(at 5.2 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.89847)
		(solder_mask_margin 0.05)
	)
	(pad "AG22" smd circle
		(at 6 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.58538)
		(solder_mask_margin 0.05)
	)
	(pad "AG23" smd circle
		(at 6.8 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AG24" smd circle
		(at 7.6 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.91772)
		(solder_mask_margin 0.05)
	)
	(pad "AG25" smd circle
		(at 8.4 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.3572)
		(solder_mask_margin 0.05)
	)
	(pad "AG26" smd circle
		(at 9.2 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.3378)
		(solder_mask_margin 0.05)
	)
	(pad "AG27" smd circle
		(at 10 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.5511)
		(solder_mask_margin 0.05)
	)
	(pad "AG28" smd circle
		(at 10.8 10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.5567)
		(solder_mask_margin 0.05)
	)
	(pad "AH1" smd circle
		(at -10.8 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AH2" smd circle
		(at -10 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.8472)
		(solder_mask_margin 0.05)
	)
	(pad "AH3" smd circle
		(at -9.2 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.3125)
		(solder_mask_margin 0.05)
	)
	(pad "AH4" smd circle
		(at -8.4 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.6604)
		(solder_mask_margin 0.05)
	)
	(pad "AH5" smd circle
		(at -7.6 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AH6" smd circle
		(at -6.8 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.4087)
		(solder_mask_margin 0.05)
	)
	(pad "AH7" smd circle
		(at -6 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.9112)
		(solder_mask_margin 0.05)
	)
	(pad "AH8" smd circle
		(at -5.2 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.9199)
		(solder_mask_margin 0.05)
	)
	(pad "AH9" smd circle
		(at -4.4 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.1831)
		(solder_mask_margin 0.05)
	)
	(pad "AH10" smd circle
		(at -3.6 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AH11" smd circle
		(at -2.8 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.1724)
		(solder_mask_margin 0.05)
	)
	(pad "AH12" smd circle
		(at -2 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.2019)
		(solder_mask_margin 0.05)
	)
	(pad "AH13" smd circle
		(at -1.2 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.226)
		(solder_mask_margin 0.05)
	)
	(pad "AH14" smd circle
		(at -0.4 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.2241)
		(solder_mask_margin 0.05)
	)
	(pad "AH15" smd circle
		(at 0.4 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AH16" smd circle
		(at 1.2 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.16717)
		(solder_mask_margin 0.05)
	)
	(pad "AH17" smd circle
		(at 2 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.91894)
		(solder_mask_margin 0.05)
	)
	(pad "AH18" smd circle
		(at 2.8 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.06068)
		(solder_mask_margin 0.05)
	)
	(pad "AH19" smd circle
		(at 3.6 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.06854)
		(solder_mask_margin 0.05)
	)
	(pad "AH20" smd circle
		(at 4.4 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AH21" smd circle
		(at 5.2 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.88398)
		(solder_mask_margin 0.05)
	)
	(pad "AH22" smd circle
		(at 6 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.76726)
		(solder_mask_margin 0.05)
	)
	(pad "AH23" smd circle
		(at 6.8 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.77593)
		(solder_mask_margin 0.05)
	)
	(pad "AH24" smd circle
		(at 7.6 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.91019)
		(solder_mask_margin 0.05)
	)
	(pad "AH25" smd circle
		(at 8.4 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "AH26" smd circle
		(at 9.2 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.3829)
		(solder_mask_margin 0.05)
	)
	(pad "AH27" smd circle
		(at 10 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 12.3923)
		(solder_mask_margin 0.05)
	)
	(pad "AH28" smd circle
		(at 10.8 10.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B1" smd circle
		(at -10.8 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.878)
		(solder_mask_margin 0.05)
	)
	(pad "B2" smd circle
		(at -10 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.0086)
		(solder_mask_margin 0.05)
	)
	(pad "B3" smd circle
		(at -9.2 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B4" smd circle
		(at -8.4 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.3744)
		(solder_mask_margin 0.05)
	)
	(pad "B5" smd circle
		(at -7.6 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.7544)
		(solder_mask_margin 0.05)
	)
	(pad "B6" smd circle
		(at -6.8 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.7885)
		(solder_mask_margin 0.05)
	)
	(pad "B7" smd circle
		(at -6 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.95)
		(solder_mask_margin 0.05)
	)
	(pad "B8" smd circle
		(at -5.2 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B9" smd circle
		(at -4.4 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.3749)
		(solder_mask_margin 0.05)
	)
	(pad "B10" smd circle
		(at -3.6 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.5494)
		(solder_mask_margin 0.05)
	)
	(pad "B11" smd circle
		(at -2.8 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.2826)
		(solder_mask_margin 0.05)
	)
	(pad "B12" smd circle
		(at -2 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.2821)
		(solder_mask_margin 0.05)
	)
	(pad "B13" smd circle
		(at -1.2 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B14" smd circle
		(at -0.4 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.82055)
		(solder_mask_margin 0.05)
	)
	(pad "B15" smd circle
		(at 0.4 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.67017)
		(solder_mask_margin 0.05)
	)
	(pad "B16" smd circle
		(at 1.2 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.68768)
		(solder_mask_margin 0.05)
	)
	(pad "B17" smd circle
		(at 2 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.40353)
		(solder_mask_margin 0.05)
	)
	(pad "B18" smd circle
		(at 2.8 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B19" smd circle
		(at 3.6 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B20" smd circle
		(at 4.4 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B21" smd circle
		(at 5.2 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.27055)
		(solder_mask_margin 0.05)
	)
	(pad "B22" smd circle
		(at 6 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.15252)
		(solder_mask_margin 0.05)
	)
	(pad "B23" smd circle
		(at 6.8 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B24" smd circle
		(at 7.6 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.2583)
		(solder_mask_margin 0.05)
	)
	(pad "B25" smd circle
		(at 8.4 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.5406)
		(solder_mask_margin 0.05)
	)
	(pad "B26" smd circle
		(at 9.2 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.5611)
		(solder_mask_margin 0.05)
	)
	(pad "B27" smd circle
		(at 10 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.6587)
		(solder_mask_margin 0.05)
	)
	(pad "B28" smd circle
		(at 10.8 -10)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.0709)
		(solder_mask_margin 0.05)
	)
	(pad "C1" smd circle
		(at -10.8 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.8573)
		(solder_mask_margin 0.05)
	)
	(pad "C2" smd circle
		(at -10 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.0053)
		(solder_mask_margin 0.05)
	)
	(pad "C3" smd circle
		(at -9.2 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.0362)
		(solder_mask_margin 0.05)
	)
	(pad "C4" smd circle
		(at -8.4 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.3799)
		(solder_mask_margin 0.05)
	)
	(pad "C5" smd circle
		(at -7.6 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "C6" smd circle
		(at -6.8 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.7707)
		(solder_mask_margin 0.05)
	)
	(pad "C7" smd circle
		(at -6 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.5656)
		(solder_mask_margin 0.05)
	)
	(pad "C8" smd circle
		(at -5.2 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.5617)
		(solder_mask_margin 0.05)
	)
	(pad "C9" smd circle
		(at -4.4 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.3545)
		(solder_mask_margin 0.05)
	)
	(pad "C10" smd circle
		(at -3.6 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "C11" smd circle
		(at -2.8 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.504)
		(solder_mask_margin 0.05)
	)
	(pad "C12" smd circle
		(at -2 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.0782)
		(solder_mask_margin 0.05)
	)
	(pad "C13" smd circle
		(at -1.2 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.0706)
		(solder_mask_margin 0.05)
	)
	(pad "C14" smd circle
		(at -0.4 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.8074)
		(solder_mask_margin 0.05)
	)
	(pad "C15" smd circle
		(at 0.4 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "C16" smd circle
		(at 1.2 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.32775)
		(solder_mask_margin 0.05)
	)
	(pad "C17" smd circle
		(at 2 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.31713)
		(solder_mask_margin 0.05)
	)
	(pad "C18" smd circle
		(at 2.8 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "C19" smd circle
		(at 3.6 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "C20" smd circle
		(at 4.4 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "C21" smd circle
		(at 5.2 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.26504)
		(solder_mask_margin 0.05)
	)
	(pad "C22" smd circle
		(at 6 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.17872)
		(solder_mask_margin 0.05)
	)
	(pad "C23" smd circle
		(at 6.8 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.27919)
		(solder_mask_margin 0.05)
	)
	(pad "C24" smd circle
		(at 7.6 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.2704)
		(solder_mask_margin 0.05)
	)
	(pad "C25" smd circle
		(at 8.4 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "C26" smd circle
		(at 9.2 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.02)
		(solder_mask_margin 0.05)
	)
	(pad "C27" smd circle
		(at 10 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.024)
		(solder_mask_margin 0.05)
	)
	(pad "C28" smd circle
		(at 10.8 -9.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.0697)
		(solder_mask_margin 0.05)
	)
	(pad "D1" smd circle
		(at -10.8 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.1649)
		(solder_mask_margin 0.05)
	)
	(pad "D2" smd circle
		(at -10 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "D3" smd circle
		(at -9.2 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.0346)
		(solder_mask_margin 0.05)
	)
	(pad "D4" smd circle
		(at -8.4 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.3704)
		(solder_mask_margin 0.05)
	)
	(pad "D5" smd circle
		(at -7.6 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.2415)
		(solder_mask_margin 0.05)
	)
	(pad "D6" smd circle
		(at -6.8 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.2234)
		(solder_mask_margin 0.05)
	)
	(pad "D7" smd circle
		(at -6 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "D8" smd circle
		(at -5.2 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.56022)
		(solder_mask_margin 0.05)
	)
	(pad "D9" smd circle
		(at -4.4 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.8662)
		(solder_mask_margin 0.05)
	)
	(pad "D10" smd circle
		(at -3.6 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.8645)
		(solder_mask_margin 0.05)
	)
	(pad "D11" smd circle
		(at -2.8 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.4978)
		(solder_mask_margin 0.05)
	)
	(pad "D12" smd circle
		(at -2 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "D13" smd circle
		(at -1.2 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.44203)
		(solder_mask_margin 0.05)
	)
	(pad "D14" smd circle
		(at -0.4 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.44014)
		(solder_mask_margin 0.05)
	)
	(pad "D15" smd circle
		(at 0.4 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.26332)
		(solder_mask_margin 0.05)
	)
	(pad "D16" smd circle
		(at 1.2 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.31505)
		(solder_mask_margin 0.05)
	)
	(pad "D17" smd circle
		(at 2 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "D18" smd circle
		(at 2.8 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "D19" smd circle
		(at 3.6 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "D20" smd circle
		(at 4.4 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.22917)
		(solder_mask_margin 0.05)
	)
	(pad "D21" smd circle
		(at 5.2 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.26258)
		(solder_mask_margin 0.05)
	)
	(pad "D22" smd circle
		(at 6 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "D23" smd circle
		(at 6.8 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.28769)
		(solder_mask_margin 0.05)
	)
	(pad "D24" smd circle
		(at 7.6 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.5911)
		(solder_mask_margin 0.05)
	)
	(pad "D25" smd circle
		(at 8.4 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.6354)
		(solder_mask_margin 0.05)
	)
	(pad "D26" smd circle
		(at 9.2 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "D27" smd circle
		(at 10 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "D28" smd circle
		(at 10.8 -8.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "E1" smd circle
		(at -10.8 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.162)
		(solder_mask_margin 0.05)
	)
	(pad "E2" smd circle
		(at -10 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.019)
		(solder_mask_margin 0.05)
	)
	(pad "E3" smd circle
		(at -9.2 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 13.0196)
		(solder_mask_margin 0.05)
	)
	(pad "E4" smd circle
		(at -8.4 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "E5" smd circle
		(at -7.6 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.2842)
		(solder_mask_margin 0.05)
	)
	(pad "E6" smd circle
		(at -6.8 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.2287)
		(solder_mask_margin 0.05)
	)
	(pad "E7" smd circle
		(at -6 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.2264)
		(solder_mask_margin 0.05)
	)
	(pad "E8" smd circle
		(at -5.2 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.53756)
		(solder_mask_margin 0.05)
	)
	(pad "E9" smd circle
		(at -4.4 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "E10" smd circle
		(at -3.6 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.1396)
		(solder_mask_margin 0.05)
	)
	(pad "E11" smd circle
		(at -2.8 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.1296)
		(solder_mask_margin 0.05)
	)
	(pad "E12" smd circle
		(at -2 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.58575)
		(solder_mask_margin 0.05)
	)
	(pad "E13" smd circle
		(at -1.2 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.47473)
		(solder_mask_margin 0.05)
	)
	(pad "E14" smd circle
		(at -0.4 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "E15" smd circle
		(at 0.4 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.24297)
		(solder_mask_margin 0.05)
	)
	(pad "E16" smd circle
		(at 1.2 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.39802)
		(solder_mask_margin 0.05)
	)
	(pad "E17" smd circle
		(at 2 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.36249)
		(solder_mask_margin 0.05)
	)
	(pad "E18" smd circle
		(at 2.8 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "E19" smd circle
		(at 3.6 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "E20" smd circle
		(at 4.4 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "E21" smd circle
		(at 5.2 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.66751)
		(solder_mask_margin 0.05)
	)
	(pad "E22" smd circle
		(at 6 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.67387)
		(solder_mask_margin 0.05)
	)
	(pad "E23" smd circle
		(at 6.8 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.84248)
		(solder_mask_margin 0.05)
	)
	(pad "E24" smd circle
		(at 7.6 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "E25" smd circle
		(at 8.4 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "E26" smd circle
		(at 9.2 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "E27" smd circle
		(at 10 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.69631)
		(solder_mask_margin 0.05)
	)
	(pad "E28" smd circle
		(at 10.8 -7.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.6902)
		(solder_mask_margin 0.05)
	)
	(pad "F1" smd circle
		(at -10.8 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "F2" smd circle
		(at -10 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.6584)
		(solder_mask_margin 0.05)
	)
	(pad "F3" smd circle
		(at -9.2 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.1391)
		(solder_mask_margin 0.05)
	)
	(pad "F4" smd circle
		(at -8.4 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.1265)
		(solder_mask_margin 0.05)
	)
	(pad "F5" smd circle
		(at -7.6 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 11.2892)
		(solder_mask_margin 0.05)
	)
	(pad "F6" smd circle
		(at -6.8 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "F7" smd circle
		(at -6 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.0709)
		(solder_mask_margin 0.05)
	)
	(pad "F8" smd circle
		(at -5.2 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.0755)
		(solder_mask_margin 0.05)
	)
	(pad "F9" smd circle
		(at -4.4 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.52059)
		(solder_mask_margin 0.05)
	)
	(pad "F10" smd circle
		(at -3.6 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.30487)
		(solder_mask_margin 0.05)
	)
	(pad "F11" smd circle
		(at -2.8 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "F12" smd circle
		(at -2 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.5666)
		(solder_mask_margin 0.05)
	)
	(pad "F13" smd circle
		(at -1.2 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.46737)
		(solder_mask_margin 0.05)
	)
	(pad "F14" smd circle
		(at -0.4 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.4361)
		(solder_mask_margin 0.05)
	)
	(pad "F15" smd circle
		(at 0.4 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.99932)
		(solder_mask_margin 0.05)
	)
	(pad "F16" smd circle
		(at 1.2 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "F17" smd circle
		(at 2 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.97244)
		(solder_mask_margin 0.05)
	)
	(pad "F18" smd circle
		(at 2.8 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.24189)
		(solder_mask_margin 0.05)
	)
	(pad "F19" smd circle
		(at 3.6 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.25108)
		(solder_mask_margin 0.05)
	)
	(pad "F20" smd circle
		(at 4.4 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.00141)
		(solder_mask_margin 0.05)
	)
	(pad "F21" smd circle
		(at 5.2 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "F22" smd circle
		(at 6 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.96772)
		(solder_mask_margin 0.05)
	)
	(pad "F23" smd circle
		(at 6.8 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.84374)
		(solder_mask_margin 0.05)
	)
	(pad "F24" smd circle
		(at 7.6 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "F25" smd circle
		(at 8.4 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.02777)
		(solder_mask_margin 0.05)
	)
	(pad "F26" smd circle
		(at 9.2 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.0161)
		(solder_mask_margin 0.05)
	)
	(pad "F27" smd circle
		(at 10 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "F28" smd circle
		(at 10.8 -6.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "G1" smd circle
		(at -10.8 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.677)
		(solder_mask_margin 0.05)
	)
	(pad "G2" smd circle
		(at -10 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.9501)
		(solder_mask_margin 0.05)
	)
	(pad "G3" smd circle
		(at -9.2 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "G4" smd circle
		(at -8.4 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.9783)
		(solder_mask_margin 0.05)
	)
	(pad "G5" smd circle
		(at -7.6 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.9752)
		(solder_mask_margin 0.05)
	)
	(pad "G6" smd circle
		(at -6.8 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.82995)
		(solder_mask_margin 0.05)
	)
	(pad "G7" smd circle
		(at -6 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.81857)
		(solder_mask_margin 0.05)
	)
	(pad "G8" smd circle
		(at -5.2 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "G9" smd circle
		(at -4.4 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.51476)
		(solder_mask_margin 0.05)
	)
	(pad "G10" smd circle
		(at -3.6 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.28648)
		(solder_mask_margin 0.05)
	)
	(pad "G11" smd circle
		(at -2.8 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.4733)
		(solder_mask_margin 0.05)
	)
	(pad "G12" smd circle
		(at -2 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.45911)
		(solder_mask_margin 0.05)
	)
	(pad "G13" smd circle
		(at -1.2 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "G14" smd circle
		(at -0.4 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.45984)
		(solder_mask_margin 0.05)
	)
	(pad "G15" smd circle
		(at 0.4 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.99337)
		(solder_mask_margin 0.05)
	)
	(pad "G16" smd circle
		(at 1.2 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.36874)
		(solder_mask_margin 0.05)
	)
	(pad "G17" smd circle
		(at 2 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.94326)
		(solder_mask_margin 0.05)
	)
	(pad "G18" smd circle
		(at 2.8 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "G19" smd circle
		(at 3.6 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.62555)
		(solder_mask_margin 0.05)
	)
	(pad "G20" smd circle
		(at 4.4 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.00125)
		(solder_mask_margin 0.05)
	)
	(pad "G21" smd circle
		(at 5.2 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.71678)
		(solder_mask_margin 0.05)
	)
	(pad "G22" smd circle
		(at 6 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.96348)
		(solder_mask_margin 0.05)
	)
	(pad "G23" smd circle
		(at 6.8 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.66387)
		(solder_mask_margin 0.05)
	)
	(pad "G24" smd circle
		(at 7.6 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "G25" smd circle
		(at 8.4 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "G26" smd circle
		(at 9.2 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "G27" smd circle
		(at 10 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.6143)
		(solder_mask_margin 0.05)
	)
	(pad "G28" smd circle
		(at 10.8 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.60742)
		(solder_mask_margin 0.05)
	)
	(pad "H1" smd circle
		(at -10.8 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.7083)
		(solder_mask_margin 0.05)
	)
	(pad "H2" smd circle
		(at -10 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.9609)
		(solder_mask_margin 0.05)
	)
	(pad "H3" smd circle
		(at -9.2 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.97706)
		(solder_mask_margin 0.05)
	)
	(pad "H4" smd circle
		(at -8.4 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.98256)
		(solder_mask_margin 0.05)
	)
	(pad "H5" smd circle
		(at -7.6 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "H6" smd circle
		(at -6.8 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.12506)
		(solder_mask_margin 0.05)
	)
	(pad "H7" smd circle
		(at -6 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.1322)
		(solder_mask_margin 0.05)
	)
	(pad "H8" smd circle
		(at -5.2 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.98125)
		(solder_mask_margin 0.05)
	)
	(pad "H9" smd circle
		(at -4.4 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.8834)
		(solder_mask_margin 0.05)
	)
	(pad "H10" smd circle
		(at -3.6 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "H11" smd circle
		(at -2.8 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.94986)
		(solder_mask_margin 0.05)
	)
	(pad "H12" smd circle
		(at -2 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.30584)
		(solder_mask_margin 0.05)
	)
	(pad "H13" smd circle
		(at -1.2 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.60705)
		(solder_mask_margin 0.05)
	)
	(pad "H14" smd circle
		(at -0.4 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.29063)
		(solder_mask_margin 0.05)
	)
	(pad "H15" smd circle
		(at 0.4 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "H16" smd circle
		(at 1.2 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.37398)
		(solder_mask_margin 0.05)
	)
	(pad "H17" smd circle
		(at 2 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.06126)
		(solder_mask_margin 0.05)
	)
	(pad "H18" smd circle
		(at 2.8 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.64296)
		(solder_mask_margin 0.05)
	)
	(pad "H19" smd circle
		(at 3.6 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.16961)
		(solder_mask_margin 0.05)
	)
	(pad "H20" smd circle
		(at 4.4 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "H21" smd circle
		(at 5.2 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.71141)
		(solder_mask_margin 0.05)
	)
	(pad "H22" smd circle
		(at 6 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.55981)
		(solder_mask_margin 0.05)
	)
	(pad "H23" smd circle
		(at 6.8 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "H24" smd circle
		(at 7.6 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "H25" smd circle
		(at 8.4 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.8429)
		(solder_mask_margin 0.05)
	)
	(pad "H26" smd circle
		(at 9.2 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.83876)
		(solder_mask_margin 0.05)
	)
	(pad "H27" smd circle
		(at 10 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "H28" smd circle
		(at 10.8 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "J1" smd circle
		(at -10.8 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.7211)
		(solder_mask_margin 0.05)
	)
	(pad "J2" smd circle
		(at -10 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "J3" smd circle
		(at -9.2 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.4035)
		(solder_mask_margin 0.05)
	)
	(pad "J4" smd circle
		(at -8.4 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.8205)
		(solder_mask_margin 0.05)
	)
	(pad "J5" smd circle
		(at -7.6 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.81283)
		(solder_mask_margin 0.05)
	)
	(pad "J6" smd circle
		(at -6.8 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.19118)
		(solder_mask_margin 0.05)
	)
	(pad "J7" smd circle
		(at -6 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "J8" smd circle
		(at -5.2 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.33324)
		(solder_mask_margin 0.05)
	)
	(pad "J9" smd circle
		(at -4.4 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.75425)
		(solder_mask_margin 0.05)
	)
	(pad "J10" smd circle
		(at -3.6 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.89012)
		(solder_mask_margin 0.05)
	)
	(pad "J11" smd circle
		(at -2.8 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 4.75161)
		(solder_mask_margin 0.05)
	)
	(pad "J12" smd circle
		(at -2 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.70843)
		(solder_mask_margin 0.05)
	)
	(pad "J13" smd circle
		(at -1.2 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 3.98627)
		(solder_mask_margin 0.05)
	)
	(pad "J14" smd circle
		(at -0.4 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.28474)
		(solder_mask_margin 0.05)
	)
	(pad "J15" smd circle
		(at 0.4 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.18934)
		(solder_mask_margin 0.05)
	)
	(pad "J16" smd circle
		(at 1.2 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.06497)
		(solder_mask_margin 0.05)
	)
	(pad "J17" smd circle
		(at 2 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "J18" smd circle
		(at 2.8 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.33637)
		(solder_mask_margin 0.05)
	)
	(pad "J19" smd circle
		(at 3.6 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.14757)
		(solder_mask_margin 0.05)
	)
	(pad "J20" smd circle
		(at 4.4 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.88361)
		(solder_mask_margin 0.05)
	)
	(pad "J21" smd circle
		(at 5.2 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.45449)
		(solder_mask_margin 0.05)
	)
	(pad "J22" smd circle
		(at 6 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "J23" smd circle
		(at 6.8 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.34572)
		(solder_mask_margin 0.05)
	)
	(pad "J24" smd circle
		(at 7.6 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.34103)
		(solder_mask_margin 0.05)
	)
	(pad "J25" smd circle
		(at 8.4 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "J26" smd circle
		(at 9.2 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "J27" smd circle
		(at 10 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.02342)
		(solder_mask_margin 0.05)
	)
	(pad "J28" smd circle
		(at 10.8 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.01483)
		(solder_mask_margin 0.05)
	)
	(pad "K1" smd circle
		(at -10.8 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.2431)
		(solder_mask_margin 0.05)
	)
	(pad "K2" smd circle
		(at -10 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.2513)
		(solder_mask_margin 0.05)
	)
	(pad "K3" smd circle
		(at -9.2 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.39797)
		(solder_mask_margin 0.05)
	)
	(pad "K4" smd circle
		(at -8.4 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "K5" smd circle
		(at -7.6 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.26569)
		(solder_mask_margin 0.05)
	)
	(pad "K6" smd circle
		(at -6.8 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.23916)
		(solder_mask_margin 0.05)
	)
	(pad "K7" smd circle
		(at -6 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.18419)
		(solder_mask_margin 0.05)
	)
	(pad "K8" smd circle
		(at -5.2 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.87852)
		(solder_mask_margin 0.05)
	)
	(pad "K9" smd circle
		(at -4.4 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "K10" smd circle
		(at -3.6 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.37011)
		(solder_mask_margin 0.05)
	)
	(pad "K11" smd circle
		(at -2.8 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "K12" smd circle
		(at -2 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.10154)
		(solder_mask_margin 0.05)
	)
	(pad "K13" smd circle
		(at -1.2 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "K14" smd circle
		(at -0.4 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "K15" smd circle
		(at 0.4 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.16415)
		(solder_mask_margin 0.05)
	)
	(pad "K16" smd circle
		(at 1.2 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.16856)
		(solder_mask_margin 0.05)
	)
	(pad "K17" smd circle
		(at 2 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.16936)
		(solder_mask_margin 0.05)
	)
	(pad "K18" smd circle
		(at 2.8 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.33479)
		(solder_mask_margin 0.05)
	)
	(pad "K19" smd circle
		(at 3.6 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "K20" smd circle
		(at 4.4 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.91205)
		(solder_mask_margin 0.05)
	)
	(pad "K21" smd circle
		(at 5.2 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.46754)
		(solder_mask_margin 0.05)
	)
	(pad "K22" smd circle
		(at 6 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "K23" smd circle
		(at 6.8 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "K24" smd circle
		(at 7.6 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "K25" smd circle
		(at 8.4 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.43964)
		(solder_mask_margin 0.05)
	)
	(pad "K26" smd circle
		(at 9.2 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.43578)
		(solder_mask_margin 0.05)
	)
	(pad "K27" smd circle
		(at 10 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "K28" smd circle
		(at 10.8 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "L1" smd circle
		(at -10.8 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "L2" smd circle
		(at -10 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.42627)
		(solder_mask_margin 0.05)
	)
	(pad "L3" smd circle
		(at -9.2 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.84525)
		(solder_mask_margin 0.05)
	)
	(pad "L4" smd circle
		(at -8.4 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.90176)
		(solder_mask_margin 0.05)
	)
	(pad "L5" smd circle
		(at -7.6 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.84919)
		(solder_mask_margin 0.05)
	)
	(pad "L6" smd circle
		(at -6.8 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "L7" smd circle
		(at -6 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.83218)
		(solder_mask_margin 0.05)
	)
	(pad "L8" smd circle
		(at -5.2 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.84445)
		(solder_mask_margin 0.05)
	)
	(pad "L9" smd circle
		(at -4.4 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.84302)
		(solder_mask_margin 0.05)
	)
	(pad "L10" smd circle
		(at -3.6 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.86028)
		(solder_mask_margin 0.05)
	)
	(pad "L11" smd circle
		(at -2.8 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "L12" smd circle
		(at -2 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "L13" smd circle
		(at -1.2 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "L14" smd circle
		(at -0.4 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "L15" smd circle
		(at 0.4 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "L16" smd circle
		(at 1.2 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "L17" smd circle
		(at 2 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "L18" smd circle
		(at 2.8 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "L19" smd circle
		(at 3.6 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "L20" smd circle
		(at 4.4 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "L21" smd circle
		(at 5.2 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "L22" smd circle
		(at 6 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "L23" smd circle
		(at 6.8 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.19434)
		(solder_mask_margin 0.05)
	)
	(pad "L24" smd circle
		(at 7.6 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.19647)
		(solder_mask_margin 0.05)
	)
	(pad "L25" smd circle
		(at 8.4 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "L26" smd circle
		(at 9.2 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "L27" smd circle
		(at 10 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.67774)
		(solder_mask_margin 0.05)
	)
	(pad "L28" smd circle
		(at 10.8 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.66894)
		(solder_mask_margin 0.05)
	)
	(pad "M1" smd circle
		(at -10.8 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.83794)
		(solder_mask_margin 0.05)
	)
	(pad "M2" smd circle
		(at -10 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.16083)
		(solder_mask_margin 0.05)
	)
	(pad "M3" smd circle
		(at -9.2 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "M4" smd circle
		(at -8.4 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.53995)
		(solder_mask_margin 0.05)
	)
	(pad "M5" smd circle
		(at -7.6 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.79354)
		(solder_mask_margin 0.05)
	)
	(pad "M6" smd circle
		(at -6.8 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.8449)
		(solder_mask_margin 0.05)
	)
	(pad "M7" smd circle
		(at -6 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.92022)
		(solder_mask_margin 0.05)
	)
	(pad "M8" smd circle
		(at -5.2 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "M9" smd circle
		(at -4.4 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.77489)
		(solder_mask_margin 0.05)
	)
	(pad "M10" smd circle
		(at -3.6 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.70055)
		(solder_mask_margin 0.05)
	)
	(pad "M11" smd circle
		(at -2.8 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.84496)
		(solder_mask_margin 0.05)
	)
	(pad "M12" smd circle
		(at -2 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "M13" smd circle
		(at -1.2 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "M14" smd circle
		(at -0.4 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "M15" smd circle
		(at 0.4 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "M16" smd circle
		(at 1.2 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "M17" smd circle
		(at 2 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "M18" smd circle
		(at 2.8 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "M19" smd circle
		(at 3.6 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "M20" smd circle
		(at 4.4 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "M21" smd circle
		(at 5.2 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "M22" smd circle
		(at 6 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "M23" smd circle
		(at 6.8 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "M24" smd circle
		(at 7.6 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "M25" smd circle
		(at 8.4 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.60007)
		(solder_mask_margin 0.05)
	)
	(pad "M26" smd circle
		(at 9.2 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.5971)
		(solder_mask_margin 0.05)
	)
	(pad "M27" smd circle
		(at 10 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "M28" smd circle
		(at 10.8 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "N1" smd circle
		(at -10.8 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.89663)
		(solder_mask_margin 0.05)
	)
	(pad "N2" smd circle
		(at -10 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.98313)
		(solder_mask_margin 0.05)
	)
	(pad "N3" smd circle
		(at -9.2 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.74162)
		(solder_mask_margin 0.05)
	)
	(pad "N4" smd circle
		(at -8.4 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.66187)
		(solder_mask_margin 0.05)
	)
	(pad "N5" smd circle
		(at -7.6 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "N6" smd circle
		(at -6.8 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.70865)
		(solder_mask_margin 0.05)
	)
	(pad "N7" smd circle
		(at -6 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.62836)
		(solder_mask_margin 0.05)
	)
	(pad "N8" smd circle
		(at -5.2 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.67834)
		(solder_mask_margin 0.05)
	)
	(pad "N9" smd circle
		(at -4.4 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.88741)
		(solder_mask_margin 0.05)
	)
	(pad "N10" smd circle
		(at -3.6 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "N11" smd circle
		(at -2.8 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.79384)
		(solder_mask_margin 0.05)
	)
	(pad "N12" smd circle
		(at -2 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "N13" smd circle
		(at -1.2 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "N14" smd circle
		(at -0.4 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "N15" smd circle
		(at 0.4 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "N16" smd circle
		(at 1.2 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "N17" smd circle
		(at 2 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "N18" smd circle
		(at 2.8 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "N19" smd circle
		(at 3.6 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "N20" smd circle
		(at 4.4 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "N21" smd circle
		(at 5.2 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "N22" smd circle
		(at 6 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "N23" smd circle
		(at 6.8 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.39885)
		(solder_mask_margin 0.05)
	)
	(pad "N24" smd circle
		(at 7.6 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.40218)
		(solder_mask_margin 0.05)
	)
	(pad "N25" smd circle
		(at 8.4 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "N26" smd circle
		(at 9.2 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "N27" smd circle
		(at 10 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.69827)
		(solder_mask_margin 0.05)
	)
	(pad "N28" smd circle
		(at 10.8 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.69767)
		(solder_mask_margin 0.05)
	)
	(pad "P1" smd circle
		(at -10.8 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.26097)
		(solder_mask_margin 0.05)
	)
	(pad "P2" smd circle
		(at -10 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "P3" smd circle
		(at -9.2 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.45085)
		(solder_mask_margin 0.05)
	)
	(pad "P4" smd circle
		(at -8.4 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.67438)
		(solder_mask_margin 0.05)
	)
	(pad "P5" smd circle
		(at -7.6 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.7374)
		(solder_mask_margin 0.05)
	)
	(pad "P6" smd circle
		(at -6.8 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.51626)
		(solder_mask_margin 0.05)
	)
	(pad "P7" smd circle
		(at -6 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "P8" smd circle
		(at -5.2 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.45301)
		(solder_mask_margin 0.05)
	)
	(pad "P9" smd circle
		(at -4.4 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.46095)
		(solder_mask_margin 0.05)
	)
	(pad "P10" smd circle
		(at -3.6 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.53506)
		(solder_mask_margin 0.05)
	)
	(pad "P11" smd circle
		(at -2.8 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.88156)
		(solder_mask_margin 0.05)
	)
	(pad "P12" smd circle
		(at -2 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "P13" smd circle
		(at -1.2 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "P14" smd circle
		(at -0.4 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "P15" smd circle
		(at 0.4 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "P16" smd circle
		(at 1.2 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "P17" smd circle
		(at 2 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "P18" smd circle
		(at 2.8 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "P19" smd circle
		(at 3.6 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "P20" smd circle
		(at 4.4 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "P21" smd circle
		(at 5.2 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "P22" smd circle
		(at 6 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "P23" smd circle
		(at 6.8 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "P24" smd circle
		(at 7.6 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "P25" smd circle
		(at 8.4 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.55477)
		(solder_mask_margin 0.05)
	)
	(pad "P26" smd circle
		(at 9.2 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.54603)
		(solder_mask_margin 0.05)
	)
	(pad "P27" smd circle
		(at 10 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "P28" smd circle
		(at 10.8 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "R1" smd circle
		(at -10.8 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.90753)
		(solder_mask_margin 0.05)
	)
	(pad "R2" smd circle
		(at -10 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.20665)
		(solder_mask_margin 0.05)
	)
	(pad "R3" smd circle
		(at -9.2 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.67014)
		(solder_mask_margin 0.05)
	)
	(pad "R4" smd circle
		(at -8.4 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "R5" smd circle
		(at -7.6 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.62414)
		(solder_mask_margin 0.05)
	)
	(pad "R6" smd circle
		(at -6.8 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.56067)
		(solder_mask_margin 0.05)
	)
	(pad "R7" smd circle
		(at -6 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.6151)
		(solder_mask_margin 0.05)
	)
	(pad "R8" smd circle
		(at -5.2 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.08189)
		(solder_mask_margin 0.05)
	)
	(pad "R9" smd circle
		(at -4.4 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "R10" smd circle
		(at -3.6 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.56449)
		(solder_mask_margin 0.05)
	)
	(pad "R11" smd circle
		(at -2.8 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.8769)
		(solder_mask_margin 0.05)
	)
	(pad "R12" smd circle
		(at -2 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "R13" smd circle
		(at -1.2 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "R14" smd circle
		(at -0.4 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "R15" smd circle
		(at 0.4 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "R16" smd circle
		(at 1.2 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "R17" smd circle
		(at 2 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "R18" smd circle
		(at 2.8 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "R19" smd circle
		(at 3.6 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "R20" smd circle
		(at 4.4 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "R21" smd circle
		(at 5.2 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "R22" smd circle
		(at 6 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "R23" smd circle
		(at 6.8 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.13771)
		(solder_mask_margin 0.05)
	)
	(pad "R24" smd circle
		(at 7.6 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.15222)
		(solder_mask_margin 0.05)
	)
	(pad "R25" smd circle
		(at 8.4 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "R26" smd circle
		(at 9.2 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "R27" smd circle
		(at 10 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.88331)
		(solder_mask_margin 0.05)
	)
	(pad "R28" smd circle
		(at 10.8 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.8731)
		(solder_mask_margin 0.05)
	)
	(pad "T1" smd circle
		(at -10.8 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "T2" smd circle
		(at -10 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.80193)
		(solder_mask_margin 0.05)
	)
	(pad "T3" smd circle
		(at -9.2 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.65928)
		(solder_mask_margin 0.05)
	)
	(pad "T4" smd circle
		(at -8.4 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.46892)
		(solder_mask_margin 0.05)
	)
	(pad "T5" smd circle
		(at -7.6 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.82595)
		(solder_mask_margin 0.05)
	)
	(pad "T6" smd circle
		(at -6.8 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "T7" smd circle
		(at -6 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.83046)
		(solder_mask_margin 0.05)
	)
	(pad "T8" smd circle
		(at -5.2 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.06348)
		(solder_mask_margin 0.05)
	)
	(pad "T9" smd circle
		(at -4.4 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.96368)
		(solder_mask_margin 0.05)
	)
	(pad "T10" smd circle
		(at -3.6 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.98927)
		(solder_mask_margin 0.05)
	)
	(pad "T11" smd circle
		(at -2.8 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "T12" smd circle
		(at -2 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "T13" smd circle
		(at -1.2 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "T14" smd circle
		(at -0.4 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "T15" smd circle
		(at 0.4 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "T16" smd circle
		(at 1.2 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "T17" smd circle
		(at 2 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "T18" smd circle
		(at 2.8 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "T19" smd circle
		(at 3.6 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "T20" smd circle
		(at 4.4 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "T21" smd circle
		(at 5.2 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "T22" smd circle
		(at 6 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "T23" smd circle
		(at 6.8 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "T24" smd circle
		(at 7.6 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "T25" smd circle
		(at 8.4 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.57005)
		(solder_mask_margin 0.05)
	)
	(pad "T26" smd circle
		(at 9.2 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.56891)
		(solder_mask_margin 0.05)
	)
	(pad "T27" smd circle
		(at 10 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "T28" smd circle
		(at 10.8 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "U1" smd circle
		(at -10.8 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.3121)
		(solder_mask_margin 0.05)
	)
	(pad "U2" smd circle
		(at -10 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.63458)
		(solder_mask_margin 0.05)
	)
	(pad "U3" smd circle
		(at -9.2 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "U4" smd circle
		(at -8.4 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.56912)
		(solder_mask_margin 0.05)
	)
	(pad "U5" smd circle
		(at -7.6 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.50044)
		(solder_mask_margin 0.05)
	)
	(pad "U6" smd circle
		(at -6.8 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.52728)
		(solder_mask_margin 0.05)
	)
	(pad "U7" smd circle
		(at -6 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.68909)
		(solder_mask_margin 0.05)
	)
	(pad "U8" smd circle
		(at -5.2 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "U9" smd circle
		(at -4.4 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.38641)
		(solder_mask_margin 0.05)
	)
	(pad "U10" smd circle
		(at -3.6 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.4897)
		(solder_mask_margin 0.05)
	)
	(pad "U11" smd circle
		(at -2.8 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.49055)
		(solder_mask_margin 0.05)
	)
	(pad "U12" smd circle
		(at -2 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "U13" smd circle
		(at -1.2 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "U14" smd circle
		(at -0.4 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "U15" smd circle
		(at 0.4 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "U16" smd circle
		(at 1.2 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "U17" smd circle
		(at 2 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "U18" smd circle
		(at 2.8 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "U19" smd circle
		(at 3.6 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "U20" smd circle
		(at 4.4 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "U21" smd circle
		(at 5.2 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "U22" smd circle
		(at 6 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "U23" smd circle
		(at 6.8 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.20018)
		(solder_mask_margin 0.05)
	)
	(pad "U24" smd circle
		(at 7.6 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 5.18934)
		(solder_mask_margin 0.05)
	)
	(pad "U25" smd circle
		(at 8.4 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "U26" smd circle
		(at 9.2 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "U27" smd circle
		(at 10 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.21809)
		(solder_mask_margin 0.05)
	)
	(pad "U28" smd circle
		(at 10.8 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.20895)
		(solder_mask_margin 0.05)
	)
	(pad "V1" smd circle
		(at -10.8 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.69201)
		(solder_mask_margin 0.05)
	)
	(pad "V2" smd circle
		(at -10 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.17878)
		(solder_mask_margin 0.05)
	)
	(pad "V3" smd circle
		(at -9.2 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.49241)
		(solder_mask_margin 0.05)
	)
	(pad "V4" smd circle
		(at -8.4 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.75224)
		(solder_mask_margin 0.05)
	)
	(pad "V5" smd circle
		(at -7.6 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "V6" smd circle
		(at -6.8 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.64979)
		(solder_mask_margin 0.05)
	)
	(pad "V7" smd circle
		(at -6 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.45789)
		(solder_mask_margin 0.05)
	)
	(pad "V8" smd circle
		(at -5.2 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.52498)
		(solder_mask_margin 0.05)
	)
	(pad "V9" smd circle
		(at -4.4 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.42987)
		(solder_mask_margin 0.05)
	)
	(pad "V10" smd circle
		(at -3.6 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "V11" smd circle
		(at -2.8 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.44024)
		(solder_mask_margin 0.05)
	)
	(pad "V12" smd circle
		(at -2 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "V13" smd circle
		(at -1.2 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "V14" smd circle
		(at -0.4 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "V15" smd circle
		(at 0.4 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "V16" smd circle
		(at 1.2 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "V17" smd circle
		(at 2 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "V18" smd circle
		(at 2.8 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "V19" smd circle
		(at 3.6 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "V20" smd circle
		(at 4.4 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "V21" smd circle
		(at 5.2 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "V22" smd circle
		(at 6 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "V23" smd circle
		(at 6.8 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "V24" smd circle
		(at 7.6 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "V25" smd circle
		(at 8.4 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.42671)
		(solder_mask_margin 0.05)
	)
	(pad "V26" smd circle
		(at 9.2 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.41742)
		(solder_mask_margin 0.05)
	)
	(pad "V27" smd circle
		(at 10 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "V28" smd circle
		(at 10.8 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "W1" smd circle
		(at -10.8 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.36307)
		(solder_mask_margin 0.05)
	)
	(pad "W2" smd circle
		(at -10 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "W3" smd circle
		(at -9.2 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.05323)
		(solder_mask_margin 0.05)
	)
	(pad "W4" smd circle
		(at -8.4 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.45003)
		(solder_mask_margin 0.05)
	)
	(pad "W5" smd circle
		(at -7.6 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.5357)
		(solder_mask_margin 0.05)
	)
	(pad "W6" smd circle
		(at -6.8 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.4291)
		(solder_mask_margin 0.05)
	)
	(pad "W7" smd circle
		(at -6 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "W8" smd circle
		(at -5.2 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.26104)
		(solder_mask_margin 0.05)
	)
	(pad "W9" smd circle
		(at -4.4 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.25889)
		(solder_mask_margin 0.05)
	)
	(pad "W10" smd circle
		(at -3.6 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.60284)
		(solder_mask_margin 0.05)
	)
	(pad "W11" smd circle
		(at -2.8 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.46764)
		(solder_mask_margin 0.05)
	)
	(pad "W12" smd circle
		(at -2 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "W13" smd circle
		(at -1.2 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "W14" smd circle
		(at -0.4 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "W15" smd circle
		(at 0.4 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.6849)
		(solder_mask_margin 0.05)
	)
	(pad "W16" smd circle
		(at 1.2 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "W17" smd circle
		(at 2 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.08659)
		(solder_mask_margin 0.05)
	)
	(pad "W18" smd circle
		(at 2.8 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "W19" smd circle
		(at 3.6 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.07606)
		(solder_mask_margin 0.05)
	)
	(pad "W20" smd circle
		(at 4.4 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.98085)
		(solder_mask_margin 0.05)
	)
	(pad "W21" smd circle
		(at 5.2 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.3343)
		(solder_mask_margin 0.05)
	)
	(pad "W22" smd circle
		(at 6 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.0846)
		(solder_mask_margin 0.05)
	)
	(pad "W23" smd circle
		(at 6.8 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "W24" smd circle
		(at 7.6 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "W25" smd circle
		(at 8.4 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "W26" smd circle
		(at 9.2 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "W27" smd circle
		(at 10 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.41039)
		(solder_mask_margin 0.05)
	)
	(pad "W28" smd circle
		(at 10.8 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.40025)
		(solder_mask_margin 0.05)
	)
	(pad "Y1" smd circle
		(at -10.8 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 8.67413)
		(solder_mask_margin 0.05)
	)
	(pad "Y2" smd circle
		(at -10 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.42614)
		(solder_mask_margin 0.05)
	)
	(pad "Y3" smd circle
		(at -9.2 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 9.41682)
		(solder_mask_margin 0.05)
	)
	(pad "Y4" smd circle
		(at -8.4 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "Y5" smd circle
		(at -7.6 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.46441)
		(solder_mask_margin 0.05)
	)
	(pad "Y6" smd circle
		(at -6.8 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.74941)
		(solder_mask_margin 0.05)
	)
	(pad "Y7" smd circle
		(at -6 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.54565)
		(solder_mask_margin 0.05)
	)
	(pad "Y8" smd circle
		(at -5.2 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.55095)
		(solder_mask_margin 0.05)
	)
	(pad "Y9" smd circle
		(at -4.4 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "Y10" smd circle
		(at -3.6 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 2.87754)
		(solder_mask_margin 0.05)
	)
	(pad "Y11" smd circle
		(at -2.8 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.55215)
		(solder_mask_margin 0.05)
	)
	(pad "Y12" smd circle
		(at -2 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.77764)
		(solder_mask_margin 0.05)
	)
	(pad "Y13" smd circle
		(at -1.2 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.20638)
		(solder_mask_margin 0.05)
	)
	(pad "Y14" smd circle
		(at -0.4 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.24207)
		(solder_mask_margin 0.05)
	)
	(pad "Y15" smd circle
		(at 0.4 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.02499)
		(solder_mask_margin 0.05)
	)
	(pad "Y16" smd circle
		(at 1.2 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.67915)
		(solder_mask_margin 0.05)
	)
	(pad "Y17" smd circle
		(at 2 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.05752)
		(solder_mask_margin 0.05)
	)
	(pad "Y18" smd circle
		(at 2.8 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.71985)
		(solder_mask_margin 0.05)
	)
	(pad "Y19" smd circle
		(at 3.6 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.11217)
		(solder_mask_margin 0.05)
	)
	(pad "Y20" smd circle
		(at 4.4 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 6.95959)
		(solder_mask_margin 0.05)
	)
	(pad "Y21" smd circle
		(at 5.2 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.3503)
		(solder_mask_margin 0.05)
	)
	(pad "Y22" smd circle
		(at 6 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.1091)
		(solder_mask_margin 0.05)
	)
	(pad "Y23" smd circle
		(at 6.8 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 10.1736)
		(solder_mask_margin 0.05)
	)
	(pad "Y24" smd circle
		(at 7.6 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "Y25" smd circle
		(at 8.4 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.2898)
		(solder_mask_margin 0.05)
	)
	(pad "Y26" smd circle
		(at 9.2 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(die_length 7.28573)
		(solder_mask_margin 0.05)
	)
	(pad "Y27" smd circle
		(at 10 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "Y28" smd circle
		(at 10.8 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(embedded_fonts no)
	(model "antmicro_rtpfs160zt_fcvg784.glb"
		(offset
			(xyz -11.5 11.5 0.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
