(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "RTPFS160ZT-FCVG784"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 129.54 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "RTPFS160ZT-FCVG784"
				(at 129.54 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "RTPFS160ZT-FCVG784"
				(at 129.54 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/FPGA/ProductDocuments/DataSheets/PolarFire-SoC-Datasheet-DS00004248.pdf"
				(at 129.54 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RISC-V System On Chip (SOC) IC PolarFire® FPGA - Radiation Tolerant - 161K Logic Modules 784-FCBGA (23x23)"
				(at 129.54 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "RTPFS160ZT-FCVG784"
				(at 129.54 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 129.54 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 129.54 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 129.54 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "IC, FPGA, SOC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "RTPFS160ZT-FCVG784_1_1"
				(text "BANK 0"
					(at 52.832 1.778 0)
				)
				(pin bidirectional line
					(at 106.68 -73.66 180)
					(length 5.08)
					(name "HSIO89NB0")
					(number "AA18")
				)
				(pin bidirectional line
					(at 106.68 -68.58 180)
					(length 5.08)
					(name "HSIO88NB0")
					(number "AA19")
				)
				(pin bidirectional line
					(at 106.68 -63.5 180)
					(length 5.08)
					(name "HSIO87NB0/DQS")
					(number "AA20")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "HSIO64PB0")
					(number "AA22")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "HSIO60PB0/CLKIN_N_9/CCC_NE_CLKIN_N_9")
					(number "AA23")
				)
				(pin bidirectional line
					(at 106.68 -66.04 180)
					(length 5.08)
					(name "HSIO88PB0")
					(number "AB19")
				)
				(pin bidirectional line
					(at 106.68 -60.96 180)
					(length 5.08)
					(name "HSIO87PB0/DQS")
					(number "AB20")
				)
				(pin bidirectional line
					(at 106.68 -45.72 180)
					(length 5.08)
					(name "HSIO84PB0")
					(number "AB21")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "HSIO64NB0")
					(number "AB22")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "HSIO56NB0")
					(number "AB24")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "HSIO56PB0/CCC_NE_CLKIN_N_10/CCC_NE_PLL0_OUT0")
					(number "AB25")
				)
				(pin bidirectional line
					(at 106.68 -101.6 180)
					(length 5.08)
					(name "HSIO95PB0")
					(number "AC16")
				)
				(pin bidirectional line
					(at 106.68 -104.14 180)
					(length 5.08)
					(name "HSIO95NB0")
					(number "AC17")
				)
				(pin bidirectional line
					(at 106.68 -83.82 180)
					(length 5.08)
					(name "HSIO91NB0")
					(number "AC18")
				)
				(pin bidirectional line
					(at 106.68 -20.32 180)
					(length 5.08)
					(name "HSIO79PB0")
					(number "AC19")
				)
				(pin bidirectional line
					(at 106.68 -48.26 180)
					(length 5.08)
					(name "HSIO84NB0")
					(number "AC21")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "HSIO63NB0/DQS")
					(number "AC22")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "HSIO62NB0")
					(number "AC23")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "HSIO59NB0")
					(number "AC24")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "HSIO54NB0")
					(number "AC26")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "HSIO54PB0/CCC_NE_CLKIN_N_11")
					(number "AC27")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "HSIO55NB0")
					(number "AC28")
				)
				(pin bidirectional line
					(at 106.68 -76.2 180)
					(length 5.08)
					(name "HSIO90PB0")
					(number "AD16")
				)
				(pin bidirectional line
					(at 106.68 -81.28 180)
					(length 5.08)
					(name "HSIO91PB0")
					(number "AD18")
				)
				(pin bidirectional line
					(at 106.68 -22.86 180)
					(length 5.08)
					(name "HSIO79NB0")
					(number "AD19")
				)
				(pin bidirectional line
					(at 106.68 -33.02 180)
					(length 5.08)
					(name "HSIO81NB0/DQS")
					(number "AD20")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "HSIO63PB0/DQS/CCC_NE_PLL1_OUT0")
					(number "AD21")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "HSIO62PB0/CLKIN_N_8/CCC_NE_CLKIN_N_8/CCC_NE_PLL1_OUT0")
					(number "AD23")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "HSIO59PB0")
					(number "AD24")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "HSIO58NB0")
					(number "AD25")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "HSIO58PB0")
					(number "AD26")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "HSIO55PB0/CCC_NE_PLL0_OUT1")
					(number "AD28")
				)
				(pin bidirectional line
					(at 106.68 -78.74 180)
					(length 5.08)
					(name "HSIO90NB0")
					(number "AE16")
				)
				(pin bidirectional line
					(at 106.68 -91.44 180)
					(length 5.08)
					(name "HSIO93PB0/DQS")
					(number "AE17")
				)
				(pin bidirectional line
					(at 106.68 -40.64 180)
					(length 5.08)
					(name "HSIO83PB0/CCC_NW_CLKIN_N_0")
					(number "AE18")
				)
				(pin bidirectional line
					(at 106.68 -30.48 180)
					(length 5.08)
					(name "HSIO81PB0/DQS")
					(number "AE20")
				)
				(pin bidirectional line
					(at 106.68 0 180)
					(length 5.08)
					(name "HSIO75PB0/DQS")
					(number "AE21")
				)
				(pin bidirectional line
					(at 106.68 -2.54 180)
					(length 5.08)
					(name "HSIO75NB0/DQS")
					(number "AE22")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "HSIO73NB0")
					(number "AE23")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "HSIO66NB0")
					(number "AE25")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "HSIO66PB0/CLKIN_N_7")
					(number "AE26")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "HSIO57PB0/DQS/CCC_NE_PLL0_OUT0")
					(number "AE27")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "HSIO57NB0/DQS")
					(number "AE28")
				)
				(pin bidirectional line
					(at 106.68 -93.98 180)
					(length 5.08)
					(name "HSIO93NB0/DQS")
					(number "AF17")
				)
				(pin bidirectional line
					(at 106.68 -43.18 180)
					(length 5.08)
					(name "HSIO83NB0")
					(number "AF18")
				)
				(pin bidirectional line
					(at 106.68 -25.4 180)
					(length 5.08)
					(name "HSIO80PB0/CLKIN_N_2/CCC_NW_CLKIN_N_2")
					(number "AF19")
				)
				(pin bidirectional line
					(at 106.68 -15.24 180)
					(length 5.08)
					(name "HSIO78PB0/CLKIN_N_3/CCC_NW_CLKIN_N_3")
					(number "AF20")
				)
				(pin bidirectional line
					(at 106.68 -12.7 180)
					(length 5.08)
					(name "HSIO77NB0")
					(number "AF22")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "HSIO73PB0")
					(number "AF23")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "HSIO68PB0/CLKIN_N_6")
					(number "AF24")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "HSIO68NB0")
					(number "AF25")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "HSIO67PB0")
					(number "AF27")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "HSIO67NB0")
					(number "AF28")
				)
				(pin bidirectional line
					(at 106.68 -96.52 180)
					(length 5.08)
					(name "HSIO94PB0")
					(number "AG16")
				)
				(pin bidirectional line
					(at 106.68 -86.36 180)
					(length 5.08)
					(name "HSIO92PB0")
					(number "AG17")
				)
				(pin bidirectional line
					(at 106.68 -27.94 180)
					(length 5.08)
					(name "HSIO80NB0")
					(number "AG19")
				)
				(pin bidirectional line
					(at 106.68 -17.78 180)
					(length 5.08)
					(name "HSIO78NB0")
					(number "AG20")
				)
				(pin bidirectional line
					(at 106.68 -7.62 180)
					(length 5.08)
					(name "HSIO76NB0")
					(number "AG21")
				)
				(pin bidirectional line
					(at 106.68 -10.16 180)
					(length 5.08)
					(name "HSIO77PB0")
					(number "AG22")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "HSIO72NB0")
					(number "AG24")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "HSIO71PB0")
					(number "AG25")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "HSIO71NB0")
					(number "AG26")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "HSIO69PB0/DQS")
					(number "AG27")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "HSIO69NB0/DQS")
					(number "AG28")
				)
				(pin bidirectional line
					(at 106.68 -99.06 180)
					(length 5.08)
					(name "HSIO94NB0")
					(number "AH16")
				)
				(pin bidirectional line
					(at 106.68 -88.9 180)
					(length 5.08)
					(name "HSIO92NB0")
					(number "AH17")
				)
				(pin bidirectional line
					(at 106.68 -35.56 180)
					(length 5.08)
					(name "HSIO82PB0/CCC_NW_CLKIN_N_1")
					(number "AH18")
				)
				(pin bidirectional line
					(at 106.68 -38.1 180)
					(length 5.08)
					(name "HSIO82NB0")
					(number "AH19")
				)
				(pin bidirectional line
					(at 106.68 -5.08 180)
					(length 5.08)
					(name "HSIO76PB0")
					(number "AH21")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "HSIO74PB0/CLKIN_N_4")
					(number "AH22")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "HSIO74NB0")
					(number "AH23")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "HSIO72PB0/CLKIN_N_5")
					(number "AH24")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "HSIO70PB0")
					(number "AH26")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "HSIO70NB0")
					(number "AH27")
				)
				(pin bidirectional line
					(at 106.68 -55.88 180)
					(length 5.08)
					(name "HSIO86PB0")
					(number "W19")
				)
				(pin bidirectional line
					(at 106.68 -50.8 180)
					(length 5.08)
					(name "HSIO85PB0")
					(number "W20")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "HSIO65NB0")
					(number "W21")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "HSIO61PB0/CCC_NE_PLL1_OUT1")
					(number "W22")
				)
				(pin bidirectional line
					(at 106.68 -71.12 180)
					(length 5.08)
					(name "HSIO89PB0")
					(number "Y18")
				)
				(pin bidirectional line
					(at 106.68 -58.42 180)
					(length 5.08)
					(name "HSIO86NB0")
					(number "Y19")
				)
				(pin bidirectional line
					(at 106.68 -53.34 180)
					(length 5.08)
					(name "HSIO85NB0")
					(number "Y20")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "HSIO65PB0")
					(number "Y21")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "HSIO61NB0")
					(number "Y22")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "HSIO60NB0")
					(number "Y23")
				)
			)
			(symbol "RTPFS160ZT-FCVG784_2_1"
				(text "BANK 1"
					(at 46.99 1.524 0)
				)
				(pin bidirectional line
					(at 97.79 -25.4 180)
					(length 5.08)
					(name "GPIO149PB1/CLKIN_S_3/CCC_SW_CLKIN_S_3")
					(number "A2")
				)
				(pin bidirectional line
					(at 97.79 -27.94 180)
					(length 5.08)
					(name "GPIO149NB1")
					(number "A3")
				)
				(pin bidirectional line
					(at 97.79 -48.26 180)
					(length 5.08)
					(name "GPIO153NB1")
					(number "A4")
				)
				(pin bidirectional line
					(at 97.79 -58.42 180)
					(length 5.08)
					(name "GPIO155NB1")
					(number "A5")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GPIO1NB1")
					(number "A7")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GPIO3PB1/CLKIN_S_6")
					(number "A8")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GPIO3NB1")
					(number "A9")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GPIO5NB1")
					(number "A10")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "GPIO17PB1/CCC_SE_CLKIN_S_11")
					(number "A12")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "GPIO17NB1")
					(number "A13")
				)
				(pin bidirectional line
					(at 97.79 -22.86 180)
					(length 5.08)
					(name "GPIO148NB1")
					(number "B1")
				)
				(pin bidirectional line
					(at 97.79 -2.54 180)
					(length 5.08)
					(name "GPIO144NB1")
					(number "B2")
				)
				(pin bidirectional line
					(at 97.79 -45.72 180)
					(length 5.08)
					(name "GPIO153PB1/CCC_SW_PLL0_OUT0")
					(number "B4")
				)
				(pin bidirectional line
					(at 97.79 -55.88 180)
					(length 5.08)
					(name "GPIO155PB1")
					(number "B5")
				)
				(pin bidirectional line
					(at 97.79 -38.1 180)
					(length 5.08)
					(name "GPIO151NB1")
					(number "B6")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GPIO1PB1/CLKIN_S_5")
					(number "B7")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GPIO4NB1/LPRB_B")
					(number "B9")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GPIO5PB1/CLKIN_S_7")
					(number "B10")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "GPIO13NB1")
					(number "B11")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "GPIO13PB1")
					(number "B12")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "GPIO15NB1")
					(number "B14")
				)
				(pin bidirectional line
					(at 97.79 -20.32 180)
					(length 5.08)
					(name "GPIO148PB1/CCC_SW_PLL1_OUT1")
					(number "C1")
				)
				(pin bidirectional line
					(at 97.79 0 180)
					(length 5.08)
					(name "GPIO144PB1/CCC_SW_CLKIN_S_0")
					(number "C2")
				)
				(pin bidirectional line
					(at 97.79 -17.78 180)
					(length 5.08)
					(name "GPIO147NB1")
					(number "C3")
				)
				(pin bidirectional line
					(at 97.79 -43.18 180)
					(length 5.08)
					(name "GPIO152NB1/DQS")
					(number "C4")
				)
				(pin bidirectional line
					(at 97.79 -35.56 180)
					(length 5.08)
					(name "GPIO151PB1")
					(number "C6")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GPIO2NB1/DQS")
					(number "C7")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GPIO2PB1/DQS")
					(number "C8")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GPIO4PB1/LPRB_A")
					(number "C9")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "GPIO16NB1")
					(number "C11")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "GPIO14NB1/DQS")
					(number "C12")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "GPIO14PB1/DQS")
					(number "C13")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "GPIO15PB1/CCC_SE_CLKIN_S_10")
					(number "C14")
				)
				(pin bidirectional line
					(at 97.79 -12.7 180)
					(length 5.08)
					(name "GPIO146NB1/DQS")
					(number "D1")
				)
				(pin bidirectional line
					(at 97.79 -15.24 180)
					(length 5.08)
					(name "GPIO147PB1/CLKIN_S_2/CCC_SW_CLKIN_S_2/CCC_SW_PLL1_OUT0")
					(number "D3")
				)
				(pin bidirectional line
					(at 97.79 -40.64 180)
					(length 5.08)
					(name "GPIO152PB1/DQS/CCC_SW_PLL0_OUT0")
					(number "D4")
				)
				(pin bidirectional line
					(at 97.79 -53.34 180)
					(length 5.08)
					(name "GPIO154NB1")
					(number "D5")
				)
				(pin bidirectional line
					(at 97.79 -50.8 180)
					(length 5.08)
					(name "GPIO154PB1/CCC_SW_PLL0_OUT1")
					(number "D6")
				)
				(pin bidirectional line
					(at 97.79 -88.9 180)
					(length 5.08)
					(name "GPIO161NB1")
					(number "D8")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GPIO0PB1/CLKIN_S_4")
					(number "D9")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GPIO0NB1")
					(number "D10")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "GPIO16PB1")
					(number "D11")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GPIO8NB1/DQS")
					(number "D13")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GPIO8PB1/DQS")
					(number "D14")
				)
				(pin bidirectional line
					(at 97.79 -10.16 180)
					(length 5.08)
					(name "GPIO146PB1/DQS/CCC_SW_PLL1_OUT0")
					(number "E1")
				)
				(pin bidirectional line
					(at 97.79 -7.62 180)
					(length 5.08)
					(name "GPIO145NB1")
					(number "E2")
				)
				(pin bidirectional line
					(at 97.79 -5.08 180)
					(length 5.08)
					(name "GPIO145PB1/CCC_SW_CLKIN_S_1")
					(number "E3")
				)
				(pin bidirectional line
					(at 97.79 -30.48 180)
					(length 5.08)
					(name "GPIO150PB1")
					(number "E5")
				)
				(pin bidirectional line
					(at 97.79 -73.66 180)
					(length 5.08)
					(name "GPIO158NB1/DQS")
					(number "E6")
				)
				(pin bidirectional line
					(at 97.79 -71.12 180)
					(length 5.08)
					(name "GPIO158PB1/DQS")
					(number "E7")
				)
				(pin bidirectional line
					(at 97.79 -86.36 180)
					(length 5.08)
					(name "GPIO161PB1")
					(number "E8")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "GPIO12NB1")
					(number "E10")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "GPIO12PB1")
					(number "E11")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GPIO6NB1")
					(number "E12")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GPIO7NB1")
					(number "E13")
				)
				(pin bidirectional line
					(at 97.79 -33.02 180)
					(length 5.08)
					(name "GPIO150NB1")
					(number "F5")
				)
				(pin bidirectional line
					(at 97.79 -83.82 180)
					(length 5.08)
					(name "GPIO160NB1")
					(number "F7")
				)
				(pin bidirectional line
					(at 97.79 -81.28 180)
					(length 5.08)
					(name "GPIO160PB1")
					(number "F8")
				)
				(pin bidirectional line
					(at 97.79 -63.5 180)
					(length 5.08)
					(name "GPIO156NB1")
					(number "F9")
				)
				(pin bidirectional line
					(at 97.79 -78.74 180)
					(length 5.08)
					(name "GPIO159NB1")
					(number "F10")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GPIO6PB1")
					(number "F12")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GPIO7PB1")
					(number "F13")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "GPIO10PB1")
					(number "F14")
				)
				(pin bidirectional line
					(at 97.79 -68.58 180)
					(length 5.08)
					(name "GPIO157NB1")
					(number "G6")
				)
				(pin bidirectional line
					(at 97.79 -66.04 180)
					(length 5.08)
					(name "GPIO157PB1")
					(number "G7")
				)
				(pin bidirectional line
					(at 97.79 -60.96 180)
					(length 5.08)
					(name "GPIO156PB1")
					(number "G9")
				)
				(pin bidirectional line
					(at 97.79 -76.2 180)
					(length 5.08)
					(name "GPIO159PB1")
					(number "G10")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GPIO9NB1")
					(number "G11")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GPIO9PB1/CLKIN_S_8/CCC_SE_CLKIN_S_8")
					(number "G12")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "GPIO10NB1")
					(number "G14")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "GPIO11NB1")
					(number "H14")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "GPIO11PB1/CLKIN_S_9/CCC_SE_CLKIN_S_9")
					(number "J14")
				)
			)
			(symbol "RTPFS160ZT-FCVG784_3_1"
				(text "BANK 2"
					(at 13.97 2.54 0)
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "MSSIO29B2")
					(number "K8")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "MSSIO23B2")
					(number "L2")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MSSIO20B2")
					(number "L3")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MSSIO21B2")
					(number "L4")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "MSSIO24B2")
					(number "L5")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "MSSIO28B2")
					(number "L7")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "MSSIO36B2")
					(number "L8")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "MSSIO37B2")
					(number "L9")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "MSSIO32B2")
					(number "L10")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MSSIO19B2")
					(number "M1")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "MSSIO22B2")
					(number "M2")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MSSIO16B2")
					(number "M4")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MSSIO17B2")
					(number "M5")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "MSSIO25B2")
					(number "M6")
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "MSSIO27B2")
					(number "M7")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "MSSIO33B2")
					(number "M9")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "MSSIO30B2")
					(number "M10")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "MSSIO34B2")
					(number "M11")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MSSIO18B2")
					(number "N1")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "MSSIO14B2")
					(number "N2")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MSSIO15B2")
					(number "N3")
				)
				(pin bidirectional line
					(at 35.56 0 180)
					(length 5.08)
					(name "MSSIO26B2")
					(number "N8")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "MSSIO31B2")
					(number "N9")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "MSSIO35B2")
					(number "N11")
				)
			)
			(symbol "RTPFS160ZT-FCVG784_4_1"
				(text "BANK 3"
					(at 13.97 2.54 0)
				)
				(pin output line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "SDO")
					(number "H8")
				)
				(pin input line
					(at 35.56 0 180)
					(length 5.08)
					(name "DEVRST_N")
					(number "H9")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "TDI")
					(number "H11")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "TCK")
					(number "H12")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "IO_CFG_INTF")
					(number "H13")
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "SCK")
					(number "J8")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "SS")
					(number "J9")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "TRSTB")
					(number "J10")
				)
				(pin output line
					(at 0 -5.08 0)
					(length 5.08)
					(name "TDO")
					(number "J11")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "TMS")
					(number "J12")
				)
				(pin input line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "SC_EXIT_FLASH_FREEZE_B")
					(number "J13")
				)
				(pin input line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "SDI")
					(number "K10")
				)
				(pin input line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "SPI_EN")
					(number "K12")
				)
			)
			(symbol "RTPFS160ZT-FCVG784_5_1"
				(text "BANK 4"
					(at 13.97 2.54 0)
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MSSIO5B4")
					(number "N4")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "MSSIO10B4")
					(number "N6")
				)
				(pin bidirectional line
					(at 35.56 0 180)
					(length 5.08)
					(name "MSSIO7B4")
					(number "N7")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MSSIO6B4")
					(number "P1")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "MSSIO11B4")
					(number "P3")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "MSSIO13B4")
					(number "P4")
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "MSSIO8B4")
					(number "P5")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "MSSIO12B4")
					(number "P6")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MSSIO3B4")
					(number "R1")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MSSIO2B4")
					(number "R2")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "MSSIO0B4")
					(number "R3")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MSSIO4B4")
					(number "R5")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MSSIO1B4")
					(number "R6")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "MSSIO9B4")
					(number "R7")
				)
			)
			(symbol "RTPFS160ZT-FCVG784_6_1"
				(text "BANK 5"
					(at 19.05 2.54 0)
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "MSS_SGMII_RXP0")
					(number "P8")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MSS_SGMII_RXN0")
					(number "P9")
				)
				(pin bidirectional line
					(at 45.72 0 180)
					(length 5.08)
					(name "MSS_SGMII_TXP0")
					(number "P10")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MSS_REFCLK_IN_P")
					(number "P11")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MSS_SGMII_RXP1")
					(number "R8")
				)
				(pin bidirectional line
					(at 45.72 -2.54 180)
					(length 5.08)
					(name "MSS_SGMII_TXN0")
					(number "R10")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MSS_REFCLK_IN_N")
					(number "R11")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MSS_SGMII_RXN1")
					(number "T8")
				)
				(pin bidirectional line
					(at 45.72 -7.62 180)
					(length 5.08)
					(name "MSS_SGMII_TXP1")
					(number "T9")
				)
				(pin bidirectional line
					(at 45.72 -10.16 180)
					(length 5.08)
					(name "MSS_SGMII_TXN1")
					(number "T10")
				)
			)
			(symbol "RTPFS160ZT-FCVG784_7_1"
				(text "BANK 6"
					(at 27.94 2.54 0)
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MSS_DDR_DQ4")
					(number "AA2")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MSS_DDR_DQ3")
					(number "AA3")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MSS_DDR_DQ2")
					(number "AA4")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "MSS_DDR_DQ11")
					(number "AA5")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "MSS_DDR_DQS_P1")
					(number "AA7")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "MSS_DDR_DQS_N1")
					(number "AA8")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "MSS_DDR_DQ14")
					(number "AA9")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "MSS_DDR_DQ34")
					(number "AA10")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "MSS_DDR_DQS_N0")
					(number "AB1")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "MSS_DDR_DQS_P0")
					(number "AB2")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MSS_DDR_DQ1")
					(number "AB4")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "MSS_DDR_DQ0")
					(number "AB5")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "MSS_DDR_DQ12")
					(number "AB6")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "MSS_DDR_DQ8")
					(number "AB7")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "MSS_DDR_DQ15")
					(number "AB9")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "MSS_DDR_DQ32")
					(number "AB10")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "MSS_DDR_DQ33")
					(number "AB11")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MSS_DDR_DQ6")
					(number "AC1")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MSS_DDR_DQ7")
					(number "AC2")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "MSS_DDR_DM0")
					(number "AC3")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MSS_DDR_DQ5")
					(number "AC4")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "MSS_DDR_DQ9")
					(number "AC6")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "MSS_DDR_DQ10")
					(number "AC7")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "MSS_DDR_DQ13")
					(number "AC8")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "MSS_DDR_DM1")
					(number "AC9")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "MSS_DDR_DQ23")
					(number "AD1")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "MSS_DDR_DQS_P2")
					(number "AD3")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "MSS_DDR_DQ19")
					(number "AD4")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "MSS_DDR_DQ18")
					(number "AD5")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "MSS_DDR_DQ16")
					(number "AD6")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "MSS_DDR_DM2")
					(number "AE1")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "MSS_DDR_DQ22")
					(number "AE2")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "MSS_DDR_DQS_N2")
					(number "AE3")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "MSS_DDR_DQ17")
					(number "AE5")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "MSS_DDR_DQ21")
					(number "AE6")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "MSS_DDR_DQ26")
					(number "AF1")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "MSS_DDR_DQS_P3")
					(number "AF2")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "MSS_DDR_DQ25")
					(number "AF3")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "MSS_DDR_DQ24")
					(number "AF4")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "MSS_DDR_DQ20")
					(number "AF5")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "MSS_DDR_DQ27")
					(number "AG1")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "MSS_DDR_DQS_N3")
					(number "AG2")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "MSS_DDR_DQ31")
					(number "AG4")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "MSS_DDR_DQ30")
					(number "AG5")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "MSS_DDR_DQ28")
					(number "AH2")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "MSS_DDR_DQ29")
					(number "AH3")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "MSS_DDR_DM3")
					(number "AH4")
				)
				(pin bidirectional line
					(at 63.5 -68.58 180)
					(length 5.08)
					(name "MSS_DDR_CKE1")
					(number "T2")
				)
				(pin bidirectional line
					(at 63.5 -63.5 180)
					(length 5.08)
					(name "MSS_DDR_CS1")
					(number "T3")
				)
				(pin bidirectional line
					(at 63.5 -60.96 180)
					(length 5.08)
					(name "MSS_DDR_CS0")
					(number "T4")
				)
				(pin bidirectional line
					(at 63.5 -132.08 180)
					(length 5.08)
					(name "MSS_DDR_ODT1")
					(number "T5")
				)
				(pin bidirectional line
					(at 63.5 -35.56 180)
					(length 5.08)
					(name "MSS_DDR_A14")
					(number "T7")
				)
				(pin bidirectional line
					(at 63.5 -58.42 180)
					(length 5.08)
					(name "MSS_DDR_RAM_RST_N/DDR_PLL0_OUT1")
					(number "U1")
				)
				(pin bidirectional line
					(at 63.5 -73.66 180)
					(length 5.08)
					(name "MSS_DDR_BG0")
					(number "U2")
				)
				(pin bidirectional line
					(at 63.5 -76.2 180)
					(length 5.08)
					(name "MSS_DDR_BG1")
					(number "U4")
				)
				(pin bidirectional line
					(at 63.5 -71.12 180)
					(length 5.08)
					(name "MSS_DDR_ACT_N")
					(number "U5")
				)
				(pin bidirectional line
					(at 63.5 -127 180)
					(length 5.08)
					(name "MSS_DDR_PARITY")
					(number "U6")
				)
				(pin bidirectional line
					(at 63.5 -38.1 180)
					(length 5.08)
					(name "MSS_DDR_A15")
					(number "U7")
				)
				(pin bidirectional line
					(at 63.5 -27.94 180)
					(length 5.08)
					(name "MSS_DDR_A11")
					(number "U9")
				)
				(pin bidirectional line
					(at 63.5 -40.64 180)
					(length 5.08)
					(name "MSS_DDR_A16")
					(number "U10")
				)
				(pin bidirectional line
					(at 63.5 -78.74 180)
					(length 5.08)
					(name "MSS_DDR_BA0")
					(number "U11")
				)
				(pin bidirectional line
					(at 63.5 0 180)
					(length 5.08)
					(name "MSS_DDR_A0")
					(number "V1")
				)
				(pin bidirectional line
					(at 63.5 -2.54 180)
					(length 5.08)
					(name "MSS_DDR_A1")
					(number "V2")
				)
				(pin bidirectional line
					(at 63.5 -129.54 180)
					(length 5.08)
					(name "MSS_DDR_ODT0")
					(number "V3")
				)
				(pin bidirectional line
					(at 63.5 -66.04 180)
					(length 5.08)
					(name "MSS_DDR_CKE0")
					(number "V4")
				)
				(pin bidirectional line
					(at 63.5 -134.62 180)
					(length 5.08)
					(name "MSS_DDR_ALERT_N")
					(number "V6")
				)
				(pin bidirectional line
					(at 63.5 -30.48 180)
					(length 5.08)
					(name "MSS_DDR_A12")
					(number "V7")
				)
				(pin bidirectional line
					(at 63.5 -33.02 180)
					(length 5.08)
					(name "MSS_DDR_A13")
					(number "V8")
				)
				(pin bidirectional line
					(at 63.5 -25.4 180)
					(length 5.08)
					(name "MSS_DDR_A10")
					(number "V9")
				)
				(pin bidirectional line
					(at 63.5 -114.3 180)
					(length 5.08)
					(name "MSS_DDR3_WE_N")
					(number "V11")
				)
				(pin bidirectional line
					(at 63.5 -7.62 180)
					(length 5.08)
					(name "MSS_DDR_A3")
					(number "W1")
				)
				(pin bidirectional line
					(at 63.5 -10.16 180)
					(length 5.08)
					(name "MSS_DDR_A4")
					(number "W3")
				)
				(pin bidirectional line
					(at 63.5 -12.7 180)
					(length 5.08)
					(name "MSS_DDR_A5")
					(number "W4")
				)
				(pin bidirectional line
					(at 63.5 -15.24 180)
					(length 5.08)
					(name "MSS_DDR_A6")
					(number "W5")
				)
				(pin bidirectional line
					(at 63.5 -20.32 180)
					(length 5.08)
					(name "MSS_DDR_A8")
					(number "W6")
				)
				(pin bidirectional line
					(at 63.5 -121.92 180)
					(length 5.08)
					(name "MSS_DDR_CK1/DDR_PLL0_OUT0")
					(number "W8")
				)
				(pin bidirectional line
					(at 63.5 -124.46 180)
					(length 5.08)
					(name "MSS_DDR_CK_N1")
					(number "W9")
				)
				(pin bidirectional line
					(at 63.5 -81.28 180)
					(length 5.08)
					(name "MSS_DDR_BA1")
					(number "W10")
				)
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 5.08)
					(name "MSS_DDR_DM4")
					(number "W11")
				)
				(pin bidirectional line
					(at 63.5 -5.08 180)
					(length 5.08)
					(name "MSS_DDR_A2")
					(number "Y1")
				)
				(pin bidirectional line
					(at 63.5 -119.38 180)
					(length 5.08)
					(name "MSS_DDR_CK_N0")
					(number "Y2")
				)
				(pin bidirectional line
					(at 63.5 -116.84 180)
					(length 5.08)
					(name "MSS_DDR_CK0/DDR_PLL0_OUT0")
					(number "Y3")
				)
				(pin bidirectional line
					(at 63.5 -22.86 180)
					(length 5.08)
					(name "MSS_DDR_A9")
					(number "Y5")
				)
				(pin bidirectional line
					(at 63.5 -17.78 180)
					(length 5.08)
					(name "MSS_DDR_A7")
					(number "Y6")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "MSS_DDR_DQS_P4")
					(number "Y7")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "MSS_DDR_DQS_N4")
					(number "Y8")
				)
				(pin input line
					(at 63.5 -137.16 180)
					(length 5.08)
					(name "MSS_DDR_VREF_IN")
					(number "Y10")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "MSS_DDR_DQ35")
					(number "Y11")
				)
			)
			(symbol "RTPFS160ZT-FCVG784_8_1"
				(text "BANK 7"
					(at 46.99 2.286 0)
				)
				(pin bidirectional line
					(at 100.33 -20.32 180)
					(length 5.08)
					(name "GPIO142PB7")
					(number "F2")
				)
				(pin bidirectional line
					(at 100.33 -12.7 180)
					(length 5.08)
					(name "GPIO140NB7")
					(number "F3")
				)
				(pin bidirectional line
					(at 100.33 -10.16 180)
					(length 5.08)
					(name "GPIO140PB7/CLKIN_W_1/CCC_SW_CLKIN_W_1")
					(number "F4")
				)
				(pin bidirectional line
					(at 100.33 -22.86 180)
					(length 5.08)
					(name "GPIO142NB7")
					(number "G1")
				)
				(pin bidirectional line
					(at 100.33 -15.24 180)
					(length 5.08)
					(name "GPIO141PB7/DQS/CCC_SW_PLL0_OUT0")
					(number "G2")
				)
				(pin bidirectional line
					(at 100.33 -27.94 180)
					(length 5.08)
					(name "GPIO143NB7")
					(number "G4")
				)
				(pin bidirectional line
					(at 100.33 -25.4 180)
					(length 5.08)
					(name "GPIO143PB7/CLKIN_W_0/CCC_SW_CLKIN_W_0")
					(number "G5")
				)
				(pin bidirectional line
					(at 100.33 -5.08 180)
					(length 5.08)
					(name "GPIO139PB7/CLKIN_W_2/CCC_SW_CLKIN_W_2/CCC_SW_PLL0_OUT0")
					(number "H1")
				)
				(pin bidirectional line
					(at 100.33 -17.78 180)
					(length 5.08)
					(name "GPIO141NB7/DQS")
					(number "H2")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GPIO135PB7/DQS")
					(number "H3")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GPIO135NB7/DQS")
					(number "H4")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GPIO137NB7")
					(number "H6")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GPIO137PB7/CLKIN_W_4")
					(number "H7")
				)
				(pin bidirectional line
					(at 100.33 -7.62 180)
					(length 5.08)
					(name "GPIO139NB7")
					(number "J1")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GPIO133PB7/CLKIN_W_7")
					(number "J3")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GPIO134NB7")
					(number "J4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GPIO134PB7/CLKIN_W_6")
					(number "J5")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GPIO136NB7")
					(number "J6")
				)
				(pin bidirectional line
					(at 100.33 0 180)
					(length 5.08)
					(name "GPIO138PB7/CLKIN_W_3/CCC_SW_CLKIN_W_3")
					(number "K1")
				)
				(pin bidirectional line
					(at 100.33 -2.54 180)
					(length 5.08)
					(name "GPIO138NB7")
					(number "K2")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GPIO133NB7")
					(number "K3")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GPIO132NB7")
					(number "K5")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GPIO132PB7")
					(number "K6")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GPIO136PB7/CLKIN_W_5")
					(number "K7")
				)
			)
			(symbol "RTPFS160ZT-FCVG784_9_1"
				(text "BANK 8"
					(at 40.64 1.27 0)
				)
				(pin bidirectional line
					(at 91.44 -17.78 180)
					(length 5.08)
					(name "HSIO120NB8")
					(number "AA12")
				)
				(pin bidirectional line
					(at 91.44 -33.02 180)
					(length 5.08)
					(name "HSIO123NB8/DQS")
					(number "AA13")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "HSIO113NB8")
					(number "AA14")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "HSIO112NB8")
					(number "AA15")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "HSIO108PB8")
					(number "AA17")
				)
				(pin bidirectional line
					(at 91.44 -20.32 180)
					(length 5.08)
					(name "HSIO121PB8/CCC_NW_PLL0_OUT1")
					(number "AB12")
				)
				(pin bidirectional line
					(at 91.44 -25.4 180)
					(length 5.08)
					(name "HSIO122PB8/CCC_NW_PLL0_OUT0")
					(number "AB14")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "HSIO110PB8")
					(number "AB15")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "HSIO110NB8")
					(number "AB16")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "HSIO108NB8")
					(number "AB17")
				)
				(pin bidirectional line
					(at 91.44 -43.18 180)
					(length 5.08)
					(name "HSIO125NB8")
					(number "AC11")
				)
				(pin bidirectional line
					(at 91.44 -40.64 180)
					(length 5.08)
					(name "HSIO125PB8")
					(number "AC12")
				)
				(pin bidirectional line
					(at 91.44 -22.86 180)
					(length 5.08)
					(name "HSIO121NB8")
					(number "AC13")
				)
				(pin bidirectional line
					(at 91.44 -27.94 180)
					(length 5.08)
					(name "HSIO122NB8")
					(number "AC14")
				)
				(pin bidirectional line
					(at 91.44 -48.26 180)
					(length 5.08)
					(name "HSIO126NB8")
					(number "AD8")
				)
				(pin bidirectional line
					(at 91.44 -45.72 180)
					(length 5.08)
					(name "HSIO126PB8/CCC_NW_CLKIN_N_15")
					(number "AD9")
				)
				(pin bidirectional line
					(at 91.44 -35.56 180)
					(length 5.08)
					(name "HSIO124PB8")
					(number "AD10")
				)
				(pin bidirectional line
					(at 91.44 -38.1 180)
					(length 5.08)
					(name "HSIO124NB8")
					(number "AD11")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "HSIO107NB8")
					(number "AD13")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "HSIO107PB8")
					(number "AD14")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "HSIO106PB8")
					(number "AD15")
				)
				(pin bidirectional line
					(at 91.44 -73.66 180)
					(length 5.08)
					(name "HSIO131NB8")
					(number "AE7")
				)
				(pin bidirectional line
					(at 91.44 -71.12 180)
					(length 5.08)
					(name "HSIO131PB8/CLKIN_N_12/CCC_NW_CLKIN_N_12")
					(number "AE8")
				)
				(pin bidirectional line
					(at 91.44 -10.16 180)
					(length 5.08)
					(name "HSIO119PB8")
					(number "AE10")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "HSIO116PB8")
					(number "AE11")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "HSIO116NB8")
					(number "AE12")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "HSIO104PB8")
					(number "AE13")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "HSIO106NB8")
					(number "AE15")
				)
				(pin bidirectional line
					(at 91.44 -66.04 180)
					(length 5.08)
					(name "HSIO130PB8/CLKIN_N_13/CCC_NW_CLKIN_N_13")
					(number "AF7")
				)
				(pin bidirectional line
					(at 91.44 -55.88 180)
					(length 5.08)
					(name "HSIO128PB8/CCC_NW_CLKIN_N_14/CCC_NW_PLL1_OUT0")
					(number "AF8")
				)
				(pin bidirectional line
					(at 91.44 -58.42 180)
					(length 5.08)
					(name "HSIO128NB8")
					(number "AF9")
				)
				(pin bidirectional line
					(at 91.44 -12.7 180)
					(length 5.08)
					(name "HSIO119NB8")
					(number "AF10")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "HSIO115NB8")
					(number "AF12")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "HSIO104NB8")
					(number "AF13")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "HSIO105PB8/DQS")
					(number "AF14")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "HSIO102PB8")
					(number "AF15")
				)
				(pin bidirectional line
					(at 91.44 -60.96 180)
					(length 5.08)
					(name "HSIO129PB8/DQS/CCC_NW_PLL1_OUT0")
					(number "AG6")
				)
				(pin bidirectional line
					(at 91.44 -68.58 180)
					(length 5.08)
					(name "HSIO130NB8")
					(number "AG7")
				)
				(pin bidirectional line
					(at 91.44 -5.08 180)
					(length 5.08)
					(name "HSIO118PB8")
					(number "AG9")
				)
				(pin bidirectional line
					(at 91.44 0 180)
					(length 5.08)
					(name "HSIO117PB8/DQS")
					(number "AG10")
				)
				(pin bidirectional line
					(at 91.44 -2.54 180)
					(length 5.08)
					(name "HSIO117NB8/DQS")
					(number "AG11")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "HSIO115PB8")
					(number "AG12")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "HSIO105NB8/DQS")
					(number "AG14")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "HSIO102NB8")
					(number "AG15")
				)
				(pin bidirectional line
					(at 91.44 -63.5 180)
					(length 5.08)
					(name "HSIO129NB8/DQS")
					(number "AH6")
				)
				(pin bidirectional line
					(at 91.44 -50.8 180)
					(length 5.08)
					(name "HSIO127PB8/CCC_NW_PLL1_OUT1")
					(number "AH7")
				)
				(pin bidirectional line
					(at 91.44 -53.34 180)
					(length 5.08)
					(name "HSIO127NB8")
					(number "AH8")
				)
				(pin bidirectional line
					(at 91.44 -7.62 180)
					(length 5.08)
					(name "HSIO118NB8")
					(number "AH9")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "HSIO114PB8")
					(number "AH11")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "HSIO114NB8")
					(number "AH12")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "HSIO103PB8")
					(number "AH13")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "HSIO103NB8")
					(number "AH14")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "HSIO111NB8/DQS")
					(number "W15")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "HSIO109PB8")
					(number "W17")
				)
				(pin bidirectional line
					(at 91.44 -15.24 180)
					(length 5.08)
					(name "HSIO120PB8")
					(number "Y12")
				)
				(pin bidirectional line
					(at 91.44 -30.48 180)
					(length 5.08)
					(name "HSIO123PB8/DQS/CCC_NW_PLL0_OUT0")
					(number "Y13")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "HSIO113PB8")
					(number "Y14")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "HSIO112PB8")
					(number "Y15")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "HSIO111PB8/DQS")
					(number "Y16")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "HSIO109NB8")
					(number "Y17")
				)
			)
			(symbol "RTPFS160ZT-FCVG784_10_1"
				(text "BANK 9"
					(at 46.99 1.524 0)
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GPIO19PB9")
					(number "A14")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GPIO19NB9")
					(number "A15")
				)
				(pin bidirectional line
					(at 97.79 -10.16 180)
					(length 5.08)
					(name "GPIO38PB9/DQS")
					(number "A22")
				)
				(pin bidirectional line
					(at 97.79 -12.7 180)
					(length 5.08)
					(name "GPIO38NB9/DQS")
					(number "A23")
				)
				(pin bidirectional line
					(at 97.79 -25.4 180)
					(length 5.08)
					(name "GPIO41PB9")
					(number "A24")
				)
				(pin bidirectional line
					(at 97.79 -27.94 180)
					(length 5.08)
					(name "GPIO41NB9")
					(number "A25")
				)
				(pin bidirectional line
					(at 97.79 -45.72 180)
					(length 5.08)
					(name "GPIO45PB9/CLKIN_S_12/CCC_SE_CLKIN_S_12/CCC_SE_PLL0_OUT0")
					(number "A27")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GPIO20PB9/DQS")
					(number "B15")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GPIO20NB9/DQS")
					(number "B16")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GPIO23NB9")
					(number "B17")
				)
				(pin bidirectional line
					(at 97.79 -5.08 180)
					(length 5.08)
					(name "GPIO37PB9")
					(number "B21")
				)
				(pin bidirectional line
					(at 97.79 -20.32 180)
					(length 5.08)
					(name "GPIO40PB9")
					(number "B22")
				)
				(pin bidirectional line
					(at 97.79 -30.48 180)
					(length 5.08)
					(name "GPIO42PB9")
					(number "B24")
				)
				(pin bidirectional line
					(at 97.79 -35.56 180)
					(length 5.08)
					(name "GPIO43PB9")
					(number "B25")
				)
				(pin bidirectional line
					(at 97.79 -38.1 180)
					(length 5.08)
					(name "GPIO43NB9")
					(number "B26")
				)
				(pin bidirectional line
					(at 97.79 -48.26 180)
					(length 5.08)
					(name "GPIO45NB9")
					(number "B27")
				)
				(pin bidirectional line
					(at 97.79 -55.88 180)
					(length 5.08)
					(name "GPIO47PB9/CLKIN_S_13/CCC_SE_CLKIN_S_13")
					(number "B28")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GPIO22NB9")
					(number "C16")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GPIO23PB9")
					(number "C17")
				)
				(pin bidirectional line
					(at 97.79 -7.62 180)
					(length 5.08)
					(name "GPIO37NB9")
					(number "C21")
				)
				(pin bidirectional line
					(at 97.79 -22.86 180)
					(length 5.08)
					(name "GPIO40NB9")
					(number "C22")
				)
				(pin bidirectional line
					(at 97.79 -15.24 180)
					(length 5.08)
					(name "GPIO39PB9")
					(number "C23")
				)
				(pin bidirectional line
					(at 97.79 -33.02 180)
					(length 5.08)
					(name "GPIO42NB9")
					(number "C24")
				)
				(pin bidirectional line
					(at 97.79 -43.18 180)
					(length 5.08)
					(name "GPIO44NB9/DQS")
					(number "C26")
				)
				(pin bidirectional line
					(at 97.79 -40.64 180)
					(length 5.08)
					(name "GPIO44PB9/DQS/CCC_SE_PLL0_OUT0")
					(number "C27")
				)
				(pin bidirectional line
					(at 97.79 -58.42 180)
					(length 5.08)
					(name "GPIO47NB9")
					(number "C28")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GPIO18NB9")
					(number "D15")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GPIO22PB9")
					(number "D16")
				)
				(pin bidirectional line
					(at 97.79 -2.54 180)
					(length 5.08)
					(name "GPIO36NB9")
					(number "D20")
				)
				(pin bidirectional line
					(at 97.79 0 180)
					(length 5.08)
					(name "GPIO36PB9")
					(number "D21")
				)
				(pin bidirectional line
					(at 97.79 -17.78 180)
					(length 5.08)
					(name "GPIO39NB9")
					(number "D23")
				)
				(pin bidirectional line
					(at 97.79 -53.34 180)
					(length 5.08)
					(name "GPIO46NB9")
					(number "D24")
				)
				(pin bidirectional line
					(at 97.79 -50.8 180)
					(length 5.08)
					(name "GPIO46PB9/CCC_SE_PLL0_OUT1")
					(number "D25")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GPIO18PB9")
					(number "E15")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GPIO21NB9")
					(number "E16")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GPIO21PB9")
					(number "E17")
				)
				(pin bidirectional line
					(at 97.79 -76.2 180)
					(length 5.08)
					(name "GPIO51PB9/CCC_SE_CLKIN_S_14/CCC_SE_PLL1_OUT0")
					(number "E21")
				)
				(pin bidirectional line
					(at 97.79 -78.74 180)
					(length 5.08)
					(name "GPIO51NB9")
					(number "E22")
				)
				(pin bidirectional line
					(at 97.79 -88.9 180)
					(length 5.08)
					(name "GPIO53NB9")
					(number "E23")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "GPIO28NB9")
					(number "F15")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GPIO25NB9")
					(number "F17")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "GPIO30PB9")
					(number "F18")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "GPIO30NB9")
					(number "F19")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "GPIO34PB9")
					(number "F20")
				)
				(pin bidirectional line
					(at 97.79 -71.12 180)
					(length 5.08)
					(name "GPIO50PB9/DQS/CCC_SE_PLL1_OUT0")
					(number "F22")
				)
				(pin bidirectional line
					(at 97.79 -86.36 180)
					(length 5.08)
					(name "GPIO53PB9/CCC_SE_CLKIN_S_15")
					(number "F23")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "GPIO28PB9")
					(number "G15")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GPIO26PB9/DQS")
					(number "G16")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GPIO25PB9")
					(number "G17")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "GPIO31PB9")
					(number "G19")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "GPIO34NB9")
					(number "G20")
				)
				(pin bidirectional line
					(at 97.79 -63.5 180)
					(length 5.08)
					(name "GPIO48NB9")
					(number "G21")
				)
				(pin bidirectional line
					(at 97.79 -73.66 180)
					(length 5.08)
					(name "GPIO50NB9/DQS")
					(number "G22")
				)
				(pin bidirectional line
					(at 97.79 -83.82 180)
					(length 5.08)
					(name "GPIO52NB9")
					(number "G23")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GPIO26NB9/DQS")
					(number "H16")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GPIO27PB9")
					(number "H17")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "GPIO31NB9")
					(number "H18")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "GPIO35PB9")
					(number "H19")
				)
				(pin bidirectional line
					(at 97.79 -60.96 180)
					(length 5.08)
					(name "GPIO48PB9")
					(number "H21")
				)
				(pin bidirectional line
					(at 97.79 -81.28 180)
					(length 5.08)
					(name "GPIO52PB9/CCC_SE_PLL1_OUT1")
					(number "H22")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GPIO24NB9")
					(number "J15")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GPIO27NB9")
					(number "J16")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "GPIO32PB9/DQS")
					(number "J18")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "GPIO35NB9")
					(number "J19")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "GPIO33NB9")
					(number "J20")
				)
				(pin bidirectional line
					(at 97.79 -68.58 180)
					(length 5.08)
					(name "GPIO49NB9")
					(number "J21")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GPIO24PB9")
					(number "K15")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "GPIO29NB9")
					(number "K16")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "GPIO29PB9")
					(number "K17")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "GPIO32NB9/DQS")
					(number "K18")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "GPIO33PB9")
					(number "K20")
				)
				(pin bidirectional line
					(at 97.79 -66.04 180)
					(length 5.08)
					(name "GPIO49PB9")
					(number "K21")
				)
			)
			(symbol "RTPFS160ZT-FCVG784_11_1"
				(text "XCVR"
					(at 22.86 2.54 0)
				)
				(pin output line
					(at 0 -25.4 0)
					(length 5.08)
					(name "XCVR_0_TX3_N")
					(number "AA27")
				)
				(pin output line
					(at 0 -22.86 0)
					(length 5.08)
					(name "XCVR_0_TX3_P")
					(number "AA28")
				)
				(pin output line
					(at 0 -46.99 0)
					(length 5.08)
					(name "XCVR_1_TX0_N")
					(number "E27")
				)
				(pin output line
					(at 0 -44.45 0)
					(length 5.08)
					(name "XCVR_1_TX0_P")
					(number "E28")
				)
				(pin input line
					(at 50.8 -46.99 180)
					(length 5.08)
					(name "XCVR_1_RX0_N")
					(number "F25")
				)
				(pin input line
					(at 50.8 -44.45 180)
					(length 5.08)
					(name "XCVR_1_RX0_P")
					(number "F26")
				)
				(pin output line
					(at 0 -54.61 0)
					(length 5.08)
					(name "XCVR_1_TX1_N")
					(number "G27")
				)
				(pin output line
					(at 0 -52.07 0)
					(length 5.08)
					(name "XCVR_1_TX1_P")
					(number "G28")
				)
				(pin input line
					(at 50.8 -54.61 180)
					(length 5.08)
					(name "XCVR_1_RX1_N")
					(number "H25")
				)
				(pin input line
					(at 50.8 -52.07 180)
					(length 5.08)
					(name "XCVR_1_RX1_P")
					(number "H26")
				)
				(pin input line
					(at 0 -82.55 0)
					(length 5.08)
					(name "XCVR_1C_REFCLK_P")
					(number "J23")
				)
				(pin input line
					(at 0 -85.09 0)
					(length 5.08)
					(name "XCVR_1C_REFCLK_N")
					(number "J24")
				)
				(pin output line
					(at 0 -62.23 0)
					(length 5.08)
					(name "XCVR_1_TX2_N")
					(number "J27")
				)
				(pin output line
					(at 0 -59.69 0)
					(length 5.08)
					(name "XCVR_1_TX2_P")
					(number "J28")
				)
				(pin input line
					(at 50.8 -62.23 180)
					(length 5.08)
					(name "XCVR_1_RX2_N")
					(number "K25")
				)
				(pin input line
					(at 50.8 -59.69 180)
					(length 5.08)
					(name "XCVR_1_RX2_P")
					(number "K26")
				)
				(pin input line
					(at 0 -74.93 0)
					(length 5.08)
					(name "XCVR_1A_REFCLK_P")
					(number "L23")
				)
				(pin input line
					(at 0 -77.47 0)
					(length 5.08)
					(name "XCVR_1A_REFCLK_N")
					(number "L24")
				)
				(pin output line
					(at 0 -69.85 0)
					(length 5.08)
					(name "XCVR_1_TX3_N")
					(number "L27")
				)
				(pin output line
					(at 0 -67.31 0)
					(length 5.08)
					(name "XCVR_1_TX3_P")
					(number "L28")
				)
				(pin input line
					(at 50.8 -74.93 180)
					(length 5.08)
					(name "XCVR_1B_REFCLK_P")
					(number "M25")
				)
				(pin input line
					(at 50.8 -77.47 180)
					(length 5.08)
					(name "XCVR_1B_REFCLK_N")
					(number "M26")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 5.08)
					(name "XCVR_0C_REFCLK_P")
					(number "N23")
				)
				(pin input line
					(at 0 -39.37 0)
					(length 5.08)
					(name "XCVR_0C_REFCLK_N")
					(number "N24")
				)
				(pin input line
					(at 50.8 -69.85 180)
					(length 5.08)
					(name "XCVR_1_RX3_N")
					(number "N27")
				)
				(pin input line
					(at 50.8 -67.31 180)
					(length 5.08)
					(name "XCVR_1_RX3_P")
					(number "N28")
				)
				(pin input line
					(at 50.8 -2.54 180)
					(length 5.08)
					(name "XCVR_0_RX0_N")
					(number "P25")
				)
				(pin input line
					(at 50.8 0 180)
					(length 5.08)
					(name "XCVR_0_RX0_P")
					(number "P26")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "XCVR_0A_REFCLK_P")
					(number "R23")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "XCVR_0A_REFCLK_N")
					(number "R24")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 5.08)
					(name "XCVR_0_TX0_N")
					(number "R27")
				)
				(pin output line
					(at 0 0 0)
					(length 5.08)
					(name "XCVR_0_TX0_P")
					(number "R28")
				)
				(pin input line
					(at 50.8 -10.16 180)
					(length 5.08)
					(name "XCVR_0_RX1_N")
					(number "T25")
				)
				(pin input line
					(at 50.8 -7.62 180)
					(length 5.08)
					(name "XCVR_0_RX1_P")
					(number "T26")
				)
				(pin input line
					(at 50.8 -30.48 180)
					(length 5.08)
					(name "XCVR_0B_REFCLK_P")
					(number "U23")
				)
				(pin input line
					(at 50.8 -33.02 180)
					(length 5.08)
					(name "XCVR_0B_REFCLK_N")
					(number "U24")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 5.08)
					(name "XCVR_0_TX1_N")
					(number "U27")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 5.08)
					(name "XCVR_0_TX1_P")
					(number "U28")
				)
				(pin input line
					(at 50.8 -17.78 180)
					(length 5.08)
					(name "XCVR_0_RX2_N")
					(number "V25")
				)
				(pin input line
					(at 50.8 -15.24 180)
					(length 5.08)
					(name "XCVR_0_RX2_P")
					(number "V26")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 5.08)
					(name "XCVR_0_TX2_N")
					(number "W27")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 5.08)
					(name "XCVR_0_TX2_P")
					(number "W28")
				)
				(pin input line
					(at 50.8 -25.4 180)
					(length 5.08)
					(name "XCVR_0_RX3_N")
					(number "Y25")
				)
				(pin input line
					(at 50.8 -22.86 180)
					(length 5.08)
					(name "XCVR_0_RX3_P")
					(number "Y26")
				)
			)
			(symbol "RTPFS160ZT-FCVG784_12_1"
				(pin power_in line
					(at 33.02 -2.54 180)
					(length 5.08)
					(name "VDDI1")
					(number "A1")
				)
				(pin power_out line
					(at 0 -25.4 0)
					(length 5.08)
					(name "VSS")
					(number "A6")
				)
				(pin passive line
					(at 33.02 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "VDDI1")
					(number "A11")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "A16")
				)
				(pin no_connect line
					(at 5.08 -27.94 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A17")
				)
				(pin no_connect line
					(at 5.08 -27.94 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A18")
				)
				(pin no_connect line
					(at 5.08 -27.94 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A19")
				)
				(pin no_connect line
					(at 5.08 -27.94 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A20")
				)
				(pin power_in line
					(at 33.02 -22.86 180)
					(length 5.08)
					(name "VDDI9")
					(number "A21")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "A26")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "A28")
				)
				(pin power_in line
					(at 33.02 -15.24 180)
					(length 5.08)
					(name "VDDI6")
					(number "AA1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA6")
				)
				(pin passive line
					(at 33.02 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VDDI6")
					(number "AA11")
				)
				(pin power_in line
					(at 33.02 -20.32 180)
					(length 5.08)
					(name "VDDI8")
					(number "AA16")
				)
				(pin power_in line
					(at 33.02 0 180)
					(length 5.08)
					(name "VDDI0")
					(number "AA21")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA24")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA25")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA26")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB3")
				)
				(pin passive line
					(at 33.02 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VDDI6")
					(number "AB8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB13")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 5.08)
					(hide yes)
					(name "VDDI0")
					(number "AB18")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB23")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB26")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB27")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB28")
				)
				(pin passive line
					(at 33.02 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VDDI6")
					(number "AC5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC10")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 5.08)
					(hide yes)
					(name "VDDI8")
					(number "AC15")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC20")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 5.08)
					(hide yes)
					(name "VDDI0")
					(number "AC25")
				)
				(pin passive line
					(at 33.02 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VDDI6")
					(number "AD2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD7")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 5.08)
					(hide yes)
					(name "VDDI8")
					(number "AD12")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD17")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 5.08)
					(hide yes)
					(name "VDDI0")
					(number "AD22")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD27")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE4")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 5.08)
					(hide yes)
					(name "VDDI8")
					(number "AE9")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE14")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 5.08)
					(hide yes)
					(name "VDDI0")
					(number "AE19")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE24")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 5.08)
					(hide yes)
					(name "VDDI8")
					(number "AF6")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF11")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 5.08)
					(hide yes)
					(name "VDDI0")
					(number "AF16")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF21")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 5.08)
					(hide yes)
					(name "VDDI0")
					(number "AF26")
				)
				(pin passive line
					(at 33.02 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VDDI6")
					(number "AG3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG8")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 5.08)
					(hide yes)
					(name "VDDI8")
					(number "AG13")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG18")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 5.08)
					(hide yes)
					(name "VDDI0")
					(number "AG23")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH5")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 5.08)
					(hide yes)
					(name "VDDI8")
					(number "AH10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH15")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 5.08)
					(hide yes)
					(name "VDDI0")
					(number "AH20")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH25")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH28")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "B3")
				)
				(pin passive line
					(at 33.02 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "VDDI1")
					(number "B8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "B13")
				)
				(pin passive line
					(at 33.02 -22.86 180)
					(length 5.08)
					(hide yes)
					(name "VDDI9")
					(number "B18")
				)
				(pin no_connect line
					(at 5.08 -27.94 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B19")
				)
				(pin no_connect line
					(at 5.08 -27.94 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B20")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "B23")
				)
				(pin passive line
					(at 33.02 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "VDDI1")
					(number "C5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C10")
				)
				(pin passive line
					(at 33.02 -22.86 180)
					(length 5.08)
					(hide yes)
					(name "VDDI9")
					(number "C15")
				)
				(pin no_connect line
					(at 5.08 -27.94 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "C18")
				)
				(pin no_connect line
					(at 5.08 -27.94 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "C19")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C20")
				)
				(pin passive line
					(at 33.02 -22.86 180)
					(length 5.08)
					(hide yes)
					(name "VDDI9")
					(number "C25")
				)
				(pin passive line
					(at 33.02 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "VDDI1")
					(number "D2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D7")
				)
				(pin passive line
					(at 33.02 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "VDDI1")
					(number "D12")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D17")
				)
				(pin no_connect line
					(at 5.08 -27.94 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D18")
				)
				(pin no_connect line
					(at 5.08 -27.94 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "D19")
				)
				(pin passive line
					(at 33.02 -22.86 180)
					(length 5.08)
					(hide yes)
					(name "VDDI9")
					(number "D22")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D26")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D27")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D28")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E4")
				)
				(pin passive line
					(at 33.02 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "VDDI1")
					(number "E9")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E14")
				)
				(pin no_connect line
					(at 5.08 -27.94 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "E18")
				)
				(pin passive line
					(at 33.02 -22.86 180)
					(length 5.08)
					(hide yes)
					(name "VDDI9")
					(number "E19")
				)
				(pin no_connect line
					(at 5.08 -27.94 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "E20")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E24")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E25")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E26")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F1")
				)
				(pin passive line
					(at 33.02 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "VDDI1")
					(number "F6")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F11")
				)
				(pin passive line
					(at 33.02 -22.86 180)
					(length 5.08)
					(hide yes)
					(name "VDDI9")
					(number "F16")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F21")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F24")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F27")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F28")
				)
				(pin power_in line
					(at 33.02 -17.78 180)
					(length 5.08)
					(name "VDDI7")
					(number "G3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G8")
				)
				(pin passive line
					(at 33.02 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "VDDI1")
					(number "G13")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G18")
				)
				(pin power_in line
					(at 33.02 -25.4 180)
					(length 5.08)
					(name "XCVR_VREF")
					(number "G24")
				)
				(pin power_in line
					(at 33.02 -27.94 180)
					(length 5.08)
					(name "VDD_XCVR_CLK")
					(number "G25")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G26")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H5")
				)
				(pin passive line
					(at 33.02 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "VDDI1")
					(number "H10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H15")
				)
				(pin passive line
					(at 33.02 -22.86 180)
					(length 5.08)
					(hide yes)
					(name "VDDI9")
					(number "H20")
				)
				(pin passive line
					(at 33.02 -25.4 180)
					(length 5.08)
					(hide yes)
					(name "XCVR_VREF")
					(number "H23")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H24")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 5.08)
					(name "VDDA")
					(number "H27")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H28")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J2")
				)
				(pin passive line
					(at 33.02 -17.78 180)
					(length 5.08)
					(hide yes)
					(name "VDDI7")
					(number "J7")
				)
				(pin passive line
					(at 33.02 -22.86 180)
					(length 5.08)
					(hide yes)
					(name "VDDI9")
					(number "J17")
				)
				(pin passive line
					(at 33.02 -22.86 180)
					(length 5.08)
					(hide yes)
					(name "VDDI9")
					(number "J22")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 5.08)
					(name "VDDA25")
					(number "J25")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J26")
				)
				(pin passive line
					(at 33.02 -17.78 180)
					(length 5.08)
					(hide yes)
					(name "VDDI7")
					(number "K4")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K9")
				)
				(pin power_in line
					(at 33.02 -7.62 180)
					(length 5.08)
					(name "VDDI3")
					(number "K11")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 5.08)
					(name "VDDAUX1")
					(number "K13")
				)
				(pin passive line
					(at 33.02 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "VDDI1")
					(number "K14")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 5.08)
					(name "VDDAUX9")
					(number "K19")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VDD25")
					(number "K22")
				)
				(pin passive line
					(at 33.02 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDD_XCVR_CLK")
					(number "K23")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K24")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDDA")
					(number "K27")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K28")
				)
				(pin power_in line
					(at 33.02 -5.08 180)
					(length 5.08)
					(name "VDDI2")
					(number "L1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L6")
				)
				(pin passive line
					(at 33.02 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "VDDI2")
					(number "L11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD25")
					(number "L12")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L13")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "VDDAUX1")
					(number "L14")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 5.08)
					(hide yes)
					(name "VDDI3")
					(number "L15")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "VDDAUX1")
					(number "L16")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L17")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(hide yes)
					(name "VDDAUX9")
					(number "L18")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L19")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(hide yes)
					(name "VDDAUX9")
					(number "L20")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L21")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(hide yes)
					(name "VDDAUX9")
					(number "L22")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDDA")
					(number "L25")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L26")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M3")
				)
				(pin passive line
					(at 33.02 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "VDDI2")
					(number "M8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M12")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 5.08)
					(name "VDDAUX7")
					(number "M13")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M14")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VDD")
					(number "M15")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "M17")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M18")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "M19")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "M21")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M22")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VDDA25")
					(number "M23")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M24")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDDA")
					(number "M27")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M28")
				)
				(pin power_in line
					(at 33.02 -10.16 180)
					(length 5.08)
					(name "VDDI4")
					(number "N5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N10")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 5.08)
					(name "VDDAUX2")
					(number "N12")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N13")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(hide yes)
					(name "VDDAUX7")
					(number "N14")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "N16")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "N18")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "N20")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N21")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "N22")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDDA")
					(number "N25")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N26")
				)
				(pin passive line
					(at 33.02 -10.16 180)
					(length 5.08)
					(hide yes)
					(name "VDDI4")
					(number "P2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P12")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "VDDAUX2")
					(number "P13")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "P15")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "P17")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P18")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "P19")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "P21")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P22")
				)
				(pin passive line
					(at 33.02 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDD_XCVR_CLK")
					(number "P23")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P24")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDDA")
					(number "P27")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P28")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R4")
				)
				(pin power_in line
					(at 33.02 -12.7 180)
					(length 5.08)
					(name "VDDI5")
					(number "R9")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 5.08)
					(name "VDDAUX4")
					(number "R12")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "R14")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "R16")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R17")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD25")
					(number "R18")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "R20")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R21")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "R22")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDDA")
					(number "R25")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R26")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T1")
				)
				(pin passive line
					(at 33.02 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VDDI6")
					(number "T6")
				)
				(pin passive line
					(at 33.02 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "VDDI5")
					(number "T11")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T12")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(hide yes)
					(name "VDDAUX4")
					(number "T13")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "T15")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "T17")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T18")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "T19")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "T21")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T22")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VDDA25")
					(number "T23")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T24")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDDA")
					(number "T27")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T28")
				)
				(pin passive line
					(at 33.02 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VDDI6")
					(number "U3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U8")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD25")
					(number "U12")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "U14")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "U16")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U17")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD18")
					(number "U18")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "U20")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U21")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD18")
					(number "U22")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VDDA25")
					(number "U25")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U26")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V5")
				)
				(pin passive line
					(at 33.02 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VDDI6")
					(number "V10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD18")
					(number "V13")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD18")
					(number "V15")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V16")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD18")
					(number "V17")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V18")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD18")
					(number "V19")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V20")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD18")
					(number "V21")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V22")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V23")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V24")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDDA")
					(number "V27")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V28")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W2")
				)
				(pin passive line
					(at 33.02 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VDDI6")
					(number "W7")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD18")
					(number "W12")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VDD18")
					(number "W13")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 5.08)
					(hide yes)
					(name "VDDI8")
					(number "W14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD18")
					(number "W16")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 5.08)
					(hide yes)
					(name "VDDI0")
					(number "W18")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD25")
					(number "W23")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W24")
				)
				(pin passive line
					(at 33.02 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDD_XCVR_CLK")
					(number "W25")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W26")
				)
				(pin passive line
					(at 33.02 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VDDI6")
					(number "Y4")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y9")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y24")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDDA")
					(number "Y27")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y28")
				)
			)
			(embedded_fonts no)
		)
)
