(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "WiFi_XBP9B-DMUT-002"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "A"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "WiFi_XBP9B-DMUT-002"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "WiFi_XBP9B-DMUT-002"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.digi.com/resources/documentation/digidocs/pdfs/90002173.pdf"
				(at 55.88 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF transceiver module"
				(at 55.88 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "XBP9B-DMUT-002"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Digi International"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "WiFi_XBP9B-DMUT-002_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "Vcc")
					(number "1")
				)
				(pin output line
					(at 40.64 -20.32 180)
					(length 2.54)
					(name "UART_Data_Out")
					(number "2")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "UART_Data_in/Config")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DO8")
					(number "4")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "/Reset")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "PWM0-RSSI")
					(number "6")
				)
				(pin output line
					(at 40.64 0 180)
					(length 2.54)
					(name "PWM1")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "Reserved")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "DTR-SLEEP-RQ-DI8")
					(number "9")
				)
				(pin power_in line
					(at 40.64 -22.86 180)
					(length 2.54)
					(name "GND")
					(number "10")
				)
				(pin bidirectional line
					(at 40.64 -12.7 180)
					(length 2.54)
					(name "AD4-DIO4")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "DIO7-/CTS")
					(number "12")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "ON-/SLEEP")
					(number "13")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "VREF")
					(number "14")
				)
				(pin bidirectional line
					(at 40.64 -15.24 180)
					(length 2.54)
					(name "AD5-DIO5")
					(number "15")
				)
				(pin bidirectional line
					(at 40.64 -17.78 180)
					(length 2.54)
					(name "AD6-DIO6-/RTS")
					(number "16")
				)
				(pin bidirectional line
					(at 40.64 -10.16 180)
					(length 2.54)
					(name "AD3-DIO3")
					(number "17")
				)
				(pin bidirectional line
					(at 40.64 -7.62 180)
					(length 2.54)
					(name "AD2-DIO2")
					(number "18")
				)
				(pin bidirectional line
					(at 40.64 -5.08 180)
					(length 2.54)
					(name "AD1-DIO1")
					(number "19")
				)
				(pin bidirectional line
					(at 40.64 -2.54 180)
					(length 2.54)
					(name "AD0-DIO0")
					(number "20")
				)
			)
			(embedded_fonts no)
		)
)
