(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "GNSS_ZED-X20P-00B"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "GNSS_ZED-X20P-00B"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "GNSS_ZED-X20P-00B"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.u-blox.com/sites/default/files/documents/ZED-X20P-00B_DataSheet_UBXDOC-963802114-12690.pdf"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "All-band high precision GNSS module Professional grade"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ZED-X20P-00B"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "u-blox"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, GNSS, RF"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "GNSS_ZED-X20P-00B_1_1"
				(pin power_in line
					(at 31.75 -45.72 180)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(name "RF_IN")
					(number "2")
				)
				(pin passive line
					(at 31.75 -45.72 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "3")
				)
				(pin input line
					(at 31.75 -2.54 180)
					(length 2.54)
					(name "ANT_DETECT")
					(number "4")
				)
				(pin output line
					(at 31.75 -7.62 180)
					(length 2.54)
					(name "ANT_OFF")
					(number "5")
				)
				(pin input line
					(at 31.75 -5.08 180)
					(length 2.54)
					(name "~{ANT_SHORT}")
					(number "6")
				)
				(pin power_out line
					(at 31.75 0 180)
					(length 2.54)
					(name "VCC_{RF}")
					(number "7")
				)
				(pin no_connect line
					(at 29.21 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "8")
				)
				(pin no_connect line
					(at 29.21 -13.97 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "9")
				)
				(pin no_connect line
					(at 29.21 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "10")
				)
				(pin no_connect line
					(at 29.21 -19.05 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "11")
				)
				(pin passive line
					(at 31.75 -45.72 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "12")
				)
				(pin no_connect line
					(at 29.21 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "13")
				)
				(pin passive line
					(at 31.75 -45.72 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "14")
				)
				(pin no_connect line
					(at 29.21 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "15")
				)
				(pin no_connect line
					(at 29.21 -22.86 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "16")
				)
				(pin no_connect line
					(at 29.21 -24.13 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "17")
				)
				(pin no_connect line
					(at 29.21 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "18")
				)
				(pin output line
					(at 31.75 -40.64 180)
					(length 2.54)
					(name "GEOFENCE_STAT")
					(number "19")
				)
				(pin output line
					(at 31.75 -38.1 180)
					(length 2.54)
					(name "RTK_STAT")
					(number "20")
				)
				(pin no_connect line
					(at 29.21 -26.67 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "21")
				)
				(pin no_connect line
					(at 29.21 -27.94 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "22")
				)
				(pin no_connect line
					(at 29.21 -29.21 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "23")
				)
				(pin no_connect line
					(at 29.21 -30.48 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "24")
				)
				(pin no_connect line
					(at 29.21 -31.75 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "25")
				)
				(pin input line
					(at 0 -29.21 0)
					(length 2.54)
					(name "RXD2")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 2.54)
					(name "TXD2")
					(number "27")
				)
				(pin no_connect line
					(at 29.21 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "28")
				)
				(pin no_connect line
					(at 29.21 -16.51 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "29")
				)
				(pin no_connect line
					(at 29.21 -34.29 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "30")
				)
				(pin no_connect line
					(at 29.21 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "31")
				)
				(pin passive line
					(at 31.75 -45.72 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "32")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "33")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "34")
				)
				(pin no_connect line
					(at 29.21 -35.56 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "35")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "V_{BCKP}")
					(number "36")
				)
				(pin passive line
					(at 31.75 -45.72 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "37")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "RSVD")
					(number "38")
				)
				(pin no_connect line
					(at 2.54 -11.43 0)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "39")
				)
				(pin no_connect line
					(at 2.54 -8.89 0)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "40")
				)
				(pin passive line
					(at 31.75 -45.72 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "41")
				)
				(pin output line
					(at 0 -21.59 0)
					(length 2.54)
					(name "TXD/MISO")
					(number "42")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 2.54)
					(name "RXD/MOSI")
					(number "43")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "SDA/~{CS}")
					(number "44")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "SCL/CLK")
					(number "45")
				)
				(pin output line
					(at 0 -31.75 0)
					(length 2.54)
					(name "TX_READY")
					(number "46")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "D_SEL")
					(number "47")
				)
				(pin passive line
					(at 31.75 -45.72 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "48")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 2.54)
					(name "~{RESET}")
					(number "49")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "~{SAFEBOOT}")
					(number "50")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "EXTINT")
					(number "51")
				)
				(pin no_connect line
					(at 29.21 -10.16 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "52")
				)
				(pin output line
					(at 31.75 -43.18 180)
					(length 2.54)
					(name "TIMEPULSE")
					(number "53")
				)
				(pin no_connect line
					(at 29.21 -11.43 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "54")
				)
				(pin passive line
					(at 31.75 -45.72 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "55")
				)
			)
			(embedded_fonts no)
		)
)
