(footprint "ZM-VF01A"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Footprint based on: https://zero-errorsystems.com/wp-content/uploads/2025/03/ZM-VF01A-Datasheet-v1.0.pdf")
	(property "Reference" "REF**"
		(at -6.6 -6.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "ZM-VF01A"
		(at -1.2 10.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -1.149 11.75 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.149 12.95 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1.149 14.15 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 4.7 -4.7)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 4.7 4.7)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -5.6 -3 90)
		(size 1.4 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -5.6 -1 90)
		(size 1.4 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -5.6 1 90)
		(size 1.4 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -5.6 3 90)
		(size 1.4 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3 5.6 180)
		(size 1.4 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -1 5.6 180)
		(size 1.4 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1 5.6 180)
		(size 1.4 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 3 5.6 180)
		(size 1.4 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 5.6 3 90)
		(size 1.4 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 5.6 1 90)
		(size 1.4 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 5.6 -1 90)
		(size 1.4 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 5.6 -3 90)
		(size 1.4 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 3 -5.6 180)
		(size 1.4 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 1 -5.6 180)
		(size 1.4 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -1 -5.6 180)
		(size 1.4 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -3 -5.6 180)
		(size 1.4 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_zm_vf01a.glb"
		(offset
			(xyz 100 100 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 90)
		)
	)
)
