(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ZM-VF01A"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 54.61 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ZM-VF01A"
				(at 54.61 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ZM-VF01A"
				(at 54.61 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://zero-errorsystems.com/wp-content/uploads/2025/03/ZM-VF01A-Datasheet-v1.0.pdf"
				(at 54.61 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Radiation-hardened voter module, TMR support, ultra-low-error FRAM module"
				(at 54.61 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ZM-VF01A"
				(at 54.61 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Zero-Error Systems"
				(at 54.61 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 54.61 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 54.61 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ZM-VF01A_1_1"
				(pin input line
					(at 31.75 0 180)
					(length 3.81)
					(name "FRAM_CS")
					(number "1")
				)
				(pin output line
					(at 31.75 -7.62 180)
					(length 3.81)
					(name "MISO_Y")
					(number "2")
				)
				(pin input line
					(at 31.75 -15.24 180)
					(length 3.81)
					(name "FRAM_WP")
					(number "3")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 3.81)
					(name "GND")
					(number "4")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 3.81)
					(name "V_IN1")
					(number "5")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "V_IN2")
					(number "6")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "V_IN3")
					(number "7")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "8")
				)
				(pin input line
					(at 31.75 -5.08 180)
					(length 3.81)
					(name "FRAM_MOSI")
					(number "9")
				)
				(pin input line
					(at 31.75 -2.54 180)
					(length 3.81)
					(name "FRAM_SCK")
					(number "10")
				)
				(pin input line
					(at 31.75 -12.7 180)
					(length 3.81)
					(name "FRAM_HD")
					(number "11")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "12")
				)
				(pin output line
					(at 31.75 -17.78 180)
					(length 3.81)
					(name "V_E")
					(number "13")
				)
				(pin power_out line
					(at 31.75 -20.32 180)
					(length 3.81)
					(name "V_Y")
					(number "14")
				)
				(pin output line
					(at 31.75 -10.16 180)
					(length 3.81)
					(name "MISO_E")
					(number "15")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
