(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "BM15x"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 0 0)
				(do_not_autoplace)
			)
			(property "Value" "BM15x"
				(at 0 -2.54 0)
				(do_not_autoplace)
			)
			(property "Footprint" "nordic-lib-kicad-nrf54-modules:BM15x-LGA-45_15.8x10mm"
				(at 0 -50.8 0)
			)
			(property "Datasheet" "https://static1.squarespace.com/static/561459a2e4b0b39f5cefa12e/t/66c3d7591cc204465c3f6e4f/1724110684125/BM15C+Product+Specifications.pdf"
				(at 0 -48.26 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "nRF54L15"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "BM15*-LGA-45*15.8x10mm*"
				(at 0 0 0)
			)
			(symbol "BM15x_0_0"
				(pin passive line
					(at 0 58.42 270)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "C8")
				)
				(pin passive line
					(at 0 -58.42 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "A9")
				)
				(pin passive line
					(at 0 -58.42 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "B1")
				)
				(pin passive line
					(at 0 -58.42 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "B7")
				)
				(pin passive line
					(at 0 -58.42 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "B9")
				)
				(pin passive line
					(at 0 -58.42 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "D1")
				)
				(pin passive line
					(at 0 -58.42 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "E1")
				)
				(pin passive line
					(at 0 -58.42 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "F1")
				)
				(pin passive line
					(at 0 -58.42 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "H8")
				)
				(pin input line
					(at 27.94 -43.18 180)
					(length 2.54)
					(name "~{RESET}")
					(number "G2")
				)
				(pin input line
					(at 27.94 -48.26 180)
					(length 2.54)
					(name "SWDCLK")
					(number "K3")
				)
				(pin bidirectional line
					(at 27.94 -50.8 180)
					(length 2.54)
					(name "SWDIO")
					(number "J3")
				)
			)
			(symbol "BM15x_1_0"
				(pin bidirectional line
					(at -27.94 38.1 0)
					(length 2.54)
					(name "P1.00")
					(number "D8")
					(alternate "XL1" bidirectional line)
				)
				(pin bidirectional line
					(at -27.94 33.02 0)
					(length 2.54)
					(name "P1.01")
					(number "C9")
					(alternate "XL2" bidirectional line)
				)
				(pin bidirectional line
					(at -27.94 25.4 0)
					(length 2.54)
					(name "P0.00")
					(number "J4")
				)
				(pin bidirectional line
					(at -27.94 22.86 0)
					(length 2.54)
					(name "P0.01")
					(number "K4")
				)
				(pin bidirectional line
					(at -27.94 20.32 0)
					(length 2.54)
					(name "P0.02")
					(number "K2")
				)
				(pin bidirectional line
					(at -27.94 17.78 0)
					(length 2.54)
					(name "P0.03")
					(number "J2")
					(alternate "GRTCPWM" output line)
				)
				(pin bidirectional line
					(at -27.94 15.24 0)
					(length 2.54)
					(name "P0.04")
					(number "H2")
					(alternate "GRTCLFCLKOUT" output line)
				)
				(pin bidirectional line
					(at -27.94 10.16 0)
					(length 2.54)
					(name "P1.02")
					(number "D9")
					(alternate "NFC1" bidirectional line)
				)
				(pin bidirectional line
					(at -27.94 7.62 0)
					(length 2.54)
					(name "P1.03")
					(number "E8")
					(alternate "NFC2" bidirectional line)
				)
				(pin bidirectional line
					(at -27.94 5.08 0)
					(length 2.54)
					(name "P1.04")
					(number "E9")
					(alternate "AIN0" input line)
					(alternate "ASO[0]" output line)
				)
				(pin bidirectional line
					(at -27.94 2.54 0)
					(length 2.54)
					(name "P1.05")
					(number "F8")
					(alternate "AIN1" bidirectional line)
					(alternate "ASI[0]" input line)
				)
				(pin bidirectional line
					(at -27.94 0 0)
					(length 2.54)
					(name "P1.06")
					(number "F9")
					(alternate "AIN2" input line)
					(alternate "ASO[1]" output line)
				)
				(pin bidirectional line
					(at -27.94 -2.54 0)
					(length 2.54)
					(name "P1.07")
					(number "G9")
					(alternate "AIN3" input line)
					(alternate "ASI[1]" input line)
				)
				(pin bidirectional line
					(at -27.94 -5.08 0)
					(length 2.54)
					(name "P1.08")
					(number "G8")
					(alternate "EXTREF" input line)
					(alternate "GRTCHFOUT" output line)
					(alternate "TAMPC.EXT" bidirectional line)
				)
				(pin bidirectional line
					(at -27.94 -7.62 0)
					(length 2.54)
					(name "P1.09")
					(number "A3")
					(alternate "ASO[2]" output line)
				)
				(pin bidirectional line
					(at -27.94 -10.16 0)
					(length 2.54)
					(name "P1.10")
					(number "B2")
					(alternate "ASI[2]" input line)
				)
				(pin bidirectional line
					(at -27.94 -12.7 0)
					(length 2.54)
					(name "P1.11")
					(number "B3")
					(alternate "AIN4" input line)
					(alternate "ASO[3]" output line)
				)
				(pin bidirectional line
					(at -27.94 -15.24 0)
					(length 2.54)
					(name "P1.12")
					(number "B4")
					(alternate "AIN5" input line)
					(alternate "ASI[3]" input line)
				)
				(pin bidirectional line
					(at -27.94 -17.78 0)
					(length 2.54)
					(name "P1.13")
					(number "B5")
					(alternate "AIN6" input line)
				)
				(pin bidirectional line
					(at -27.94 -20.32 0)
					(length 2.54)
					(name "P1.14")
					(number "B6")
					(alternate "AIN7" input line)
				)
				(pin bidirectional line
					(at -27.94 -25.4 0)
					(length 2.54)
					(name "P2.00")
					(number "H9")
					(alternate "QSPI_D3" bidirectional line)
					(alternate "SPIM_DCX" output line)
					(alternate "UARTE_RXD" input line)
				)
				(pin bidirectional line
					(at -27.94 -27.94 0)
					(length 2.54)
					(name "P2.01")
					(number "J9")
					(alternate "QSPI_SCK" output line)
					(alternate "SPIM_SCK" output line)
					(alternate "SPIS_SCK" output line)
				)
				(pin bidirectional line
					(at -27.94 -30.48 0)
					(length 2.54)
					(name "P2.02")
					(number "J8")
					(alternate "QSPI_D0" bidirectional line)
					(alternate "SPIM_MOSI" output line)
					(alternate "SPIS_MISO" output line)
					(alternate "SWO" output line)
					(alternate "UARTE_TXD" output line)
				)
				(pin bidirectional line
					(at -27.94 -33.02 0)
					(length 2.54)
					(name "P2.03")
					(number "J7")
					(alternate "QSPI_D2" bidirectional line)
				)
				(pin bidirectional line
					(at -27.94 -35.56 0)
					(length 2.54)
					(name "P2.04")
					(number "K9")
					(alternate "QSPI_D1" bidirectional line)
					(alternate "SPIM_MISO" input line)
					(alternate "SPIS_MOSI" input line)
					(alternate "UARTE_CTS" input line)
				)
				(pin bidirectional line
					(at -27.94 -38.1 0)
					(length 2.54)
					(name "K8")
					(number "16")
					(alternate "QSPI_CS" output line)
					(alternate "SPIM_CS" output line)
					(alternate "UARTE_RTS" output line)
				)
				(pin bidirectional line
					(at -27.94 -40.64 0)
					(length 2.54)
					(name "P2.06")
					(number "K7")
					(alternate "SPIM_SCK" output line)
					(alternate "SPIS_SCK" input line)
					(alternate "TRACE_CLK" input line)
				)
				(pin bidirectional line
					(at -27.94 -43.18 0)
					(length 2.54)
					(name "J6")
					(number "18")
					(alternate "SPIM_DCX" output line)
					(alternate "SWO" output line)
					(alternate "TRACEDATA[0]" output line)
					(alternate "UARTE_RXD" input line)
				)
				(pin bidirectional line
					(at -27.94 -45.72 0)
					(length 2.54)
					(name "P2.08")
					(number "K6")
					(alternate "SPIM_MOSI" output line)
					(alternate "SPIS_MISO" input line)
					(alternate "TRACEDATA[1]" output line)
					(alternate "UARTE_TXD" output line)
				)
				(pin bidirectional line
					(at -27.94 -48.26 0)
					(length 2.54)
					(name "P2.09")
					(number "J5")
					(alternate "SPIM_MISO" input line)
					(alternate "SPIS_MOSI" input line)
					(alternate "TRACEDATA[2]" output line)
					(alternate "UARTE_CTS" input line)
				)
				(pin bidirectional line
					(at -27.94 -50.8 0)
					(length 2.54)
					(name "P2.10")
					(number "K5")
					(alternate "SPIM_CS" output line)
					(alternate "TRACEDATA[3]" output line)
					(alternate "UARTE_RTS" output line)
				)
				(pin power_in line
					(at 0 58.42 270)
					(length 2.54)
					(name "VDD")
					(number "B8")
				)
				(pin power_in line
					(at 0 -58.42 90)
					(length 2.54)
					(name "GND")
					(number "A1")
				)
			)
			(symbol "BM15x_1_1"
				(text "CLK"
					(at -15.24 17.78 0)
				)
				(text "CLK"
					(at -15.24 15.24 0)
				)
				(text "CLK"
					(at -15.24 7.62 0)
				)
				(text "CLK"
					(at -15.24 5.08 0)
				)
				(text "CLK"
					(at -15.24 -5.08 0)
				)
				(text "CLK"
					(at -15.24 -12.7 0)
				)
				(text "CLK"
					(at -15.24 -15.24 0)
				)
				(text "CLK"
					(at -15.24 -27.94 0)
				)
				(text "CLK"
					(at -15.24 -40.64 0)
				)
			)
			(embedded_fonts no)
		)
)
