(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "BM20x"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 0 0)
				(do_not_autoplace)
			)
			(property "Value" "BM20x"
				(at 0 -2.54 0)
				(do_not_autoplace)
			)
			(property "Footprint" "nordic-lib-kicad-nrf54-modules:BM20x-LGA-90_15.8x10mm"
				(at 0 5.08 0)
			)
			(property "Datasheet" ""
				(at 0 -2.54 0)
			)
			(property "Description" ""
				(at 0 -2.54 0)
			)
			(property "ki_fp_filters" "BM20*-LGA-90*15.8x10mm*"
				(at 0 0 0)
			)
			(symbol "BM20x_0_0"
				(pin power_in line
					(at -22.86 48.26 0)
					(length 2.54)
					(name "VBUS")
					(number "H7")
				)
				(pin bidirectional line
					(at -22.86 38.1 0)
					(length 2.54)
					(name "P6.00")
					(number "J9")
				)
				(pin bidirectional line
					(at -22.86 35.56 0)
					(length 2.54)
					(name "P6.01")
					(number "J6")
				)
				(pin bidirectional line
					(at -22.86 33.02 0)
					(length 2.54)
					(name "P6.02/RWDS")
					(number "D7")
				)
				(pin bidirectional line
					(at -22.86 30.48 0)
					(length 2.54)
					(name "P6.03/CS0")
					(number "E8")
				)
				(pin bidirectional line
					(at -22.86 27.94 0)
					(length 2.54)
					(name "P6.04/DQ7")
					(number "E9")
				)
				(pin bidirectional line
					(at -22.86 25.4 0)
					(length 2.54)
					(name "P6.05")
					(number "K9")
				)
				(pin bidirectional line
					(at -22.86 22.86 0)
					(length 2.54)
					(name "P6.06/DQ6")
					(number "F9")
				)
				(pin bidirectional line
					(at -22.86 20.32 0)
					(length 2.54)
					(name "P6.07")
					(number "J8")
				)
				(pin bidirectional line
					(at -22.86 17.78 0)
					(length 2.54)
					(name "P6.08/DQ5")
					(number "F8")
				)
				(pin bidirectional line
					(at -22.86 15.24 0)
					(length 2.54)
					(name "P6.09/DQ3")
					(number "H9")
				)
				(pin bidirectional line
					(at -22.86 12.7 0)
					(length 2.54)
					(name "P6.10")
					(number "J7")
				)
				(pin bidirectional line
					(at -22.86 10.16 0)
					(length 2.54)
					(name "P6.11")
					(number "A5")
				)
				(pin bidirectional line
					(at -22.86 5.08 0)
					(length 2.54)
					(name "P6.13")
					(number "K8")
				)
				(pin bidirectional line
					(at -22.86 0 0)
					(length 2.54)
					(name "P7.00")
					(number "J5")
				)
				(pin bidirectional line
					(at -22.86 -2.54 0)
					(length 2.54)
					(name "P7.01")
					(number "K7")
				)
				(pin bidirectional line
					(at -22.86 -5.08 0)
					(length 2.54)
					(name "P7.02")
					(number "K5")
				)
				(pin bidirectional line
					(at -22.86 -7.62 0)
					(length 2.54)
					(name "P7.03")
					(number "K6")
				)
				(pin bidirectional line
					(at -22.86 -10.16 0)
					(length 2.54)
					(name "P7.04")
					(number "K4")
				)
				(pin bidirectional line
					(at -22.86 -12.7 0)
					(length 2.54)
					(name "P7.05")
					(number "A7")
				)
				(pin bidirectional line
					(at -22.86 -15.24 0)
					(length 2.54)
					(name "P7.06")
					(number "A6")
				)
				(pin bidirectional line
					(at -22.86 -17.78 0)
					(length 2.54)
					(name "P7.07")
					(number "A8")
				)
				(pin bidirectional line
					(at -22.86 -22.86 0)
					(length 2.54)
					(name "P9.00")
					(number "C9")
				)
				(pin bidirectional line
					(at -22.86 -25.4 0)
					(length 2.54)
					(name "P9.01")
					(number "D8")
				)
				(pin bidirectional line
					(at -22.86 -27.94 0)
					(length 2.54)
					(name "P9.02")
					(number "H4")
				)
				(pin bidirectional line
					(at -22.86 -30.48 0)
					(length 2.54)
					(name "P9.03")
					(number "H5")
				)
				(pin bidirectional line
					(at -22.86 -33.02 0)
					(length 2.54)
					(name "P9.04")
					(number "H6")
				)
				(pin bidirectional line
					(at -22.86 -35.56 0)
					(length 2.54)
					(name "P9.05")
					(number "D4")
				)
				(pin input line
					(at -22.86 -40.64 0)
					(length 2.54)
					(name "~{RESET}")
					(number "G2")
				)
				(pin input line
					(at -22.86 -45.72 0)
					(length 2.54)
					(name "SWDCLK")
					(number "K3")
				)
				(pin bidirectional line
					(at -22.86 -48.26 0)
					(length 2.54)
					(name "SWDIO")
					(number "J3")
				)
				(pin no_connect line
					(at -15.24 50.8 270)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "A4")
				)
				(pin no_connect line
					(at -10.16 50.8 270)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "C6")
				)
				(pin power_in line
					(at -2.54 53.34 270)
					(length 2.54)
					(name "VDD")
					(number "B8")
				)
				(pin power_in line
					(at 0 53.34 270)
					(length 2.54)
					(name "VDD_HV")
					(number "C8")
				)
				(pin passive line
					(at 0 -53.34 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "A9")
				)
				(pin passive line
					(at 0 -53.34 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "B1")
				)
				(pin passive line
					(at 0 -53.34 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "B7")
				)
				(pin passive line
					(at 0 -53.34 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "B9")
				)
				(pin passive line
					(at 0 -53.34 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "C1")
				)
				(pin passive line
					(at 0 -53.34 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "D1")
				)
				(pin passive line
					(at 0 -53.34 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "E1")
				)
				(pin passive line
					(at 0 -53.34 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "F1")
				)
				(pin passive line
					(at 0 -53.34 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "G1")
				)
				(pin passive line
					(at 0 -53.34 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "H1")
				)
				(pin passive line
					(at 0 -53.34 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "H8")
				)
				(pin passive line
					(at 0 -53.34 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "J1")
				)
				(pin passive line
					(at 0 -53.34 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "K1")
				)
				(pin power_in line
					(at 2.54 53.34 270)
					(length 2.54)
					(name "VDD_P9")
					(number "C7")
				)
				(pin bidirectional line
					(at 22.86 48.26 180)
					(length 2.54)
					(name "P0.00")
					(number "F5")
				)
				(pin bidirectional line
					(at 22.86 45.72 180)
					(length 2.54)
					(name "P0.01")
					(number "D6")
				)
				(pin bidirectional line
					(at 22.86 43.18 180)
					(length 2.54)
					(name "P0.02")
					(number "K2")
				)
				(pin bidirectional line
					(at 22.86 40.64 180)
					(length 2.54)
					(name "P0.03")
					(number "J2")
				)
				(pin bidirectional line
					(at 22.86 38.1 180)
					(length 2.54)
					(name "P0.04")
					(number "H2")
				)
				(pin bidirectional line
					(at 22.86 35.56 180)
					(length 2.54)
					(name "P0.05")
					(number "D9")
				)
				(pin bidirectional line
					(at 22.86 33.02 180)
					(length 2.54)
					(name "P0.06")
					(number "D5")
				)
				(pin bidirectional line
					(at 22.86 30.48 180)
					(length 2.54)
					(name "P0.07")
					(number "E3")
				)
				(pin bidirectional line
					(at 22.86 27.94 180)
					(length 2.54)
					(name "P0.08")
					(number "E5")
				)
				(pin bidirectional line
					(at 22.86 25.4 180)
					(length 2.54)
					(name "P0.09")
					(number "E4")
				)
				(pin bidirectional line
					(at 22.86 22.86 180)
					(length 2.54)
					(name "P0.10")
					(number "E6")
				)
				(pin bidirectional line
					(at 22.86 20.32 180)
					(length 2.54)
					(name "P0.11")
					(number "E7")
				)
				(pin bidirectional line
					(at 22.86 15.24 180)
					(length 2.54)
					(name "P1.00")
					(number "G3")
				)
				(pin bidirectional line
					(at 22.86 12.7 180)
					(length 2.54)
					(name "P1.01")
					(number "F3")
				)
				(pin bidirectional line
					(at 22.86 10.16 180)
					(length 2.54)
					(name "P1.02")
					(number "F2")
				)
				(pin bidirectional line
					(at 22.86 7.62 180)
					(length 2.54)
					(name "P1.03")
					(number "D3")
				)
				(pin bidirectional line
					(at 22.86 5.08 180)
					(length 2.54)
					(name "P1.04")
					(number "F4")
				)
				(pin bidirectional line
					(at 22.86 2.54 180)
					(length 2.54)
					(name "P1.05")
					(number "F6")
				)
				(pin bidirectional line
					(at 22.86 0 180)
					(length 2.54)
					(name "P1.06")
					(number "F7")
				)
				(pin bidirectional line
					(at 22.86 -5.08 180)
					(length 2.54)
					(name "P1.08")
					(number "G8")
				)
				(pin bidirectional line
					(at 22.86 -7.62 180)
					(length 2.54)
					(name "P1.09")
					(number "H3")
				)
				(pin bidirectional line
					(at 22.86 -10.16 180)
					(length 2.54)
					(name "P1.10")
					(number "G5")
				)
				(pin bidirectional line
					(at 22.86 -12.7 180)
					(length 2.54)
					(name "P1.11")
					(number "G4")
				)
				(pin bidirectional line
					(at 22.86 -17.78 180)
					(length 2.54)
					(name "P2.00")
					(number "B3")
				)
				(pin bidirectional line
					(at 22.86 -20.32 180)
					(length 2.54)
					(name "P2.01")
					(number "B2")
				)
				(pin bidirectional line
					(at 22.86 -22.86 180)
					(length 2.54)
					(name "P2.02")
					(number "E2")
				)
				(pin bidirectional line
					(at 22.86 -25.4 180)
					(length 2.54)
					(name "P2.03")
					(number "B4")
				)
				(pin bidirectional line
					(at 22.86 -27.94 180)
					(length 2.54)
					(name "P2.04")
					(number "B5")
				)
				(pin bidirectional line
					(at 22.86 -30.48 180)
					(length 2.54)
					(name "P2.05")
					(number "B6")
				)
				(pin bidirectional line
					(at 22.86 -33.02 180)
					(length 2.54)
					(name "P2.06")
					(number "A3")
				)
				(pin bidirectional line
					(at 22.86 -35.56 180)
					(length 2.54)
					(name "P2.07")
					(number "C4")
				)
				(pin bidirectional line
					(at 22.86 -38.1 180)
					(length 2.54)
					(name "P2.08")
					(number "C5")
				)
				(pin bidirectional line
					(at 22.86 -40.64 180)
					(length 2.54)
					(name "P2.09")
					(number "C3")
				)
			)
			(symbol "BM20x_1_0"
				(pin bidirectional line
					(at -22.86 45.72 0)
					(length 2.54)
					(name "D+")
					(number "G7")
				)
				(pin bidirectional line
					(at -22.86 43.18 0)
					(length 2.54)
					(name "D-")
					(number "G6")
				)
				(pin bidirectional line
					(at -22.86 7.62 0)
					(length 2.54)
					(name "P6.12")
					(number "J4")
				)
				(pin no_connect line
					(at -12.7 50.8 270)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "A2")
				)
				(pin power_in line
					(at 0 -53.34 90)
					(length 2.54)
					(name "GND")
					(number "A1")
				)
				(pin bidirectional line
					(at 22.86 -2.54 180)
					(length 2.54)
					(name "P1.07")
					(number "G9")
				)
				(pin bidirectional line
					(at 22.86 -43.18 180)
					(length 2.54)
					(name "P2.10/NFC1")
					(number "D2")
				)
				(pin bidirectional line
					(at 22.86 -45.72 180)
					(length 2.54)
					(name "P2.11/NFC2")
					(number "C2")
				)
			)
			(symbol "BM20x_1_1")
			(embedded_fonts no)
		)
)
