(footprint "E73-2G4M08S1C"
	(version 20260206)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Ebyte E73-2G4M08S1C module, 13.0x18.0mm, 43 Pad, generated with kicad-footprint-generator ipc_bga_generator.py, https://www.ebyte.com/product/1317.html")
	(tags "LGA 43")
	(property "Reference" "REF**"
		(at 0 -10 0)
		(layer "F.SilkS")
	)
	(property "Value" "E73-2G4M08S1C"
		(at 0 10 0)
		(layer "F.Fab")
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -6 -5.03)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -6 -3.76)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -6 -2.49)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -6 -1.22)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -6 0.05)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -6 1.32)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -6 2.59)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -6 3.86)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -6 5.13)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -6 6.4)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -4.44 8.5 90)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -3.81 6.9 90)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -3.17 8.5 90)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -2.54 6.9 90)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -1.9 8.5 90)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -1.27 6.9 90)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at -0.63 8.5 90)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 0 6.9 90)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 0.64 8.5 90)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 1.27 6.9 90)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 1.91 8.5 90)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 2.54 6.9 90)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 3.18 8.5 90)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 3.81 6.9 90)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 4.45 8.5 90)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 6 6.4)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 6 5.13)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 4.4 4.495 90)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at 6 3.86)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at 4.4 3.225 90)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at 6 2.59)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at 4.4 1.955 90)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at 6 1.32)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at 4.4 0.685 90)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at 6 0.05)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at 4.4 -0.585 90)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at 6 -1.22)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at 4.4 -1.855 90)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at 6 -2.49)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at 4.4 -3.125 90)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "41" smd roundrect
		(at 6 -3.76)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "42" smd roundrect
		(at 4.4 -4.395 90)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "43" smd roundrect
		(at 6 -5.03)
		(size 1 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Cu" "Dwgs.User")
		(name "Keepout")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -8.5 -11)
				(xy 8.5 -11)
				(xy 8.5 -5.5)
				(xy -8.5 -5.5)
			)
		)
	)
	(embedded_fonts no)
	(model "nordic_e73_2g4m08s1c.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
