(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "E73-2G4M08S1C"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 13.97 41.91 0)
				(do_not_autoplace)
			)
			(property "Value" "E73-2G4M08S1C"
				(at 26.67 39.37 0)
				(do_not_autoplace)
			)
			(property "Footprint" "nordic-lib-kicad-nrf52-modules:E73-2G4M08S1C"
				(at -5.08 0 90)
			)
			(property "Datasheet" "https://www.ebyte.com/en/downpdf.aspx?id=445"
				(at 0 -53.34 0)
			)
			(property "Description" "nRF52840 BT LE module"
				(at 0 0 0)
			)
			(property "LCSC" "C356849"
				(at 0 0 0)
			)
			(property "ki_keywords" "Bluetooth LE nRF nordic"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "E73*2G4M08S1C*"
				(at 0 0 0)
			)
			(symbol "E73-2G4M08S1C_0_0"
				(pin bidirectional line
					(at 22.86 -27.94 180)
					(length 2.54)
					(name "P1.11")
					(number "1")
				)
				(pin power_in line
					(at 22.86 15.24 180)
					(length 2.54)
					(name "P0.30/AIN6")
					(number "10")
				)
				(pin bidirectional line
					(at 22.86 7.62 180)
					(length 2.54)
					(name "P0.00/XL1")
					(number "11")
				)
				(pin bidirectional line
					(at -22.86 -30.48 0)
					(length 2.54)
					(name "P0.26")
					(number "12")
				)
				(pin bidirectional line
					(at 22.86 5.08 180)
					(length 2.54)
					(name "P0.01/XL2")
					(number "13")
				)
				(pin bidirectional line
					(at -22.86 -5.08 0)
					(length 2.54)
					(name "P0.06")
					(number "14")
				)
				(pin bidirectional line
					(at 22.86 22.86 180)
					(length 2.54)
					(name "P0.05/AIN3")
					(number "15")
				)
				(pin bidirectional line
					(at -22.86 -10.16 0)
					(length 2.54)
					(name "P0.08")
					(number "16")
				)
				(pin bidirectional line
					(at 22.86 -22.86 180)
					(length 2.54)
					(name "P1.09")
					(number "17")
				)
				(pin bidirectional line
					(at 22.86 25.4 180)
					(length 2.54)
					(name "P0.04/AIN2")
					(number "18")
				)
				(pin bidirectional line
					(at -2.54 40.64 270)
					(length 2.54)
					(name "VDD")
					(number "19")
				)
				(pin bidirectional line
					(at 22.86 -25.4 180)
					(length 2.54)
					(name "P1.10")
					(number "2")
				)
				(pin bidirectional line
					(at -22.86 -12.7 0)
					(length 2.54)
					(name "P0.12")
					(number "20")
				)
				(pin bidirectional line
					(at -22.86 -7.62 0)
					(length 2.54)
					(name "P0.07")
					(number "22")
				)
				(pin bidirectional line
					(at 2.54 40.64 270)
					(length 2.54)
					(name "VDDH")
					(number "23")
				)
				(pin bidirectional line
					(at 5.08 40.64 270)
					(length 2.54)
					(name "DCCH")
					(number "25")
				)
				(pin input line
					(at -22.86 17.78 0)
					(length 2.54)
					(name "VBUS")
					(number "27")
				)
				(pin bidirectional line
					(at -22.86 -17.78 0)
					(length 2.54)
					(name "P0.15")
					(number "28")
				)
				(pin bidirectional line
					(at -22.86 15.24 0)
					(length 2.54)
					(name "D-")
					(number "29")
				)
				(pin bidirectional line
					(at 22.86 27.94 180)
					(length 2.54)
					(name "P0.03/AIN1")
					(number "3")
				)
				(pin bidirectional line
					(at -22.86 -20.32 0)
					(length 2.54)
					(name "P0.17")
					(number "30")
				)
				(pin bidirectional line
					(at -22.86 12.7 0)
					(length 2.54)
					(name "D+")
					(number "31")
				)
				(pin bidirectional line
					(at -22.86 -22.86 0)
					(length 2.54)
					(name "P0.20")
					(number "32")
				)
				(pin bidirectional line
					(at -22.86 -15.24 0)
					(length 2.54)
					(name "P0.13")
					(number "33")
				)
				(pin bidirectional line
					(at -22.86 -25.4 0)
					(length 2.54)
					(name "P0.22")
					(number "34")
				)
				(pin bidirectional line
					(at -22.86 -27.94 0)
					(length 2.54)
					(name "P0.24")
					(number "35")
				)
				(pin bidirectional line
					(at 22.86 -12.7 180)
					(length 2.54)
					(name "P1.00")
					(number "36")
				)
				(pin bidirectional line
					(at -22.86 27.94 0)
					(length 2.54)
					(name "SWDIO")
					(number "37")
				)
				(pin bidirectional line
					(at 22.86 -15.24 180)
					(length 2.54)
					(name "P1.02")
					(number "38")
				)
				(pin power_in line
					(at -22.86 30.48 0)
					(length 2.54)
					(name "SWDCLK")
					(number "39")
				)
				(pin bidirectional line
					(at 22.86 20.32 180)
					(length 2.54)
					(name "P0.28/AIN4")
					(number "4")
				)
				(pin bidirectional line
					(at 22.86 -17.78 180)
					(length 2.54)
					(name "P1.04")
					(number "40")
				)
				(pin bidirectional line
					(at 22.86 0 180)
					(length 2.54)
					(name "P0.09/NFC1")
					(number "41")
				)
				(pin power_in line
					(at 22.86 -20.32 180)
					(length 2.54)
					(name "P1.06")
					(number "42")
				)
				(pin power_in line
					(at 22.86 -2.54 180)
					(length 2.54)
					(name "P0.10/NFC2")
					(number "43")
				)
				(pin bidirectional line
					(at 22.86 -30.48 180)
					(length 2.54)
					(name "P1.13")
					(number "6")
				)
				(pin bidirectional line
					(at 22.86 30.48 180)
					(length 2.54)
					(name "P0.02/AIN0")
					(number "7")
				)
				(pin bidirectional line
					(at 22.86 17.78 180)
					(length 2.54)
					(name "P0.29/AIN5")
					(number "8")
				)
				(pin power_in line
					(at 22.86 12.7 180)
					(length 2.54)
					(name "P0.31/AIN7")
					(number "9")
				)
			)
			(symbol "E73-2G4M08S1C_0_1")
			(symbol "E73-2G4M08S1C_1_0"
				(pin passive line
					(at 0 -40.64 90)
					(length 2.54) hide
					(name "GND")
					(number "21")
				)
				(pin passive line
					(at 0 -40.64 90)
					(length 2.54) hide
					(name "GND")
					(number "24")
				)
				(pin bidirectional line
					(at -22.86 35.56 0)
					(length 2.54)
					(name "P0.18/~{RESET}")
					(number "26")
				)
				(pin power_in line
					(at 0 -40.64 90)
					(length 2.54)
					(name "GND")
					(number "5")
				)
			)
		)
)
