(footprint "E83-2G4M03S_16x16mm_LGA"
	(version 20260206)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Ebyte E83-2G4M03S module, 16.0x16.0mm, 65 Pad, generated with kicad-footprint-generator ipc_bga_generator.py, https://www.cdebyte.com/products/E83-2G4M03S")
	(tags "LGA 65")
	(property "Reference" "REF**"
		(at 0 -9 0)
		(layer "F.SilkS")
	)
	(property "Value" "E83-2G4M03S_16x16mm_LGA"
		(at 0 9 0)
		(layer "F.Fab")
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -7.3 -5.715)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "2" smd roundrect
		(at -7.3 -4.445)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "3" smd roundrect
		(at -7.3 -3.175)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "4" smd roundrect
		(at -7.3 -1.905)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "5" smd roundrect
		(at -7.3 -0.635)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "6" smd roundrect
		(at -7.3 0.635)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "7" smd roundrect
		(at -7.3 1.905)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "8" smd roundrect
		(at -7.3 3.175)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "9" smd roundrect
		(at -7.3 4.445)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "10" smd roundrect
		(at -7.3 5.715)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "11" smd roundrect
		(at -6.03 -5.08)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "12" smd roundrect
		(at -6.03 -3.81)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "13" smd roundrect
		(at -6.03 -2.54)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "14" smd roundrect
		(at -6.03 -1.27)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "15" smd roundrect
		(at -6.03 0)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "16" smd roundrect
		(at -6.03 1.27)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "17" smd roundrect
		(at -6.03 2.54)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "18" smd roundrect
		(at -6.03 3.81)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "19" smd roundrect
		(at -5.715 7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "20" smd roundrect
		(at -4.445 7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "21" smd roundrect
		(at -3.175 7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "22" smd roundrect
		(at -1.905 7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "23" smd roundrect
		(at -0.635 7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "24" smd roundrect
		(at 0.635 7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "25" smd roundrect
		(at 1.905 7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "26" smd roundrect
		(at 3.175 7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "27" smd roundrect
		(at 4.445 7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "28" smd roundrect
		(at 5.715 7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "29" smd roundrect
		(at -5.08 6.03)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "30" smd roundrect
		(at -3.81 6.03)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "31" smd roundrect
		(at -2.54 6.03)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "32" smd roundrect
		(at -1.27 6.03)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "33" smd roundrect
		(at 0 6.03)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "34" smd roundrect
		(at 1.27 6.03)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "35" smd roundrect
		(at 2.54 6.03)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "36" smd roundrect
		(at 3.81 6.03)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "37" smd roundrect
		(at 5.08 6.03)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "38" smd roundrect
		(at 7.3 5.715)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "39" smd roundrect
		(at 7.3 4.445)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "40" smd roundrect
		(at 7.3 3.175)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "41" smd roundrect
		(at 7.3 1.905)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "42" smd roundrect
		(at 7.3 0.635)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "43" smd roundrect
		(at 7.3 -0.635)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "44" smd roundrect
		(at 7.3 -1.905)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "45" smd roundrect
		(at 7.3 -3.175)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "46" smd roundrect
		(at 7.3 -4.445)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "47" smd roundrect
		(at 7.3 -5.715)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "48" smd roundrect
		(at 6.03 3.81)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "49" smd roundrect
		(at 6.03 2.54)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "50" smd roundrect
		(at 6.03 1.27)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "51" smd roundrect
		(at 6.03 0)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "52" smd roundrect
		(at 6.03 -1.27)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "53" smd roundrect
		(at 6.03 -2.54)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "54" smd roundrect
		(at 6.03 -3.81)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "55" smd roundrect
		(at 6.03 -5.08)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "56" smd roundrect
		(at 5.715 -7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "57" smd roundrect
		(at 4.445 -7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "58" smd roundrect
		(at 3.175 -7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "59" smd roundrect
		(at 1.905 -7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "60" smd roundrect
		(at 0.635 -7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "61" smd roundrect
		(at -0.635 -7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "62" smd roundrect
		(at -1.905 -7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "63" smd roundrect
		(at -3.175 -7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "64" smd roundrect
		(at -4.445 -7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "65" smd roundrect
		(at -5.715 -7.3)
		(size 0.81 0.81)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(embedded_fonts no)
	(model "nordic_e83_2g4m03s.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
