(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "E83-2G4M03S"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 0 0)
			)
			(property "Value" "E83-2G4M03S"
				(at 0 -2.54 0)
			)
			(property "Footprint" "nordic-lib-kicad-nrf53-modules:E83-2G4M03S_16x16mm_LGA"
				(at 0 21.59 0)
			)
			(property "Datasheet" "https://www.cdebyte.com/products/E83-2G4M03S"
				(at 0 21.59 0)
			)
			(property "Description" "nRF5340 Module External Antenna"
				(at 0 21.59 0)
			)
			(property "LCSC" "C5333991"
				(at 0 0 0)
			)
			(property "ki_keywords" "nRF5340 Module External Antenna"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "E83*2G4M03S*16x16mm*LGA*"
				(at 0 0 0)
			)
			(symbol "E83-2G4M03S_0_0"
				(pin input line
					(at 22.86 -5.08 180)
					(length 2.54)
					(name "~{RESET}")
					(number "1")
				)
				(pin power_in line
					(at 22.86 46.99 180)
					(length 2.54)
					(name "VBUS")
					(number "10")
				)
				(pin bidirectional line
					(at 22.86 2.54 180)
					(length 2.54)
					(name "P0.28/AIN7")
					(number "11")
				)
				(pin power_in line
					(at 0 -57.15 90)
					(length 2.54)
					(name "GND")
					(number "12")
				)
				(pin bidirectional line
					(at -22.86 33.02 0)
					(length 2.54)
					(name "P0.29")
					(number "13")
				)
				(pin bidirectional line
					(at -22.86 30.48 0)
					(length 2.54)
					(name "P0.30")
					(number "14")
				)
				(pin bidirectional line
					(at -22.86 2.54 0)
					(length 2.54)
					(name "P1.11")
					(number "15")
				)
				(pin bidirectional line
					(at -22.86 -2.54 0)
					(length 2.54)
					(name "P1.13")
					(number "16")
				)
				(pin bidirectional line
					(at -22.86 -7.62 0)
					(length 2.54)
					(name "P1.15")
					(number "17")
				)
				(pin bidirectional line
					(at 22.86 41.91 180)
					(length 2.54)
					(name "D-")
					(number "18")
				)
				(pin passive line
					(at 0 -57.15 90)
					(length 2.54) hide
					(name "GND")
					(number "19")
				)
				(pin bidirectional line
					(at 22.86 -2.54 180)
					(length 2.54)
					(name "SWDIO")
					(number "2")
				)
				(pin passive line
					(at 0 -57.15 90)
					(length 2.54) hide
					(name "GND")
					(number "20")
				)
				(pin passive line
					(at 0 -57.15 90)
					(length 2.54) hide
					(name "GND")
					(number "22")
				)
				(pin power_in line
					(at 2.54 57.15 270)
					(length 2.54)
					(name "VDD")
					(number "23")
				)
				(pin passive line
					(at 0 -57.15 90)
					(length 2.54) hide
					(name "GND")
					(number "24")
				)
				(pin bidirectional line
					(at 22.86 36.83 180)
					(length 2.54)
					(name "P0.00/XL1")
					(number "25")
				)
				(pin bidirectional line
					(at 22.86 31.75 180)
					(length 2.54)
					(name "P0.01/XL2")
					(number "26")
				)
				(pin bidirectional line
					(at 22.86 27.94 180)
					(length 2.54)
					(name "P0.02/NFC1")
					(number "27")
				)
				(pin bidirectional line
					(at 22.86 25.4 180)
					(length 2.54)
					(name "P0.03/NFC2")
					(number "28")
				)
				(pin bidirectional line
					(at -22.86 22.86 0)
					(length 2.54)
					(name "P1.01")
					(number "29")
				)
				(pin bidirectional line
					(at -22.86 25.4 0)
					(length 2.54)
					(name "P1.00")
					(number "30")
				)
				(pin bidirectional line
					(at 22.86 17.78 180)
					(length 2.54)
					(name "P0.05/AIN1")
					(number "31")
				)
				(pin bidirectional line
					(at 22.86 15.24 180)
					(length 2.54)
					(name "P0.06/AIN2")
					(number "32")
				)
				(pin bidirectional line
					(at 22.86 12.7 180)
					(length 2.54)
					(name "P0.07/AIN3")
					(number "33")
				)
				(pin bidirectional line
					(at -22.86 -45.72 0)
					(length 2.54)
					(name "P1.03/I2C")
					(number "34")
				)
				(pin bidirectional line
					(at -22.86 -43.18 0)
					(length 2.54)
					(name "P1.02/I2C")
					(number "35")
				)
				(pin bidirectional line
					(at -22.86 5.08 0)
					(length 2.54)
					(name "P1.10")
					(number "4")
				)
				(pin bidirectional line
					(at -22.86 -16.51 0)
					(length 2.54)
					(name "P0.13/QSPI0")
					(number "40")
				)
				(pin bidirectional line
					(at -22.86 48.26 0)
					(length 2.54)
					(name "P0.19")
					(number "41")
				)
				(pin bidirectional line
					(at -22.86 20.32 0)
					(length 2.54)
					(name "P1.04")
					(number "42")
				)
				(pin bidirectional line
					(at -22.86 10.16 0)
					(length 2.54)
					(name "P1.08")
					(number "43")
				)
				(pin bidirectional line
					(at -22.86 45.72 0)
					(length 2.54)
					(name "P0.20")
					(number "44")
				)
				(pin bidirectional line
					(at 22.86 7.62 180)
					(length 2.54)
					(name "P0.26/AIN5")
					(number "45")
				)
				(pin passive line
					(at 0 -57.15 90)
					(length 2.54) hide
					(name "GND")
					(number "46")
				)
				(pin passive line
					(at 0 -57.15 90)
					(length 2.54) hide
					(name "GND")
					(number "47")
				)
				(pin bidirectional line
					(at -22.86 -24.13 0)
					(length 2.54)
					(name "P0.16/QSPI3")
					(number "49")
				)
				(pin bidirectional line
					(at -22.86 27.94 0)
					(length 2.54)
					(name "P0.31")
					(number "5")
				)
				(pin bidirectional line
					(at -22.86 43.18 0)
					(length 2.54)
					(name "P0.21")
					(number "50")
				)
				(pin bidirectional line
					(at -22.86 15.24 0)
					(length 2.54)
					(name "P1.06")
					(number "51")
				)
				(pin bidirectional line
					(at -22.86 -19.05 0)
					(length 2.54)
					(name "P0.14/QSPI1")
					(number "52")
				)
				(pin bidirectional line
					(at -22.86 35.56 0)
					(length 2.54)
					(name "P0.24")
					(number "53")
				)
				(pin bidirectional line
					(at -22.86 40.64 0)
					(length 2.54)
					(name "P0.22")
					(number "54")
				)
				(pin passive line
					(at 0 -57.15 90)
					(length 2.54) hide
					(name "GND")
					(number "55")
				)
				(pin passive line
					(at 0 -57.15 90)
					(length 2.54) hide
					(name "GND")
					(number "56")
				)
				(pin bidirectional line
					(at -22.86 38.1 0)
					(length 2.54)
					(name "P0.23")
					(number "57")
				)
				(pin bidirectional line
					(at -22.86 17.78 0)
					(length 2.54)
					(name "P1.05")
					(number "58")
				)
				(pin bidirectional line
					(at 22.86 10.16 180)
					(length 2.54)
					(name "P0.25/AIN4")
					(number "59")
				)
				(pin bidirectional line
					(at -22.86 0 0)
					(length 2.54)
					(name "P1.12")
					(number "6")
				)
				(pin bidirectional line
					(at 22.86 5.08 180)
					(length 2.54)
					(name "P0.27/AIN6")
					(number "60")
				)
				(pin bidirectional line
					(at -22.86 -13.97 0)
					(length 2.54)
					(name "P0.17/QSPI_CLK")
					(number "61")
				)
				(pin bidirectional line
					(at -22.86 -21.59 0)
					(length 2.54)
					(name "P0.15/QSPI2")
					(number "62")
				)
				(pin bidirectional line
					(at -22.86 -11.43 0)
					(length 2.54)
					(name "P0.18/QSPI_~{CS}")
					(number "63")
				)
				(pin bidirectional line
					(at -22.86 7.62 0)
					(length 2.54)
					(name "P1.09")
					(number "64")
				)
				(pin bidirectional line
					(at -22.86 12.7 0)
					(length 2.54)
					(name "P1.07")
					(number "65")
				)
				(pin bidirectional line
					(at -22.86 -5.08 0)
					(length 2.54)
					(name "P1.14")
					(number "7")
				)
				(pin bidirectional line
					(at 22.86 20.32 180)
					(length 2.54)
					(name "P0.04/AIN0")
					(number "8")
				)
				(pin bidirectional line
					(at 22.86 44.45 180)
					(length 2.54)
					(name "D+")
					(number "9")
				)
			)
			(symbol "E83-2G4M03S_1_0"
				(pin power_in line
					(at 0 57.15 270)
					(length 2.54)
					(name "VDDH")
					(number "21")
				)
				(pin input line
					(at 22.86 -7.62 180)
					(length 2.54)
					(name "SWDCLK")
					(number "3")
				)
				(pin bidirectional line
					(at -22.86 -36.83 0)
					(length 2.54)
					(name "P0.08/TD3/SCK")
					(number "36")
				)
				(pin bidirectional line
					(at -22.86 -34.29 0)
					(length 2.54)
					(name "P0.09/TD2/MOSI")
					(number "37")
				)
				(pin bidirectional line
					(at -22.86 -31.75 0)
					(length 2.54)
					(name "P0.10/TD1/MISO")
					(number "38")
				)
				(pin bidirectional line
					(at -22.86 -29.21 0)
					(length 2.54)
					(name "P0.11/TD0/~{CS}")
					(number "39")
				)
				(pin bidirectional line
					(at -22.86 -39.37 0)
					(length 2.54)
					(name "P0.12/TC/DCX")
					(number "48")
				)
			)
			(symbol "E83-2G4M03S_1_1")
		)
)
