(footprint "ISP1907_8x8mm_LGA"
	(version 20260206)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Insight SiP ISP1907-LL module, 8.0x8.0mm, 62 Pad, generated with kicad-footprint-generator ipc_bga_generator.py, https://www.insightsip.com/fichiers_insightsip/pdf/ble/ISP1907/isp_ble_DS1907.pdf")
	(tags "LGA 62")
	(property "Reference" "REF**"
		(at 0 -5 0)
		(layer "F.SilkS")
	)
	(property "Value" "ISP1907_8x8mm_LGA"
		(at 0 5 0)
		(layer "F.Fab")
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -3.5 -3.5)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "2" smd roundrect
		(at -3.7 -2.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "3" smd roundrect
		(at -3.05 -2.275)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "4" smd roundrect
		(at -3.7 -1.95)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "5" smd roundrect
		(at -3.05 -1.625)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "6" smd roundrect
		(at -3.7 -1.3)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "7" smd roundrect
		(at -3.5 -0.4)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "8" smd roundrect
		(at -2.6 -0.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "9" smd roundrect
		(at -2.275 -0.85)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "10" smd roundrect
		(at -1.95 -0.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "11" smd roundrect
		(at -1.625 -0.85)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "12" smd roundrect
		(at -1.3 -0.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "13" smd roundrect
		(at -0.975 -0.85)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "14" smd roundrect
		(at -0.65 -0.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "15" smd roundrect
		(at -0.325 -0.85)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "16" smd roundrect
		(at 0 -0.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "17" smd roundrect
		(at 0.325 -0.85)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "18" smd roundrect
		(at 0.65 -0.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "19" smd roundrect
		(at 0.975 -0.85)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "20" smd roundrect
		(at 1.3 -0.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "21" smd roundrect
		(at 1.625 -0.85)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "22" smd roundrect
		(at 1.95 -0.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "23" smd roundrect
		(at 2.275 -0.85)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "24" smd roundrect
		(at 2.6 -0.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "25" smd roundrect
		(at 3.5 -0.4)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "26" smd roundrect
		(at 3.7 -1.3 180)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "27" smd roundrect
		(at 3.05 -1.625 180)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "28" smd roundrect
		(at 3.7 -1.95 180)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "29" smd roundrect
		(at 3.05 -2.275 180)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "30" smd roundrect
		(at 3.7 -2.6 180)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "31" smd roundrect
		(at 3.5 -3.5)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "32" smd roundrect
		(at 2.6 -3.7)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "33" smd roundrect
		(at 2.275 -3.05)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "34" smd roundrect
		(at 1.95 -3.7)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "35" smd roundrect
		(at 1.625 -3.05)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "36" smd roundrect
		(at 1.3 -3.7)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "37" smd roundrect
		(at 0.975 -3.05)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "38" smd roundrect
		(at 0.65 -3.7)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "39" smd roundrect
		(at 0.325 -3.05)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "40" smd roundrect
		(at 0 -3.7)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "41" smd roundrect
		(at -0.325 -3.05)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "42" smd roundrect
		(at -0.65 -3.7)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "43" smd roundrect
		(at -0.975 -3.05)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "44" smd roundrect
		(at -1.3 -3.7)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "45" smd roundrect
		(at -1.625 -3.05)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "46" smd roundrect
		(at -1.95 -3.7)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "47" smd roundrect
		(at -2.275 -3.05)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "48" smd roundrect
		(at -2.6 -3.7)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "49" smd roundrect
		(at -3.65 0.55)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "50" smd roundrect
		(at -3.65 1.55)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "51" smd roundrect
		(at -3.65 2.55)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "52" smd roundrect
		(at -3.5 3.5)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "53" smd roundrect
		(at -2.5 3.7)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "54" smd roundrect
		(at -1.5 3.7)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "55" smd roundrect
		(at -0.5 3.7)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "56" smd roundrect
		(at 0.5 3.7)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "57" smd roundrect
		(at 1.5 3.7)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "58" smd roundrect
		(at 2.5 3.7)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "59" smd roundrect
		(at 3.5 3.5)
		(size 0.8 0.8)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "60" smd roundrect
		(at 3.7 2.55)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "61" smd roundrect
		(at 3.7 1.55)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "62" smd roundrect
		(at 3.7 0.55)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Cu" "Dwgs.User")
		(name "Keepout")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -4.5 0.1)
				(xy 4.5 0.1)
				(xy 4.5 4.5)
				(xy -4.5 4.5)
			)
		)
	)
	(embedded_fonts no)
	(model "nordic_isp1907_ll.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
