(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ISP2053-AX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 0 0)
				(do_not_autoplace)
			)
			(property "Value" "ISP2053-AX"
				(at 0 -2.54 0)
				(do_not_autoplace)
			)
			(property "Footprint" "nordic-lib-kicad-nrf53-modules:ISP2053_8x8mm_LGA"
				(at 0 -5.08 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "ISP2053*8x8mm*LGA*"
				(at 0 0 0)
			)
			(symbol "ISP2053-AX_0_0"
				(pin unspecified line
					(at 30.48 55.88 180)
					(length 5.08)
					(name "VBUS")
					(number "A2")
				)
				(pin unspecified line
					(at -30.48 -48.26 0)
					(length 5.08)
					(name "P1.03/I2C")
					(number "A3")
				)
				(pin unspecified line
					(at 30.48 53.34 180)
					(length 5.08)
					(name "D+")
					(number "A4")
				)
				(pin unspecified line
					(at 30.48 50.8 180)
					(length 5.08)
					(name "D-")
					(number "A5")
				)
				(pin unspecified line
					(at 0 71.12 270)
					(length 5.08)
					(name "VDDH")
					(number "A6")
				)
				(pin unspecified line
					(at -2.54 71.12 270)
					(length 5.08)
					(name "DCCH")
					(number "A7")
				)
				(pin unspecified line
					(at -30.48 -53.34 0)
					(length 5.08)
					(name "P0.02/NFC1")
					(number "A8")
				)
				(pin unspecified line
					(at -30.48 -55.88 0)
					(length 5.08)
					(name "P0.03/NFC2")
					(number "A9")
				)
				(pin unspecified line
					(at -30.48 -45.72 0)
					(length 5.08)
					(name "P1.02/I2C")
					(number "B10")
				)
				(pin unspecified line
					(at -30.48 55.88 0)
					(length 5.08)
					(name "P1.15")
					(number "B2")
				)
				(pin unspecified line
					(at -30.48 -10.16 0)
					(length 5.08)
					(name "P0.06/AIN2")
					(number "B3")
				)
				(pin unspecified line
					(at -30.48 -5.08 0)
					(length 5.08)
					(name "P0.04/AIN0")
					(number "B4")
				)
				(pin unspecified line
					(at -30.48 53.34 0)
					(length 5.08)
					(name "P1.01")
					(number "B5")
				)
				(pin unspecified line
					(at -30.48 -12.7 0)
					(length 5.08)
					(name "P0.07/AIN3")
					(number "B6")
				)
				(pin unspecified line
					(at -30.48 50.8 0)
					(length 5.08)
					(name "P1.00")
					(number "B7")
				)
				(pin unspecified line
					(at -30.48 -7.62 0)
					(length 5.08)
					(name "P0.05/AIN1")
					(number "B8")
				)
				(pin unspecified line
					(at 30.48 20.32 180)
					(length 5.08)
					(name "P0.08/TD3")
					(number "B9")
				)
				(pin unspecified line
					(at 2.54 71.12 270)
					(length 5.08)
					(name "VDD")
					(number "C1")
				)
				(pin unspecified line
					(at -30.48 43.18 0)
					(length 5.08)
					(name "P1.05")
					(number "C10")
				)
				(pin unspecified line
					(at 30.48 38.1 180)
					(length 5.08)
					(name "SWDIO")
					(number "C11")
				)
				(pin unspecified line
					(at -30.48 -27.94 0)
					(length 5.08)
					(name "P0.13/QSPI0")
					(number "C2")
				)
				(pin unspecified line
					(at -30.48 48.26 0)
					(length 5.08)
					(name "P0.19")
					(number "C3")
				)
				(pin unspecified line
					(at -30.48 -33.02 0)
					(length 5.08)
					(name "P0.15/QSPI2")
					(number "C4")
				)
				(pin unspecified line
					(at -30.48 -30.48 0)
					(length 5.08)
					(name "P0.14/QSPI1")
					(number "C5")
				)
				(pin unspecified line
					(at -30.48 45.72 0)
					(length 5.08)
					(name "P0.16")
					(number "C6")
				)
				(pin unspecified line
					(at 30.48 22.86 180)
					(length 5.08)
					(name "P0.09/TD2")
					(number "C7")
				)
				(pin unspecified line
					(at 30.48 27.94 180)
					(length 5.08)
					(name "P0.11/TD0")
					(number "C8")
				)
				(pin unspecified line
					(at -30.48 -38.1 0)
					(length 5.08)
					(name "P0.17/QSPI_CLK")
					(number "C9")
				)
				(pin unspecified line
					(at -30.48 40.64 0)
					(length 5.08)
					(name "P1.13")
					(number "D1")
				)
				(pin unspecified line
					(at -30.48 22.86 0)
					(length 5.08)
					(name "P0.24")
					(number "D10")
				)
				(pin unspecified line
					(at 30.48 35.56 180)
					(length 5.08)
					(name "SWDCLK")
					(number "D11")
				)
				(pin unspecified line
					(at -30.48 38.1 0)
					(length 5.08)
					(name "P0.21")
					(number "D3")
				)
				(pin unspecified line
					(at -30.48 35.56 0)
					(length 5.08)
					(name "P0.22")
					(number "D5")
				)
				(pin unspecified line
					(at -30.48 33.02 0)
					(length 5.08)
					(name "P0.20")
					(number "D6")
				)
				(pin unspecified line
					(at -30.48 30.48 0)
					(length 5.08)
					(name "P1.08")
					(number "D7")
				)
				(pin unspecified line
					(at -30.48 27.94 0)
					(length 5.08)
					(name "P1.09")
					(number "D8")
				)
				(pin unspecified line
					(at -30.48 25.4 0)
					(length 5.08)
					(name "P1.04")
					(number "D9")
				)
				(pin unspecified line
					(at -30.48 20.32 0)
					(length 5.08)
					(name "P1.14")
					(number "E1")
				)
				(pin unspecified line
					(at -30.48 -17.78 0)
					(length 5.08)
					(name "P0.26/AIN5")
					(number "E10")
				)
				(pin unspecified line
					(at -30.48 17.78 0)
					(length 5.08)
					(name "P0.30")
					(number "E2")
				)
				(pin unspecified line
					(at -30.48 15.24 0)
					(length 5.08)
					(name "P0.31")
					(number "E3")
				)
				(pin unspecified line
					(at -30.48 12.7 0)
					(length 5.08)
					(name "P1.12")
					(number "E4")
				)
				(pin unspecified line
					(at -30.48 10.16 0)
					(length 5.08)
					(name "P1.11")
					(number "E5")
				)
				(pin unspecified line
					(at -30.48 -22.86 0)
					(length 5.08)
					(name "P0.28/AIN7")
					(number "E6")
				)
				(pin unspecified line
					(at -30.48 7.62 0)
					(length 5.08)
					(name "P0.29")
					(number "E8")
				)
				(pin unspecified line
					(at -30.48 -20.32 0)
					(length 5.08)
					(name "P0.27/AIN6")
					(number "E9")
				)
				(pin unspecified line
					(at -30.48 -15.24 0)
					(length 5.08)
					(name "P0.25/AIN4")
					(number "F10")
				)
				(pin unspecified line
					(at -30.48 5.08 0)
					(length 5.08)
					(name "P0.23")
					(number "F3")
				)
				(pin unspecified line
					(at -30.48 2.54 0)
					(length 5.08)
					(name "P1.07")
					(number "F4")
				)
				(pin unspecified line
					(at -30.48 0 0)
					(length 5.08)
					(name "P1.10")
					(number "F5")
				)
			)
			(symbol "ISP2053-AX_1_0"
				(pin passive line
					(at 0 -71.12 90)
					(length 5.08)
					(name "VSS")
					(number "A1")
				)
				(pin unspecified line
					(at 30.48 25.4 180)
					(length 5.08)
					(name "P0.10/TD1")
					(number "A10")
				)
				(pin passive line
					(at 0 -71.12 90)
					(length 5.08) hide
					(name "VSS")
					(number "A11")
				)
				(pin unspecified line
					(at 30.48 17.78 180)
					(length 5.08)
					(name "P0.12/TC")
					(number "D2")
				)
				(pin unspecified line
					(at -30.48 -40.64 0)
					(length 5.08)
					(name "P0.18/QSPI_~{CS}")
					(number "D4")
				)
				(pin unspecified line
					(at 30.48 33.02 180)
					(length 5.08)
					(name "~{RST}")
					(number "E11")
				)
				(pin passive line
					(at 0 -71.12 90)
					(length 5.08) hide
					(name "VSS")
					(number "E7")
				)
				(pin passive line
					(at 0 -71.12 90)
					(length 5.08) hide
					(name "VSS")
					(number "F1")
				)
				(pin passive line
					(at 0 -71.12 90)
					(length 5.08) hide
					(name "VSS")
					(number "F11")
				)
				(pin unspecified line
					(at -30.48 -35.56 0)
					(length 5.08)
					(name "P1.06/QSPI3")
					(number "F2")
				)
				(pin passive line
					(at 0 -71.12 90)
					(length 5.08) hide
					(name "VSS")
					(number "F6")
				)
				(pin output line
					(at 30.48 45.72 180)
					(length 5.08)
					(name "OUT_ANT")
					(number "F7")
				)
				(pin input line
					(at 30.48 43.18 180)
					(length 5.08)
					(name "OUT_MOD")
					(number "F8")
				)
				(pin passive line
					(at 0 -71.12 90)
					(length 5.08) hide
					(name "VSS")
					(number "F9")
				)
				(pin no_connect line
					(at 25.4 -20.32 180)
					(length 5.08) hide
					(name "NC")
					(number "H1")
				)
				(pin no_connect line
					(at 25.4 -22.86 180)
					(length 5.08) hide
					(name "NC")
					(number "H11")
				)
				(pin no_connect line
					(at 25.4 -25.4 180)
					(length 5.08) hide
					(name "NC")
					(number "K1")
				)
				(pin no_connect line
					(at 25.4 -27.94 180)
					(length 5.08) hide
					(name "NC")
					(number "K11")
				)
				(pin no_connect line
					(at 25.4 -30.48 180)
					(length 5.08) hide
					(name "NC")
					(number "L1")
				)
				(pin no_connect line
					(at 25.4 -33.02 180)
					(length 5.08) hide
					(name "NC")
					(number "L11")
				)
				(pin no_connect line
					(at 25.4 -35.56 180)
					(length 5.08) hide
					(name "NC")
					(number "L3")
				)
				(pin no_connect line
					(at 25.4 -15.24 180)
					(length 5.08) hide
					(name "NC")
					(number "L5")
				)
				(pin no_connect line
					(at 25.4 -38.1 180)
					(length 5.08) hide
					(name "NC")
					(number "L7")
				)
				(pin no_connect line
					(at 25.4 -17.78 180)
					(length 5.08) hide
					(name "NC")
					(number "L9")
				)
			)
			(symbol "ISP2053-AX_1_1")
		)
)
