(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "FB_1kZ_0.8A_WE-CBF_0805"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "FB"
				(at 15.24 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "FB_1kZ_0.8A_WE-CBF_0805"
				(at 15.24 -8.128 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "FB_1kZ_0.8A_WE-CBF_0805"
				(at 15.24 -10.668 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.we-online.com/components/products/datasheet/742792096.pdf"
				(at 15.24 -13.208 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Ferrite Beads WE-CBF 0805 100MHz 1kOhm 1A, High Current"
				(at 15.24 -23.368 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "742792096"
				(at 15.24 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Würth Elektronik"
				(at 15.24 -15.748 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "1kZ/0.8A"
				(at 15.24 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Current" ""
				(at 20.32 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 15.24 -18.288 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 15.24 -20.828 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "FERRITE BEAD, PASSIVE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "FB_1kZ_0.8A_WE-CBF_0805_0_1")
			(symbol "FB_1kZ_0.8A_WE-CBF_0805_1_1"
				(pin passive line
					(at 0 0 0)
					(length 1.27)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 1.27)
					(name "")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
)
