(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Oscillator_Divider_1Bit_74AHC1G4210"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 30.48 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Oscillator_Divider_1Bit_74AHC1G4210"
				(at 30.48 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Oscillator_Divider_1Bit_74AHC1G4210"
				(at 30.48 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC1G4210.pdf"
				(at 30.48 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "10-stage divider and oscillator -40°C to 125°C Automotive AEC-Q100 5-Pin TSSOP"
				(at 30.48 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "74AHC1G4210GWH"
				(at 30.48 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Nexperia"
				(at 30.48 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 30.48 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "OSCILLATOR, DIVIDER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Oscillator_Divider_1Bit_74AHC1G4210_1_1"
				(text "÷1024"
					(at 7.62 -4.445 0)
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "X1")
					(number "1")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "X2")
					(number "2")
				)
				(pin power_in line
					(at 15.24 -6.35 180)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin output line
					(at 15.24 -2.54 180)
					(length 2.54)
					(name "Q")
					(number "4")
				)
				(pin power_in line
					(at 15.24 1.27 180)
					(length 2.54)
					(name "V_{CC}")
					(number "5")
				)
			)
			(embedded_fonts no)
		)
)
