(footprint "Oscillator_SMD_Abracon_AK2LPHEF1_2.5x2x1mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -1.275 -1.75 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Oscillator_SMD_Abracon_AK2LPHEF1_2.5x2x1mm"
		(at 0 2.8 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -1.25 4.15 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1.25 5.35 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -1.25 6.55 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.625 -1 270)
		(size 0.7 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "2" smd roundrect
		(at -0.625 0 270)
		(size 0.7 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "3" smd roundrect
		(at -0.625 1 270)
		(size 0.7 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "4" smd roundrect
		(at 0.625 1 270)
		(size 0.7 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "5" smd roundrect
		(at 0.625 0 270)
		(size 0.7 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "6" smd roundrect
		(at 0.625 -1 270)
		(size 0.7 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(embedded_fonts no)
	(model "antmicro_ak2lphef1_156_2500t.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 90)
		)
	)
)
