(footprint "Oscillator_SMD_Abracon_AMJM_3.2x2.5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Oscillator SMD, AMJM, 3.2x2.5mm")
	(property "Reference" "REF**"
		(at -1.93 -2.21 0)
		(layer "F.SilkS")
	)
	(property "Value" "Oscillator_SMD_Abracon_AMJM_3.2x2.5mm"
		(at -10.211 2.895 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "."
		(at -1.379 -1.944 0)
		(layer "F.SilkS")
	)
	(fp_text user "License: Apache-2.0"
		(at -10.211 4.895 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -10.211 6.095 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -10.211 7.296 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.876 -1.045)
		(size 1 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(chamfer_ratio 0.2)
		(chamfer top_left)
	)
	(pad "2" smd roundrect
		(at -0.876 1.056)
		(size 1 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "3" smd roundrect
		(at 0.922 1.056)
		(size 1 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "4" smd roundrect
		(at 0.922 -1.045)
		(size 1 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(embedded_fonts no)
	(model "antmicro_amjmefb_100_0000t.glb"
		(offset
			(xyz -4.9845 2.4425 4.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 90)
		)
	)
)
