(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "L_470n_4.5A_0805"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "L"
				(at 15.24 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "L_470n_4.5A_0805"
				(at 15.24 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "L_470n_4.5A_0805"
				(at 15.24 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.yageogroup.com/content/datasheet/asset/file/DATASHEET_BEBE00201210_SERIES"
				(at 15.24 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Inductor 470nH, 20%, 20 mOhm"
				(at 15.24 -34.036 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "470n/4.5A"
				(at 15.24 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Pulse Electronics"
				(at 15.24 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "BEBE00201210R47MMS"
				(at 15.24 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ISat" "5.3A"
				(at 15.24 -21.844 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "IMax" "4.5A"
				(at 15.24 -24.638 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Size" "2.0x1.2"
				(at 15.24 -26.67 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 15.24 -28.956 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 15.24 -31.496 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "L_470n_4.5A_0805_0_1")
			(symbol "L_470n_4.5A_0805_1_1"
				(pin passive line
					(at 0 0 0)
					(length 0.508)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 0.508)
					(name "")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
)
