(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "FB_120Z_3A_Murata-BLM18SG_0603"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "FB"
				(at 13.97 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "FB_120Z_3A_Murata-BLM18SG_0603"
				(at 13.97 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "FB_120Z_3A_Murata-BLM18SG_0603"
				(at 13.97 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.murata.com/products/productdata/8796738650142/ENFA0003.pdf?1681308024000"
				(at 13.97 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Ferrite Bead, 0603 [1608 Metric], 120 ohm, 3 A, BLM18S, 0.025 ohm, ± 25%, DC power line (thin type)"
				(at 13.97 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "BLM18SG121TN1D"
				(at 13.97 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Murata"
				(at 13.97 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "120Z/3A"
				(at 13.97 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Current" ""
				(at 20.32 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 13.97 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 13.97 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "0603, SMT, FERRITE BEAD, PASSIVE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "FB_120Z_3A_Murata-BLM18SG_0603_0_1")
			(symbol "FB_120Z_3A_Murata-BLM18SG_0603_1_1"
				(pin passive line
					(at 0 0 0)
					(length 1.27)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 1.27)
					(name "")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
)
