(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "C_4x100nF_1206_3216Metric_array"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "C"
				(at 14.732 -1.905 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "C_4x100nF_1206_3216Metric_array"
				(at 14.732 -9.525 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "C_4x100nF_1206_3216Metric_array"
				(at 14.732 -12.065 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=CKCA43JB1C104M100AA"
				(at 14.732 -14.605 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "4x0.1µF isolated capacitor array 16 V JB 1206 (3216 Metric)"
				(at 14.732 -24.765 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CKCA43JB1C104M100AA"
				(at 14.732 -6.985 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "TDK"
				(at 14.732 -17.145 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "C_4x100nF_1206_3216Metric"
				(at 14.732 -4.445 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 14.732 -19.685 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 14.732 -22.225 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "1206, SMT, CAPACITOR, PASSIVE, ARRAY, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "C_4x100nF_1206_3216Metric_array_0_1")
			(symbol "C_4x100nF_1206_3216Metric_array_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "R1.1")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "R2.1")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "R3.1")
					(number "3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "R4.1")
					(number "4")
				)
				(pin passive line
					(at 8.89 -7.62 180)
					(length 2.54)
					(name "R4.2")
					(number "5")
				)
				(pin passive line
					(at 8.89 -5.08 180)
					(length 2.54)
					(name "R3.2")
					(number "6")
				)
				(pin passive line
					(at 8.89 -2.54 180)
					(length 2.54)
					(name "R2.2")
					(number "7")
				)
				(pin passive line
					(at 8.89 0 180)
					(length 2.54)
					(name "R1.2")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
