(footprint "Resonator_SMD_Citizen_CM309S_12.4x4.4x3.6mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(tags "SMD SMT crystal")
	(property "Reference" "REF**"
		(at 0 -3.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Resonator_SMD_Citizen_CM309S_12.4x4.4x3.6mm"
		(at 0 4.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -6.1 6.1 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -6.1 7.3 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -6.1 8.5 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.7 1.8)
		(size 1.8 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 4.7 1.8)
		(size 1.8 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 4.7 -1.8)
		(size 1.8 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -4.7 -1.8)
		(size 1.8 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_cm309s_30_000mabj_ut.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
