(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Resonator_40MHz_CS2016"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Y"
				(at 22.86 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CX2016FB40000F0FZZH1"
				(at 22.86 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Resonator_40MHz_CS2016"
				(at 22.86 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ele.kyocera.com/assets/products/crystal-device/specification/CX2016FB_10pF.pdf"
				(at 22.86 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Crystal, 40 MHz ±10ppm, f_stability: ±30ppm), CL: 10pF, ESR: 40 Ohm,  2016 4-SMD, No Lead"
				(at 22.86 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CX2016FB40000F0FZZH1"
				(at 22.86 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "KYOCERA AVX"
				(at 22.86 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 22.86 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 22.86 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "40MHz"
				(at 22.86 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "OSCILLATOR"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Resonator_40MHz_CS2016_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 3.81 -5.08 90)
					(length 2.54)
					(name "SH")
					(number "2")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin passive line
					(at 3.81 -5.08 90)
					(length 2.54)
					(hide yes)
					(name "SH")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
)
