(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "L_470n_3.6A_0806"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "L"
				(at 15.24 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "L_470n_3.6A_0806"
				(at 15.24 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "L_470n_3.6A_0806"
				(at 15.24 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/P02/J(E)TE243A-0001.pdf"
				(at 15.24 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Inductor 470n, 20%  32mOhm"
				(at 15.24 -35.306 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "470n/3.6A"
				(at 15.24 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Murata"
				(at 15.24 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "DFE201610E-R47M=P2"
				(at 15.24 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ISat" "4.8A"
				(at 15.24 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "IMax" "3.6A"
				(at 15.24 -25.146 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Size" "2.0x1.6"
				(at 15.24 -27.686 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 15.24 -30.226 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 15.24 -32.766 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "L_470n_3.6A_0806_0_1")
			(symbol "L_470n_3.6A_0806_1_1"
				(pin passive line
					(at 0 0 0)
					(length 0.508)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 0.508)
					(name "")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
)
