(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "L_3u3_4.2A_Murata_DFE322520FD-3R3M=P2"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "L"
				(at 13.97 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "DFE322520FD-3R3M=P2"
				(at 13.97 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "L_3u3_4.2A_Murata_DFE322520FD-3R3M=P2"
				(at 13.97 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/3/76/2/J_E_TE243A_9104.pdf"
				(at 13.97 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Power Inductors - SMD 3.3 UH 20%"
				(at 13.97 -30.48 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "3u3"
				(at 13.97 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Murata"
				(at 13.97 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "DFE322520FD-3R3M=P2"
				(at 13.97 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ISat" "4.2"
				(at 13.97 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "IMax" "5.2"
				(at 13.97 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Size" "1210"
				(at 13.97 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 13.97 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 13.97 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "L_3u3_4.2A_Murata_DFE322520FD-3R3M=P2_0_1")
			(symbol "L_3u3_4.2A_Murata_DFE322520FD-3R3M=P2_1_1"
				(pin passive line
					(at 0 0 0)
					(length 0.508)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 0.508)
					(name "")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
)
