(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Oscillator_125MHz_DSC1103DI2"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Y"
				(at 28.575 -1.905 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Oscillator_125MHz_DSC1103DI2"
				(at 28.575 -12.065 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Oscillator_125MHz_DSC1103DI2"
				(at 28.575 -14.605 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/TCG/ProductDocuments/DataSheets/DSC1103-23-Low-Jitter-Precision-LVDS-Oscillator-DS20005745C.pdf"
				(at 28.575 -17.145 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "125 MHz XO (Standard) LVDS Oscillator 3.3V Enable/Disable 6-SMD, No Lead"
				(at 28.575 -24.765 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "125 MHz"
				(at 28.575 -9.525 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "MPN" "DSC1103DI2-125.0000"
				(at 28.575 -6.985 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 28.575 -4.445 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 28.575 -19.685 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 28.575 -22.225 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "OSCILLATOR, LVDS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Oscillator_125MHz_DSC1103DI2_1_1"
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "EN")
					(number "1")
				)
				(pin no_connect line
					(at 16.51 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "2")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin output line
					(at 19.05 0 180)
					(length 2.54)
					(name "OUT+")
					(number "4")
				)
				(pin output line
					(at 19.05 -2.54 180)
					(length 2.54)
					(name "OUT-")
					(number "5")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
