(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Oscillator_32.768kHz_ECS-327ATQMV"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Y"
				(at 25.4 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Oscillator_32.768kHz_ECS-327ATQMV"
				(at 25.4 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Oscillator_32.768kHz_ECS-327ATQMV"
				(at 25.4 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ecsxtal.com/store/pdf/ECS-327ATQMV.pdf"
				(at 25.4 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Standard Clock Oscillators XTAL OSC XO 32.768 KHZ CMOS SMD"
				(at 25.4 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "32.768 kHz"
				(at 25.4 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "MPN" "ECS-327ATQMV-BS-TR"
				(at 25.4 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "ECS Inc. International"
				(at 25.4 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 25.4 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 25.4 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "OSCILLATOR"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Oscillator_32.768kHz_ECS-327ATQMV_1_1"
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "EN")
					(number "1")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin output line
					(at 19.05 0 180)
					(length 2.54)
					(name "OUT")
					(number "3")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
)
