(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Oscillator_20MHz_ECS-3953M-200-AU"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Y"
				(at 26.67 -1.778 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Oscillator_20MHz_ECS-3953M-200-AU"
				(at 26.67 -9.398 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Oscillator_20MHz_ECS-3953M-200-AU"
				(at 26.67 -11.938 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ecsxtal.com/store/pdf/ECS_3951_53m_AU.pdf"
				(at 26.67 -14.478 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Standard Clock Oscillator 3V3 HCMOS 20MHz +/-100ppm"
				(at 26.67 -27.178 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "20 MHz"
				(at 26.67 -6.858 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "MPN" "ECS-3953M-200-AU"
				(at 26.67 -4.318 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "ECS Inc. International"
				(at 26.67 -19.558 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 26.67 -22.098 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 26.67 -24.638 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "OSCILLATOR, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Oscillator_20MHz_ECS-3953M-200-AU_1_1"
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "EN")
					(number "1")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin output line
					(at 19.05 0 180)
					(length 2.54)
					(name "OUT")
					(number "3")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
)
