(footprint "C_Pol_Panasonic-F-D8mm-H10.2mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(tags "capacitor electrolytic")
	(property "Reference" "REF**"
		(at 0.325 -5.535 0)
		(layer "F.SilkS")
	)
	(property "Value" "C_Pol_Panasonic-F-D8mm-H10.2mm"
		(at -6.15 5.535 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -6.15 7.535 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -6.15 8.735 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -6.15 9.935 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3.55 0)
		(size 4 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "2" smd rect
		(at 3.55 0)
		(size 4 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(embedded_fonts no)
	(model "antmicro_eee_ft1v331ap.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
