(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "4x0R_0402_array"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "R"
				(at 25.4 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "4x0R_0402_array"
				(at 25.4 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "4x0R_0402_array"
				(at 25.4 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://industrial.panasonic.com/cdbs/www-data/pdf/AOC0000/AOC0000C14.pdf"
				(at 25.4 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Zero Ohm Network Resistor, Jumper, 0402 [1005 Metric], Thick Film, Isolated, Convex, 4 Resistors"
				(at 25.4 -26.67 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "EXB28VR000X"
				(at 25.4 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Panasonic"
				(at 25.4 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 25.4 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 25.4 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "4x0R_0402"
				(at 25.4 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "0201, SMT, RESISTOR, PASSIVE, ARRAY, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "4x0R_0402_array_0_1")
			(symbol "4x0R_0402_array_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "R1.1")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "R2.1")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "R3.1")
					(number "3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "R4.1")
					(number "4")
				)
				(pin passive line
					(at 10.16 -7.62 180)
					(length 2.54)
					(name "R4.2")
					(number "5")
				)
				(pin passive line
					(at 10.16 -5.08 180)
					(length 2.54)
					(name "R3.2")
					(number "6")
				)
				(pin passive line
					(at 10.16 -2.54 180)
					(length 2.54)
					(name "R2.2")
					(number "7")
				)
				(pin passive line
					(at 10.16 0 180)
					(length 2.54)
					(name "R1.2")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
