(footprint "antmicro_grm155r60j106me15d"
  (version 20240108) (generator "partreel")
  (layer "F.Cu")
  (descr "Chip 1005 metric 2-terminal SMD. Land pattern per IPC-7351 density level B (nominal), values as tabulated in KEMET C1002 X7R SMD datasheet Table 3")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.6) (layer "F.SilkS"))
  (fp_text value "VAL**" (at 0 1.6) (layer "F.Fab"))
  (pad "1" smd rect (at -0.535 0) (size 0.62 0.62) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 0.535 0) (size 0.62 0.62) (layers "F.Cu" "F.Paste" "F.Mask"))
  (model "antmicro_grm155r60j106me15d.glb" (offset (xyz 0 0 0)) (scale (xyz 1 1 1)) (rotate (xyz 0 0 0)))
)
