(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "C_Pol_100u_50V_Nichicon_GYB1H101MCQADNGS"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "C"
				(at 13.97 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "C_Pol_100u_50V_Nichicon_GYB1H101MCQADNGS"
				(at 13.97 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "C_Pol_100u_50V_Nichicon_GYB1H101MCQADNGS"
				(at 13.97 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nichicon.com//getmedia/430b3115-57af-4dba-a958-b2a427e2b69e/e-gyb-DB.pdf"
				(at 13.97 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Capacitor: hybrid; 100uF ±20%; 50VDC; 2A; SMD Ø10x10mm; ESR: 28mΩ; -55...105°C"
				(at 13.97 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "GYB1H101MCQADNGS"
				(at 13.97 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Nichicon"
				(at 13.97 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 13.97 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 13.97 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "100u"
				(at 13.97 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Voltage" "50V"
				(at 13.97 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Dielectric" "CONDUCTIVE POLYMER HYBRID ALUMINUM ELECTROLYTIC"
				(at 13.97 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "C_Pol_100u_50V_Nichicon_GYB1H101MCQADNGS_0_1")
			(symbol "C_Pol_100u_50V_Nichicon_GYB1H101MCQADNGS_1_1"
				(pin passive line
					(at 0 0 0)
					(length 1.8542)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 1.8542)
					(name "")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
)
