(footprint "R_0402_1005Metric_EIA"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
	(tags "resistor 0402")
	(property "Reference" "REF**"
		(at 0 -1.17 0)
		(layer "F.SilkS")
	)
	(property "Value" "R_0402_1005Metric_EIA"
		(at 0 1.169 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -0.95 3.169 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -0.95 4.369 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -0.95 5.569 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.5 0 90)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at 0.499 0)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "antmicro_mc00625w0402180r6.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
