(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Oscillator_8MHz_KYOCERA-AVX_MC2520Z"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Y"
				(at 25.4 3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Oscillator_8MHz_KYOCERA-AVX_MC2520Z"
				(at 25.4 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Oscillator_8MHz_KYOCERA-AVX_MC2520Z"
				(at 25.4 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ele.kyocera.com/assets/products/crystal-device/clock_mcz_e.pdf"
				(at 25.4 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Oscillator, 8MHz, CMOS, SMD, 2,5mm x 2mm, 3.63V, MC2520Z Series"
				(at 25.4 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "8 MHz"
				(at 25.4 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "MPN" "MC2520Z8.00000C19XSH"
				(at 25.4 1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "KYOCERA AVX"
				(at 25.4 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 25.4 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 25.4 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "OSCILLATOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Oscillator_8MHz_KYOCERA-AVX_MC2520Z_1_1"
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "EN")
					(number "1")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin output line
					(at 19.05 0 180)
					(length 2.54)
					(name "OUT")
					(number "3")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
)
