(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Choke_MCZ1210AH900L2TA0G"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "T"
				(at 26.67 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Choke_MCZ1210AH900L2TA0G"
				(at 26.67 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Choke_MCZ1210AH900L2TA0G"
				(at 26.67 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://product.tdk.com/en/search/emc/emc/cmf_cmc/info?part_no=MCZ1210AH900L2TA0G"
				(at 26.67 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Choke, Common Mode, MCZ-AH Series, 90 ohm, 100 mA, 0504, 1.25mm x 1mm x 0.6mm"
				(at 26.67 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "TDK"
				(at 26.67 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MCZ1210AH900L2TA0G"
				(at 26.67 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "IMax" "0.1 A"
				(at 26.67 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 26.67 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 26.67 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CHOKE, PASSIVE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "IND_ACM9070_TDK"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Choke_MCZ1210AH900L2TA0G_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at 10.16 -5.08 180)
					(length 2.54)
					(name "3")
					(number "3")
				)
				(pin passive line
					(at 10.16 0 180)
					(length 2.54)
					(name "4")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
)
