(footprint "Oscillator_SMD_YIC_OSC-S5_5x3.2mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3.25 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Oscillator_SMD_YIC_OSC-S5_5x3.2mm"
		(at 0 3.85 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -3 6.999 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3 8.198 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -3 9.399 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.101 -1.3 270)
		(size 1.6 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "2" smd roundrect
		(at -1.101 1.3 270)
		(size 1.6 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "3" smd roundrect
		(at 1.1 1.3 270)
		(size 1.6 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "4" smd roundrect
		(at 1.1 -1.3 270)
		(size 1.6 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(embedded_fonts no)
	(model "antmicro_osc40m_3_3_s5.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 90)
		)
	)
)
