(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Oscillator_100MHz_QT735"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Y"
				(at 34.29 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Oscillator_template_6pin"
				(at 34.29 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Footprint" "Oscillator_100MHz_QT735"
				(at 34.29 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://q-tech.com/wp-content/uploads/QPDS-0238-QT735.pdf"
				(at 34.29 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Rad-hardened oscillator generator, 100MHz, Vin 3.3V, 3.2x5mm, ±100ppm at -40°C to +125°C"
				(at 34.29 -16.256 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "100 MHz"
				(at 34.29 -18.288 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "MPN" "QT735LWD17E - 100.000MHZ"
				(at 34.036 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Q-Tech Corporation"
				(at 34.29 -22.606 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 34.29 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 34.544 -24.892 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "OSCILLATOR"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Oscillator_100MHz_QT735_1_1"
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "EN")
					(number "1")
				)
				(pin no_connect line
					(at 16.51 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "2")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin output line
					(at 19.05 0 180)
					(length 2.54)
					(name "OUT+")
					(number "4")
				)
				(pin output line
					(at 19.05 -2.54 180)
					(length 2.54)
					(name "OUT-")
					(number "5")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
